From 33f002d751efb756f2eac188be11a53dd90e1018 Mon Sep 17 00:00:00 2001
From: Emekcan Aras <emekcan.aras@arm.com>
Date: Thu, 20 Mar 2025 15:49:26 +0000
Subject: [PATCH] corstone1000: set CONFIG_FFA_SHARED_MM_BUF_ADDR

Set the MM communication buffer to a new address

Signed-off-by: Emekcan Aras <emekcan.aras@arm.com>
Signed-off-by: Abdellatif El Khlifi <abdellatif.elkhlifi@arm.com>
Upstream-Status: Pending [Not submitted to upstream yet]
---
 configs/corstone1000_defconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/configs/corstone1000_defconfig b/configs/corstone1000_defconfig
index d7c5d030e9a..3e0fe47bbaf 100644
--- a/configs/corstone1000_defconfig
+++ b/configs/corstone1000_defconfig
@@ -14,7 +14,7 @@ CONFIG_FWU_NUM_IMAGES_PER_BANK=4
 CONFIG_EFI_MM_COMM_TEE=y
 CONFIG_FFA_SHARED_MM_BUF_SIZE=4096
 CONFIG_FFA_SHARED_MM_BUF_OFFSET=0
-CONFIG_FFA_SHARED_MM_BUF_ADDR=0x02000000
+CONFIG_FFA_SHARED_MM_BUF_ADDR=0x81FFF000
 CONFIG_EFI_RUNTIME_UPDATE_CAPSULE=y
 CONFIG_EFI_CAPSULE_ON_DISK=y
 CONFIG_EFI_CAPSULE_FIRMWARE_RAW=y
