From 9fe529a146f4528ec80a3d04588e387f3651dc22 Mon Sep 17 00:00:00 2001
From: Ryan Harkin <ryan.harkin@linaro.org>
Date: Wed, 16 Nov 2016 14:43:02 +0000
Subject: [PATCH] ARM: vexpress: enable GICv3

Upstream-Status: Pending

ARMv8 targets such as ARM's FVP Cortex-A32 model can run the 32-bit
ARMv7 kernel.  And these targets often contain GICv3.

Signed-off-by: Ryan Harkin <ryan.harkin@linaro.org>
Signed-off-by: Jon Medhurst <tixy@linaro.org>
---
 arch/arm/mach-versatile/Kconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/mach-versatile/Kconfig b/arch/arm/mach-versatile/Kconfig
index 2ef226194c3a..3d54877fe339 100644
--- a/arch/arm/mach-versatile/Kconfig
+++ b/arch/arm/mach-versatile/Kconfig
@@ -251,6 +251,7 @@ menuconfig ARCH_VEXPRESS
 	depends on ARCH_MULTI_V7
 	select ARM_AMBA
 	select ARM_GIC
+	select ARM_GIC_V3
 	select ARM_GLOBAL_TIMER
 	select ARM_TIMER_SP804
 	select GPIOLIB
-- 
2.30.2

