From 0060b1a4fbe3bc9992f59a2d4cb986821f7bcf13 Mon Sep 17 00:00:00 2001
From: Arunachalam Ganapathy <arunachalam.ganapathy@arm.com>
Date: Mon, 11 Apr 2022 18:31:01 +0100
Subject: [PATCH 3/7] fix(plat/arm): increase sp max image size

Increase ARM_SP_MAX_SIZE to support Trusty image.

Signed-off-by: Arunachalam Ganapathy <arunachalam.ganapathy@arm.com>
Change-Id: I9ef9e755769445aee998062a7fba508fad50b33e
Upstream-Status: Pending [Not submitted to upstream yet]
---
 include/plat/arm/common/fconf_arm_sp_getter.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/include/plat/arm/common/fconf_arm_sp_getter.h b/include/plat/arm/common/fconf_arm_sp_getter.h
index aa628dfd3..3ed953d1c 100644
--- a/include/plat/arm/common/fconf_arm_sp_getter.h
+++ b/include/plat/arm/common/fconf_arm_sp_getter.h
@@ -13,7 +13,7 @@
 /* arm_sp getter */
 #define arm__sp_getter(prop)	arm_sp.prop
 
-#define ARM_SP_MAX_SIZE		U(0xb0000)
+#define ARM_SP_MAX_SIZE		U(0x2000000)
 #define ARM_SP_OWNER_NAME_LEN	U(8)
 
 struct arm_sp_t {
-- 
2.30.2

