From 8dd3e03bd83939746b6a849dce37435ea7581032 Mon Sep 17 00:00:00 2001
From: Davidson K <davidson.kumaresan@arm.com>
Date: Thu, 14 Jul 2022 19:35:41 +0530
Subject: [PATCH 3/7] arm: total_compute: enable psci

psci is used for system reset

Signed-off-by: Davidson K <davidson.kumaresan@arm.com>
Change-Id: Iff4f769dc5e64b6000e892d77a011102b090acfd
Upstream-Status: Submitted [https://patchwork.ozlabs.org/project/uboot/patch/20220809102652.23776-1-davidson.kumaresan@arm.com/]
---
 arch/arm/dts/total_compute.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/dts/total_compute.dts b/arch/arm/dts/total_compute.dts
index 4399269a44..96edacda0b 100644
--- a/arch/arm/dts/total_compute.dts
+++ b/arch/arm/dts/total_compute.dts
@@ -45,4 +45,8 @@
 		clock-frequency = <24000000>;
 		clock-output-names = "bp:clock24mhz";
 	};
+	psci {
+		compatible = "arm,psci-1.0", "arm,psci-0.2";
+		method = "smc";
+	};
 };
-- 
2.34.1

