From 0c3d61d499039ff0828376bb21b4fb1de071b8d2 Mon Sep 17 00:00:00 2001
From: Abdellatif El Khlifi <abdellatif.elkhlifi@arm.com>
Date: Mon, 19 Dec 2022 13:25:23 +0000
Subject: [PATCH 31/43] corstone1000: enable NVM XIP QSPI flash

add the QSPI flash device with block storage capability

Upstream-Status: Submitted
Signed-off-by: Abdellatif El Khlifi <abdellatif.elkhlifi@arm.com>
Signed-off-by: Rui Miguel Silva <rui.silva@linaro.org>
---
 configs/corstone1000_defconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/configs/corstone1000_defconfig b/configs/corstone1000_defconfig
index 1179bf5f3bfd..2986cc95932f 100644
--- a/configs/corstone1000_defconfig
+++ b/configs/corstone1000_defconfig
@@ -58,6 +58,7 @@ CONFIG_DM_SERIAL=y
 CONFIG_USB=y
 CONFIG_USB_ISP1760=y
 CONFIG_ERRNO_STR=y
+CONFIG_NVMXIP_QSPI=y
 CONFIG_EFI_MM_COMM_TEE=y
 CONFIG_ARM_FFA_TRANSPORT=y
 CONFIG_EFI_RUNTIME_UPDATE_CAPSULE=y
-- 
2.39.2

