From 928cb457b9ab2abefbacad655eefdde943b4ee9a Mon Sep 17 00:00:00 2001
From: sahil <sahil@arm.com>
Date: Thu, 17 Mar 2022 16:28:05 +0530
Subject: [PATCH] Platform/ARM/N1sdp: Add support to parse NT_FW_CONFIG

NT_FW_CONFIG DTB contains platform information passed by
Tf-A boot stage.
This information is used for Virtual memory map generation
during PEI phase and passed on to DXE phase as a HOB, where
it is used in ConfigurationManagerDxe.

Upstream-Status: Pending
Signed-off-by: Adam Johnston <adam.johnston@arm.com>
Signed-off-by: Xueliang Zhong <xueliang.zhong@arm.com>
Signed-off-by: sahil <sahil@arm.com>
Change-Id: I54a86277719607eb00d4a472fae8f13c180eafca
---
 .../ConfigurationManager.c                    |  24 ++--
 .../ConfigurationManagerDxe.inf               |   3 +-
 .../ARM/NeoverseN1Soc/Include/NeoverseN1Soc.h |  16 +--
 .../Library/PlatformLib/AArch64/Helper.S      |   4 +-
 .../Library/PlatformLib/PlatformLib.c         |  12 +-
 .../Library/PlatformLib/PlatformLib.inf       |   8 +-
 .../Library/PlatformLib/PlatformLibMem.c      | 103 +++++++++++++++++-
 Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec   |   7 +-
 8 files changed, 152 insertions(+), 25 deletions(-)

diff --git a/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManager.c b/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManager.c
index a6b4cb0e..c15020f5 100644
--- a/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManager.c
+++ b/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManager.c
@@ -1,7 +1,7 @@
 /** @file
   Configuration Manager Dxe
 
-  Copyright (c) 2021, ARM Limited. All rights reserved.<BR>
+  Copyright (c) 2021 - 2023, ARM Limited. All rights reserved.<BR>
 
   SPDX-License-Identifier: BSD-2-Clause-Patent
 
@@ -16,6 +16,7 @@
 #include <IndustryStandard/SerialPortConsoleRedirectionTable.h>
 #include <Library/ArmLib.h>
 #include <Library/DebugLib.h>
+#include <Library/HobLib.h>
 #include <Library/IoLib.h>
 #include <Library/PcdLib.h>
 #include <Library/UefiBootServicesTableLib.h>
@@ -28,6 +29,7 @@
 #include "Platform.h"
 
 extern struct EFI_ACPI_HETEROGENEOUS_MEMORY_ATTRIBUTE_TABLE Hmat;
+static NEOVERSEN1SOC_PLAT_INFO *PlatInfo;
 
 /** The platform configuration repository information.
 */
@@ -1242,13 +1244,11 @@ InitializePlatformRepository (
   IN  EDKII_PLATFORM_REPOSITORY_INFO  * CONST PlatRepoInfo
   )
 {
-  NEOVERSEN1SOC_PLAT_INFO       *PlatInfo;
   UINT64                        Dram2Size;
   UINT64                        RemoteDdrSize;
 
   RemoteDdrSize = 0;
 
-  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE;
   Dram2Size = ((PlatInfo->LocalDdrSize - 2) * SIZE_1GB);
 
   PlatRepoInfo->MemAffInfo[LOCAL_DDR_REGION2].Length = Dram2Size;
@@ -1512,7 +1512,6 @@ GetGicCInfo (
   )
 {
   EDKII_PLATFORM_REPOSITORY_INFO  * PlatformRepo;
-  NEOVERSEN1SOC_PLAT_INFO           *PlatInfo;
   UINT32                            TotalObjCount;
   UINT32                            ObjIndex;
 
@@ -1523,7 +1522,6 @@ GetGicCInfo (
   }
 
   PlatformRepo = This->PlatRepoInfo;
-  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE;
 
   if (PlatInfo->MultichipMode == 1) {
     TotalObjCount = PLAT_CPU_COUNT * 2;
@@ -1623,7 +1621,6 @@ GetStandardNameSpaceObject (
 {
   EFI_STATUS                        Status;
   EDKII_PLATFORM_REPOSITORY_INFO  * PlatformRepo;
-  NEOVERSEN1SOC_PLAT_INFO           *PlatInfo;
   UINT32                            AcpiTableCount;
 
   if ((This == NULL) || (CmObject == NULL)) {
@@ -1634,7 +1631,7 @@ GetStandardNameSpaceObject (
 
   Status = EFI_NOT_FOUND;
   PlatformRepo = This->PlatRepoInfo;
-  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE;
+
   AcpiTableCount = ARRAY_SIZE (PlatformRepo->CmAcpiTableList);
   if (PlatInfo->MultichipMode == 0)
         AcpiTableCount -= 1;
@@ -1697,7 +1694,6 @@ GetArmNameSpaceObject (
 {
   EFI_STATUS                        Status;
   EDKII_PLATFORM_REPOSITORY_INFO  * PlatformRepo;
-  NEOVERSEN1SOC_PLAT_INFO           *PlatInfo;
   UINT32                            GicRedistCount;
   UINT32                            GicCpuCount;
   UINT32                            ProcHierarchyInfoCount;
@@ -1718,8 +1714,6 @@ GetArmNameSpaceObject (
   Status = EFI_NOT_FOUND;
   PlatformRepo = This->PlatRepoInfo;
 
-  // Probe for multi chip information
-  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE;
   if (PlatInfo->MultichipMode == 1) {
     GicRedistCount = 2;
     GicCpuCount = PLAT_CPU_COUNT * 2;
@@ -2162,8 +2156,18 @@ ConfigurationManagerDxeInitialize (
   IN EFI_SYSTEM_TABLE  * SystemTable
   )
 {
+  VOID *PlatInfoHob;
   EFI_STATUS  Status;
 
+  PlatInfoHob = GetFirstGuidHob (&gArmNeoverseN1SocPlatformInfoDescriptorGuid);
+
+  if (PlatInfoHob == NULL) {
+    DEBUG ((DEBUG_ERROR, "Platform HOB is NULL\n"));
+    return EFI_NOT_FOUND;
+  }
+
+  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)GET_GUID_HOB_DATA (PlatInfoHob);
+
   // Initialize the Platform Configuration Repository before installing the
   // Configuration Manager Protocol
   Status = InitializePlatformRepository (
diff --git a/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManagerDxe.inf b/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManagerDxe.inf
index 4f8e7f13..a4e8b783 100644
--- a/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManagerDxe.inf
+++ b/Platform/ARM/N1Sdp/ConfigurationManager/ConfigurationManagerDxe/ConfigurationManagerDxe.inf
@@ -1,7 +1,7 @@
 ## @file
 #  Configuration Manager Dxe
 #
-#  Copyright (c) 2021, ARM Limited. All rights reserved.<BR>
+#  Copyright (c) 2021 - 2023, ARM Limited. All rights reserved.<BR>
 #
 #  SPDX-License-Identifier: BSD-2-Clause-Patent
 #
@@ -42,6 +42,7 @@
 
 [LibraryClasses]
   ArmPlatformLib
+  HobLib
   PrintLib
   UefiBootServicesTableLib
   UefiDriverEntryPoint
diff --git a/Silicon/ARM/NeoverseN1Soc/Include/NeoverseN1Soc.h b/Silicon/ARM/NeoverseN1Soc/Include/NeoverseN1Soc.h
index 097160c7..4966011e 100644
--- a/Silicon/ARM/NeoverseN1Soc/Include/NeoverseN1Soc.h
+++ b/Silicon/ARM/NeoverseN1Soc/Include/NeoverseN1Soc.h
@@ -1,6 +1,6 @@
 /** @file
 *
-* Copyright (c) 2018 - 2020, ARM Limited. All rights reserved.
+* Copyright (c) 2018 - 2023, ARM Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-2-Clause-Patent
 *
@@ -41,11 +41,6 @@
 #define NEOVERSEN1SOC_EXP_PERIPH_BASE0               0x1C000000
 #define NEOVERSEN1SOC_EXP_PERIPH_BASE0_SZ            0x1300000
 
-// Base address to a structure of type NEOVERSEN1SOC_PLAT_INFO which is
-// pre-populated by a earlier boot stage
-#define NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE          (NEOVERSEN1SOC_NON_SECURE_SRAM_BASE + \
-                                                      0x00008000)
-
 /*
  * Platform information structure stored in Non-secure SRAM. Platform
  * information are passed from the trusted firmware with the below structure
@@ -55,12 +50,17 @@
 typedef struct {
   /*! 0 - Single Chip, 1 - Chip to Chip (C2C) */
   UINT8   MultichipMode;
-  /*! Slave count in C2C mode */
-  UINT8   SlaveCount;
+  /*! Secondary chip count in C2C mode */
+  UINT8   SecondaryChipCount;
   /*! Local DDR memory size in GigaBytes */
   UINT8   LocalDdrSize;
   /*! Remote DDR memory size in GigaBytes */
   UINT8   RemoteDdrSize;
 } NEOVERSEN1SOC_PLAT_INFO;
 
+// NT_FW_CONFIG DT structure
+typedef struct {
+  UINT64                  NtFwConfigDtAddr;
+} NEOVERSEN1SOC_NT_FW_CONFIG_INFO_PPI;
+
 #endif
diff --git a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/AArch64/Helper.S b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/AArch64/Helper.S
index 8d2069de..a0b89a7b 100644
--- a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/AArch64/Helper.S
+++ b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/AArch64/Helper.S
@@ -1,6 +1,6 @@
 /** @file
 *
-*  Copyright (c) 2019 - 2020, ARM Limited. All rights reserved.
+*  Copyright (c) 2019 - 2023, ARM Limited. All rights reserved.
 *
 *  SPDX-License-Identifier: BSD-2-Clause-Patent
 *
@@ -25,6 +25,8 @@ GCC_ASM_EXPORT(ArmPlatformIsPrimaryCore)
 // the UEFI firmware through the CPU registers.
 //
 ASM_PFX(ArmPlatformPeiBootAction):
+  adr  x10, NtFwConfigDtBlob
+  str  x0, [x10]
   ret
 
 //
diff --git a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.c b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.c
index c0effd37..2f753be7 100644
--- a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.c
+++ b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.c
@@ -1,6 +1,6 @@
 /** @file
 
-  Copyright (c) 2018-2021, ARM Limited. All rights reserved.<BR>
+  Copyright (c) 2018 - 2023, ARM Limited. All rights reserved.<BR>
 
   SPDX-License-Identifier: BSD-2-Clause-Patent
 
@@ -8,8 +8,12 @@
 
 #include <Library/ArmPlatformLib.h>
 #include <Library/BaseLib.h>
+#include <NeoverseN1Soc.h>
 #include <Ppi/ArmMpCoreInfo.h>
 
+UINT64 NtFwConfigDtBlob;
+STATIC NEOVERSEN1SOC_NT_FW_CONFIG_INFO_PPI mNtFwConfigDtInfoPpi;
+
 STATIC ARM_CORE_INFO mCoreInfoTable[] = {
   { 0x0, 0x0 }, // Cluster 0, Core 0
   { 0x0, 0x1 }, // Cluster 0, Core 1
@@ -46,6 +50,7 @@ ArmPlatformInitialize (
   IN     UINTN                  MpId
   )
 {
+  mNtFwConfigDtInfoPpi.NtFwConfigDtAddr = NtFwConfigDtBlob;
   return RETURN_SUCCESS;
 }
 
@@ -80,6 +85,11 @@ EFI_PEI_PPI_DESCRIPTOR gPlatformPpiTable[] = {
     EFI_PEI_PPI_DESCRIPTOR_PPI,
     &gArmMpCoreInfoPpiGuid,
     &mMpCoreInfoPpi
+  },
+  {
+    EFI_PEI_PPI_DESCRIPTOR_PPI,
+    &gNtFwConfigDtInfoPpiGuid,
+    &mNtFwConfigDtInfoPpi
   }
 };
 
diff --git a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.inf b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.inf
index 96e590cd..78f309c3 100644
--- a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.inf
+++ b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLib.inf
@@ -1,7 +1,7 @@
 ## @file
 #  Platform Library for N1Sdp.
 #
-#  Copyright (c) 2018-2021, ARM Limited. All rights reserved.<BR>
+#  Copyright (c) 2018 - 2023, ARM Limited. All rights reserved.<BR>
 #
 #  SPDX-License-Identifier: BSD-2-Clause-Patent
 #
@@ -18,10 +18,14 @@
 [Packages]
   ArmPkg/ArmPkg.dec
   ArmPlatformPkg/ArmPlatformPkg.dec
+  EmbeddedPkg/EmbeddedPkg.dec
   MdeModulePkg/MdeModulePkg.dec
   MdePkg/MdePkg.dec
   Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec
 
+[LibraryClasses]
+  FdtLib
+
 [Sources.common]
   PlatformLibMem.c
   PlatformLib.c
@@ -59,7 +63,9 @@
   gEfiMdePkgTokenSpaceGuid.PcdPciExpressBaseAddress
 
 [Guids]
+  gArmNeoverseN1SocPlatformInfoDescriptorGuid
   gEfiHobListGuid          ## CONSUMES  ## SystemTable
 
 [Ppis]
   gArmMpCoreInfoPpiGuid
+  gNtFwConfigDtInfoPpiGuid
diff --git a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLibMem.c b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLibMem.c
index 339fa07b..1d53ec75 100644
--- a/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLibMem.c
+++ b/Silicon/ARM/NeoverseN1Soc/Library/PlatformLib/PlatformLibMem.c
@@ -1,6 +1,6 @@
 /** @file
 
-  Copyright (c) 2018 - 2021, ARM Limited. All rights reserved.<BR>
+  Copyright (c) 2018 - 2023, ARM Limited. All rights reserved.<BR>
 
   SPDX-License-Identifier: BSD-2-Clause-Patent
 
@@ -10,11 +10,95 @@
 #include <Library/DebugLib.h>
 #include <Library/HobLib.h>
 #include <Library/MemoryAllocationLib.h>
+#include <Library/PeiServicesLib.h>
+#include <libfdt.h>
 #include <NeoverseN1Soc.h>
 
 // The total number of descriptors, including the final "end-of-table" descriptor.
 #define MAX_VIRTUAL_MEMORY_MAP_DESCRIPTORS 19
 
+/** A helper function to locate the NtFwConfig PPI and get the base address of
+  NT_FW_CONFIG DT from which values are obtained using FDT helper functions.
+
+  @param [out]  plat_info  Pointer to the NeoverseN1Soc PLATFORM_INFO HOB
+
+  @retval EFI_SUCCESS            Success.
+  returns EFI_INVALID_PARAMETER  A parameter is invalid.
+**/
+EFI_STATUS
+GetNeoverseN1SocPlatInfo (
+  OUT NEOVERSEN1SOC_PLAT_INFO *plat_info
+  )
+{
+  CONST UINT32                   *Property;
+  INT32                          Offset;
+  CONST VOID                     *NtFwCfgDtBlob;
+  NEOVERSEN1SOC_NT_FW_CONFIG_INFO_PPI  *NtFwConfigInfoPpi;
+  EFI_STATUS                     Status;
+
+  Status = PeiServicesLocatePpi (
+             &gNtFwConfigDtInfoPpiGuid,
+             0,
+             NULL,
+             (VOID **)&NtFwConfigInfoPpi
+             );
+
+  if (EFI_ERROR (Status)) {
+    DEBUG ((
+      DEBUG_ERROR,
+      "PeiServicesLocatePpi failed with error %r\n",
+      Status
+      ));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  NtFwCfgDtBlob = (VOID *)(UINTN)NtFwConfigInfoPpi->NtFwConfigDtAddr;
+  if (fdt_check_header (NtFwCfgDtBlob) != 0) {
+    DEBUG ((DEBUG_ERROR, "Invalid DTB file %p passed\n", NtFwCfgDtBlob));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  Offset = fdt_subnode_offset (NtFwCfgDtBlob, 0, "platform-info");
+  if (Offset == -FDT_ERR_NOTFOUND) {
+    DEBUG ((DEBUG_ERROR, "Invalid DTB : platform-info node not found\n"));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  Property = fdt_getprop (NtFwCfgDtBlob, Offset, "local-ddr-size", NULL);
+  if (Property == NULL) {
+    DEBUG ((DEBUG_ERROR, "local-ddr-size property not found\n"));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  plat_info->LocalDdrSize = fdt32_to_cpu (*Property);
+
+  Property = fdt_getprop (NtFwCfgDtBlob, Offset, "remote-ddr-size", NULL);
+  if (Property == NULL) {
+    DEBUG ((DEBUG_ERROR, "remote-ddr-size property not found\n"));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  plat_info->RemoteDdrSize = fdt32_to_cpu (*Property);
+
+  Property = fdt_getprop (NtFwCfgDtBlob, Offset, "secondary-chip-count", NULL);
+  if (Property == NULL) {
+    DEBUG ((DEBUG_ERROR, "secondary-chip-count property not found\n"));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  plat_info->SecondaryChipCount = fdt32_to_cpu (*Property);
+
+  Property = fdt_getprop (NtFwCfgDtBlob, Offset, "multichip-mode", NULL);
+  if (Property == NULL) {
+    DEBUG ((DEBUG_ERROR, "multichip-mode property not found\n"));
+    return EFI_INVALID_PARAMETER;
+  }
+
+  plat_info->MultichipMode = fdt32_to_cpu (*Property);
+
+  return EFI_SUCCESS;
+}
+
 /**
   Returns the Virtual Memory Map of the platform.
 
@@ -36,9 +120,24 @@ ArmPlatformGetVirtualMemoryMap (
   NEOVERSEN1SOC_PLAT_INFO       *PlatInfo;
   UINT64                        DramBlock2Size;
   UINT64                        RemoteDdrSize;
+  EFI_STATUS                    Status;
 
   Index = 0;
-  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)NEOVERSEN1SOC_PLAT_INFO_STRUCT_BASE;
+
+  // Create platform info HOB
+  PlatInfo = (NEOVERSEN1SOC_PLAT_INFO *)BuildGuidHob (
+                                        &gArmNeoverseN1SocPlatformInfoDescriptorGuid,
+                                        sizeof (NEOVERSEN1SOC_PLAT_INFO)
+                                        );
+
+  if (PlatInfo == NULL) {
+    DEBUG ((DEBUG_ERROR, "Platform HOB is NULL\n"));
+    ASSERT (FALSE);
+    return;
+  }
+
+  Status = GetNeoverseN1SocPlatInfo (PlatInfo);
+  ASSERT (Status == 0);
   DramBlock2Size = ((UINT64)(PlatInfo->LocalDdrSize -
                              NEOVERSEN1SOC_DRAM_BLOCK1_SIZE / SIZE_1GB) *
                             (UINT64)SIZE_1GB);
diff --git a/Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec b/Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec
index d59f25a5..9e257ebd 100644
--- a/Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec
+++ b/Silicon/ARM/NeoverseN1Soc/NeoverseN1Soc.dec
@@ -1,7 +1,7 @@
 ## @file
 #  Describes the entire platform configuration.
 #
-#  Copyright (c) 2018 - 2021, ARM Limited. All rights reserved.<BR>
+#  Copyright (c) 2018 - 2023, ARM Limited. All rights reserved.<BR>
 #
 #  SPDX-License-Identifier: BSD-2-Clause-Patent
 #
@@ -22,6 +22,8 @@
   Include                        # Root include for the package
 
 [Guids.common]
+  # ARM NeoverseN1Soc Platform Info descriptor
+  gArmNeoverseN1SocPlatformInfoDescriptorGuid = { 0x095cb024, 0x1e00, 0x4d6f, { 0xaa, 0x34, 0x4a, 0xf8, 0xaf, 0x0e, 0xad, 0x99 } }
   gArmNeoverseN1SocTokenSpaceGuid = { 0xab93eb78, 0x60d7, 0x4099, { 0xac, 0xeb, 0x6d, 0xb5, 0x02, 0x58, 0x7c, 0x24 } }
 
 [PcdsFixedAtBuild]
@@ -83,3 +85,6 @@
   gArmNeoverseN1SocTokenSpaceGuid.PcdRemotePcieMmio32Translation|0x40000000000|UINT64|0x0000004F
   gArmNeoverseN1SocTokenSpaceGuid.PcdRemotePcieMmio64Translation|0x40000000000|UINT64|0x00000050
   gArmNeoverseN1SocTokenSpaceGuid.PcdRemotePcieSegmentNumber|2|UINT32|0x00000051
+
+[Ppis]
+  gNtFwConfigDtInfoPpiGuid =  { 0xb50dee0e, 0x577f, 0x47fb, { 0x83, 0xd0, 0x41, 0x78, 0x61, 0x8b, 0x33, 0x8a } }
