From ceae4ec0d459b1ef12e544f4e36d6043a09d3b05 Mon Sep 17 00:00:00 2001
From: Rui Miguel Silva <rui.silva@linaro.org>
Date: Wed, 1 Feb 2023 16:15:30 +0000
Subject: [PATCH 38/43] corstone1000: add boot index

it is expected that the firmware that runs before
u-boot somehow provide the information of the bank
(index) of it is booting.
We will need to extend tf-a to pass that info,
meanwhile just set it to the default bank.

Upstream-Status: Pending
Signed-off-by: Rui Miguel Silva <rui.silva@linaro.org>
---
 board/armltd/corstone1000/corstone1000.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/board/armltd/corstone1000/corstone1000.c b/board/armltd/corstone1000/corstone1000.c
index d6ca6e896140..0a58ccd99cdd 100644
--- a/board/armltd/corstone1000/corstone1000.c
+++ b/board/armltd/corstone1000/corstone1000.c
@@ -106,6 +106,7 @@ int dram_init_banksize(void)
 	return 0;
 }
 
-void reset_cpu(ulong addr)
+void fwu_plat_get_bootidx(int *boot_idx)
 {
+	*boot_idx = 0;
 }
-- 
2.39.2

