# PPPoE Server options

# Maximum segment size, not used for in kernel PPPoE
#MSS=1412

# Device(s) - Space seperated list of devices to listen on
#DEVICES="eth1"

# Local IP
#LOCAL_IP=10.0.0.1

# Starting remote IP
#REMOTE_IP=10.67.15.1

# Service name
#SERVICE_NAME="acme"

# Maximum number of sessions, default is 16
#MAX_SESSIONS=64

# Access concentrator name, default is the hostname
#ACCESS_CONCENTRATOR_NAME="pppoe-rtr-1"
