# This is a basic configuration file with some examples, for device mapper
# multipath.
# For a complete list of the default configuration values, see
# /usr/share/doc/device-mapper-multipath-0.4.9/multipath.conf.defaults
# For a list of configuration options with descriptions, see
# /usr/share/doc/device-mapper-multipath-0.4.9/multipath.conf.annotated

## By default, devices with vendor = "IBM" and product = "S/390.*" are
## blacklisted. To enable mulitpathing on these devies, uncomment the
## following lines.
#blacklist_exceptions {
#	device {
#		vendor	"IBM"
#		product	"S/390.*"
#	}
#}

## Use user friendly names, instead of using WWIDs as names.
defaults {
	user_friendly_names yes
}
##
## Here is an example of how to configure some standard options.
##
#
#defaults {
#	udev_dir		/dev
#	polling_interval 	10
#	selector		"round-robin 0"
#	path_grouping_policy	multibus
#	getuid_callout		"/lib/udev/scsi_id --whitelisted --device=/dev/%n"
#	prio			alua
#	path_checker		readsector0
#	rr_min_io		100
#	max_fds			8192
#	rr_weight		priorities
#	failback		immediate
#	no_path_retry		fail
#	user_friendly_names	yes
#}
##
## The wwid line in the following blacklist section is shown as an example
## of how to blacklist devices by wwid.  The 2 devnode lines are the
## compiled in default blacklist. If you want to blacklist entire types
## of devices, such as all scsi devices, you should use a devnode line.
## However, if you want to blacklist specific devices, you should use
## a wwid line.  Since there is no guarantee that a specific device will
## not change names on reboot (from /dev/sda to /dev/sdb for example)
## devnode lines are not recommended for blacklisting specific devices.
##
#blacklist {
#       wwid 26353900f02796769
#	devnode "^(ram|raw|loop|fd|md|dm-|sr|scd|st)[0-9]*"
#	devnode "^hd[a-z]"
#}
#multipaths {
#	multipath {
#		wwid			3600508b4000156d700012000000b0000
#		alias			yellow
#		path_grouping_policy	multibus
#		path_checker		readsector0
#		path_selector		"round-robin 0"
#		failback		manual
#		rr_weight		priorities
#		no_path_retry		5
#	}
#	multipath {
#		wwid			1DEC_____321816758474
#		alias			red
#	}
#}
#devices {
#	device {
#		vendor			"COMPAQ  "
#		product			"HSV110 (C)COMPAQ"
#		path_grouping_policy	multibus
#		getuid_callout          "/lib/udev/scsi_id --whitelisted --device=/dev/%n"
#		path_checker		readsector0
#		path_selector		"round-robin 0"
#		hardware_handler	"0"
#		failback		15
#		rr_weight		priorities
#		no_path_retry		queue
#	}
#	device {
#		vendor			"COMPAQ  "
#		product			"MSA1000         "
#		path_grouping_policy	multibus
#	}
#}
