isic: add missing header file

Backport:
http://pkgs.fedoraproject.org/cgit/isic.git/tree/isic-0.07-netinet.patch

Signed-off-by: Armin Kuster <akuster808@gmail.com>

Index: isic-0.07/multisic.c
===================================================================
--- isic-0.07.orig/multisic.c
+++ isic-0.07/multisic.c
@@ -1,5 +1,8 @@
 #include "isic.h"
 
+#include <netinet/udp.h>
+/*#include <netinet/tcp.h>*/
+
 /* This is tuned for ethernet sized frames (1500 bytes)
  * For user over a modem or frame (or other) you will have to change the
  * 'rand() & 0x4ff' line below.  The 0x4ff needs to be less than the size of
Index: isic-0.07/tcpsic.c
===================================================================
--- isic-0.07.orig/tcpsic.c
+++ isic-0.07/tcpsic.c
@@ -1,5 +1,7 @@
 #include "isic.h"
 
+#include <netinet/tcp.h>
+
 /* This is tuned for ethernet sized frames (1500 bytes)
  * For user over a modem or frame (or other) you will have to change the
  * 'rand() & 0x4ff' line below.  The 0x4ff needs to be less than the size of
Index: isic-0.07/tcpsic6.c
===================================================================
--- isic-0.07.orig/tcpsic6.c
+++ isic-0.07/tcpsic6.c
@@ -1,5 +1,7 @@
 #include "isic.h"
 
+#include <netinet/tcp.h>
+
 /* This is tuned for ethernet sized frames (1500 bytes)
  * For user over a modem or frame (or other) you will have to change the
  * 'rand() & 0x4ff' line below.  The 0x4ff needs to be less than the size of
Index: isic-0.07/udpsic.c
===================================================================
--- isic-0.07.orig/udpsic.c
+++ isic-0.07/udpsic.c
@@ -1,5 +1,7 @@
 #include "isic.h"
 
+#include <netinet/udp.h>
+
 /* This is tuned for ethernet sized frames (1500 bytes)
  * For user over a modem or frame (or other) you will have to change the
  * 'rand() & 0x4ff' line below.  The 0x4ff needs to be less than the size of
Index: isic-0.07/udpsic6.c
===================================================================
--- isic-0.07.orig/udpsic6.c
+++ isic-0.07/udpsic6.c
@@ -1,5 +1,7 @@
 #include "isic.h"
 
+#include <netinet/udp.h>
+
 /* This is tuned for ethernet sized frames (1500 bytes)
  * For user over a modem or frame (or other) you will have to change the
  * 'rand() & 0x4ff' line below.  The 0x4ff needs to be less than the size of
