From 46ea520a3c80914ae5ad3e35be7b8650706da3e6 Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Thu, 17 Dec 2009 14:27:15 -0800
Subject: [PATCH 19/32] ARM: OMAP: Add twl4030 madc support to Overo

Signed-off-by: Steve Sakoman <steve@sakoman.com>
---
 arch/arm/mach-omap2/board-overo.c |    5 +++++
 1 files changed, 5 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-overo.c b/arch/arm/mach-omap2/board-overo.c
index 59ca333..86f76e9 100644
--- a/arch/arm/mach-omap2/board-overo.c
+++ b/arch/arm/mach-omap2/board-overo.c
@@ -637,10 +637,15 @@ static struct twl4030_codec_data overo_codec_data = {
 	.audio = &overo_audio_data,
 };
 
+static struct twl4030_madc_platform_data overo_madc_data = {
+	.irq_line	= 1,
+};
+
 static struct twl4030_platform_data overo_twldata = {
 	.irq_base	= TWL4030_IRQ_BASE,
 	.irq_end	= TWL4030_IRQ_END,
 	.gpio		= &overo_gpio_data,
+	.madc		= &overo_madc_data,
 	.usb		= &overo_usb_data,
 	.codec		= &overo_codec_data,
 	.vmmc1		= &overo_vmmc1,
-- 
1.6.6.1

