From 1714658473cd1abe2ad5f6fa81119384297a926e Mon Sep 17 00:00:00 2001
From: archit taneja <archit@ti.com>
Date: Fri, 5 Aug 2011 07:19:21 +0000
Subject: [PATCH 1/4] OMAP_VOUT: Fix build break caused by update_mode removal in DSS2

The DSS2 driver does not support the configuration of the update_mode of a
panel anymore. Remove the setting of update_mode done in omap_vout_probe().
Ignore configuration of TE since omap_vout driver doesn't support manual update
displays anyway.

Signed-off-by: Archit Taneja <archit@ti.com>
Tested-by: Koen Kooi <koen@dominion.thruhere.net>
Signed-off-by: Vaibhav Hiremath <hvaibhav@ti.com>
---
 drivers/media/video/omap/omap_vout.c |   13 -------------
 1 files changed, 0 insertions(+), 13 deletions(-)

diff --git a/drivers/media/video/omap/omap_vout.c b/drivers/media/video/omap/omap_vout.c
index 4d07c58..d17d6b6 100644
--- a/drivers/media/video/omap/omap_vout.c
+++ b/drivers/media/video/omap/omap_vout.c
@@ -2557,19 +2557,6 @@ static int __init omap_vout_probe(struct platform_device *pdev)
 					"'%s' Display already enabled\n",
 					def_display->name);
 			}
-			/* set the update mode */
-			if (def_display->caps &
-					OMAP_DSS_DISPLAY_CAP_MANUAL_UPDATE) {
-				if (dssdrv->enable_te)
-					dssdrv->enable_te(def_display, 0);
-				if (dssdrv->set_update_mode)
-					dssdrv->set_update_mode(def_display,
-							OMAP_DSS_UPDATE_MANUAL);
-			} else {
-				if (dssdrv->set_update_mode)
-					dssdrv->set_update_mode(def_display,
-							OMAP_DSS_UPDATE_AUTO);
-			}
 		}
 	}
 
-- 
1.6.6.1

