From 87d3b74e7a34d655ae16a847986a9a7ac05bc29d Mon Sep 17 00:00:00 2001
From: Andy Green <andy@warmcat.com>
Date: Sun, 10 Jul 2011 05:27:14 -0600
Subject: [PATCH 068/149] I2C: OMAP2+: Set hwmod flags to only allow 16-bit accesses to i2c

Peter Maydell noticed when running under QEMU he was getting
errors reporting 32-bit access to I2C peripheral unit registers
that are documented to be 8 or 16-bit only[1][2]

The I2C driver is blameless as it wraps its accesses in a
function using __raw_writew and __raw_readw, it turned out it
is the hwmod stuff.

However the hwmod code already has a flag to force a
perhipheral unit to only be accessed using 16-bit operations.

This patch applies the 16-bit only flag to the 2430,
OMAP3xxx and OMAP44xx hwmod structs.  2420 was already
correctly marked up as 16-bit.

The 2430 change will need testing by TI as arranged
in the comments to the previous patch version.

When the 16-bit flag is or-ed with other flags, it is placed
first as requested in comments.

[1] OMAP4430 Technical reference manual section 23.1.6.2
[2] OMAP3530 Techincal reference manual section 18.6

Cc: patches@linaro.org
Cc: Ben Dooks <ben-linux@fluff.org>
Reported-by: Peter Maydell <peter.maydell@linaro.org>
Signed-off-by: Andy Green <andy.green@linaro.org>
Signed-off-by: Tony Lindgren <tony@atomide.com>
Signed-off-by: Kevin Hilman <khilman@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/omap_hwmod_2430_data.c |    2 ++
 arch/arm/mach-omap2/omap_hwmod_3xxx_data.c |    3 +++
 arch/arm/mach-omap2/omap_hwmod_44xx_data.c |    8 ++++----
 3 files changed, 9 insertions(+), 4 deletions(-)

diff --git a/arch/arm/mach-omap2/omap_hwmod_2430_data.c b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
index 2a52f02..19ddf08 100644
--- a/arch/arm/mach-omap2/omap_hwmod_2430_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
@@ -1092,6 +1092,7 @@ static struct omap_hwmod_ocp_if *omap2430_i2c1_slaves[] = {
 
 static struct omap_hwmod omap2430_i2c1_hwmod = {
 	.name		= "i2c1",
+	.flags		= HWMOD_16BIT_REG,
 	.mpu_irqs	= omap2_i2c1_mpu_irqs,
 	.sdma_reqs	= omap2_i2c1_sdma_reqs,
 	.main_clk	= "i2chs1_fck",
@@ -1127,6 +1128,7 @@ static struct omap_hwmod_ocp_if *omap2430_i2c2_slaves[] = {
 
 static struct omap_hwmod omap2430_i2c2_hwmod = {
 	.name		= "i2c2",
+	.flags		= HWMOD_16BIT_REG,
 	.mpu_irqs	= omap2_i2c2_mpu_irqs,
 	.sdma_reqs	= omap2_i2c2_sdma_reqs,
 	.main_clk	= "i2chs2_fck",
diff --git a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
index 1a52716..542a11b 100644
--- a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
@@ -1615,6 +1615,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_i2c1_slaves[] = {
 
 static struct omap_hwmod omap3xxx_i2c1_hwmod = {
 	.name		= "i2c1",
+	.flags		= HWMOD_16BIT_REG,
 	.mpu_irqs	= omap2_i2c1_mpu_irqs,
 	.sdma_reqs	= omap2_i2c1_sdma_reqs,
 	.main_clk	= "i2c1_fck",
@@ -1646,6 +1647,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_i2c2_slaves[] = {
 
 static struct omap_hwmod omap3xxx_i2c2_hwmod = {
 	.name		= "i2c2",
+	.flags		= HWMOD_16BIT_REG,
 	.mpu_irqs	= omap2_i2c2_mpu_irqs,
 	.sdma_reqs	= omap2_i2c2_sdma_reqs,
 	.main_clk	= "i2c2_fck",
@@ -1688,6 +1690,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_i2c3_slaves[] = {
 
 static struct omap_hwmod omap3xxx_i2c3_hwmod = {
 	.name		= "i2c3",
+	.flags		= HWMOD_16BIT_REG,
 	.mpu_irqs	= i2c3_mpu_irqs,
 	.sdma_reqs	= i2c3_sdma_reqs,
 	.main_clk	= "i2c3_fck",
diff --git a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
index b25ab83..2ebccb8 100644
--- a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
@@ -2201,7 +2201,7 @@ static struct omap_hwmod_ocp_if *omap44xx_i2c1_slaves[] = {
 static struct omap_hwmod omap44xx_i2c1_hwmod = {
 	.name		= "i2c1",
 	.class		= &omap44xx_i2c_hwmod_class,
-	.flags		= HWMOD_INIT_NO_RESET,
+	.flags		= HWMOD_16BIT_REG | HWMOD_INIT_NO_RESET,
 	.mpu_irqs	= omap44xx_i2c1_irqs,
 	.sdma_reqs	= omap44xx_i2c1_sdma_reqs,
 	.main_clk	= "i2c1_fck",
@@ -2254,7 +2254,7 @@ static struct omap_hwmod_ocp_if *omap44xx_i2c2_slaves[] = {
 static struct omap_hwmod omap44xx_i2c2_hwmod = {
 	.name		= "i2c2",
 	.class		= &omap44xx_i2c_hwmod_class,
-	.flags		= HWMOD_INIT_NO_RESET,
+	.flags		= HWMOD_16BIT_REG | HWMOD_INIT_NO_RESET,
 	.mpu_irqs	= omap44xx_i2c2_irqs,
 	.sdma_reqs	= omap44xx_i2c2_sdma_reqs,
 	.main_clk	= "i2c2_fck",
@@ -2307,7 +2307,7 @@ static struct omap_hwmod_ocp_if *omap44xx_i2c3_slaves[] = {
 static struct omap_hwmod omap44xx_i2c3_hwmod = {
 	.name		= "i2c3",
 	.class		= &omap44xx_i2c_hwmod_class,
-	.flags		= HWMOD_INIT_NO_RESET,
+	.flags		= HWMOD_16BIT_REG | HWMOD_INIT_NO_RESET,
 	.mpu_irqs	= omap44xx_i2c3_irqs,
 	.sdma_reqs	= omap44xx_i2c3_sdma_reqs,
 	.main_clk	= "i2c3_fck",
@@ -2360,7 +2360,7 @@ static struct omap_hwmod_ocp_if *omap44xx_i2c4_slaves[] = {
 static struct omap_hwmod omap44xx_i2c4_hwmod = {
 	.name		= "i2c4",
 	.class		= &omap44xx_i2c_hwmod_class,
-	.flags		= HWMOD_INIT_NO_RESET,
+	.flags		= HWMOD_16BIT_REG | HWMOD_INIT_NO_RESET,
 	.mpu_irqs	= omap44xx_i2c4_irqs,
 	.sdma_reqs	= omap44xx_i2c4_sdma_reqs,
 	.main_clk	= "i2c4_fck",
-- 
1.6.6.1

