From a9847b4b964b65b8a3f041550c4a15342d151b88 Mon Sep 17 00:00:00 2001
From: Roger Monk <r-monk@ti.com>
Date: Wed, 19 May 2010 13:43:53 +0100
Subject: [PATCH] Hawkboard Support:  Add Hawkboard (DA850/OMAPL138 based) Board Support

   * Hawkboard(.org) (http://www.hawkboard.org) Board Support
   * Support based on DA850_OMAPL138 EVM Board Support
   * This board contains the following components
      * DA850/OMAPL138/(AM1808) - ARM9 + 674x DSP + PRU + Peripherals
      * 128MB DDR2 SDRAM (MT47H64M16HR-3:G)
      * 128MB NAND Flash (MT29F1G08ABCHC-ET)
      * Video Capture (TVP5147M1) - Composite Video
      * Video Display (THS8135) - VGA
      * Ethernet (LAN8710A)
      * Audio (AIC31xx) - Stereo Audio Codec
      * Serial ATA
      * SD/MMC
      * USB 1.1 (OHCI) (Host/Gadget)
      * USB 2.0 (MUSB) (Host)
      * Serial Console
      * CpuFreq/CpuIdle/PM(Suspend-to-Ram) with RTC wakeup
   * TODO
      * USB MUSB (host) Disconnect Issues
      * USB MUSB (gadget) Config + Testing
      * VPIF Capture Driver creates 2 device nodes
      * VPIF Capture Driver fails with mplayer tv:// test
      * Further Board File Cleanup
   * Notes
      * RTC not tested
      * RTC requires battery populated on hawkboard
         * CONFIG_DRV_RTC_OMAP should be disabled if no battery
      * No Regulator on hawkboard - CONFIG_REGULATOR should be disabled
      * Wake-Up source from pm (suspend-to-ram) is RTC

Signed-off-by: Roger Monk <r-monk@ti.com>
---
 .../arm/configs/da850_omapl138_hawkboard_defconfig | 1867 ++++++++++++++++++++
 arch/arm/mach-davinci/Kconfig                      |    7 +
 arch/arm/mach-davinci/Makefile                     |    1 +
 arch/arm/mach-davinci/board-da850-hawk.c           |  657 +++++++
 arch/arm/mach-davinci/da850.c                      |    2 +-
 arch/arm/mach-davinci/devices-da8xx.c              |    8 +
 arch/arm/mach-davinci/include/mach/da8xx.h         |    2 +
 arch/arm/mach-davinci/include/mach/debug-macro.S   |    3 +-
 drivers/media/video/Kconfig                        |    4 +-
 drivers/video/da8xx-fb.c                           |   14 +
 sound/soc/davinci/Kconfig                          |    6 +-
 sound/soc/davinci/davinci-evm.c                    |    5 +-
 12 files changed, 2567 insertions(+), 9 deletions(-)
 create mode 100644 arch/arm/configs/da850_omapl138_hawkboard_defconfig
 create mode 100644 arch/arm/mach-davinci/board-da850-hawk.c

diff --git a/arch/arm/configs/da850_omapl138_hawkboard_defconfig b/arch/arm/configs/da850_omapl138_hawkboard_defconfig
new file mode 100644
index 0000000..19fcbdf
--- /dev/null
+++ b/arch/arm/configs/da850_omapl138_hawkboard_defconfig
@@ -0,0 +1,1867 @@
+#
+# Automatically generated make config: don't edit
+# Linux kernel version: 2.6.33-rc4
+# Tue Mar  2 15:34:51 2010
+#
+CONFIG_ARM=y
+CONFIG_SYS_SUPPORTS_APM_EMULATION=y
+CONFIG_GENERIC_GPIO=y
+CONFIG_GENERIC_TIME=y
+CONFIG_GENERIC_CLOCKEVENTS=y
+CONFIG_GENERIC_HARDIRQS=y
+CONFIG_STACKTRACE_SUPPORT=y
+CONFIG_HAVE_LATENCYTOP_SUPPORT=y
+CONFIG_LOCKDEP_SUPPORT=y
+CONFIG_TRACE_IRQFLAGS_SUPPORT=y
+CONFIG_HARDIRQS_SW_RESEND=y
+CONFIG_GENERIC_IRQ_PROBE=y
+CONFIG_RWSEM_GENERIC_SPINLOCK=y
+CONFIG_ARCH_HAS_CPUFREQ=y
+CONFIG_GENERIC_HWEIGHT=y
+CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_ZONE_DMA=y
+CONFIG_GENERIC_HARDIRQS_NO__DO_IRQ=y
+CONFIG_VECTORS_BASE=0xffff0000
+CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
+CONFIG_CONSTRUCTORS=y
+
+#
+# General setup
+#
+CONFIG_EXPERIMENTAL=y
+CONFIG_BROKEN_ON_SMP=y
+CONFIG_LOCK_KERNEL=y
+CONFIG_INIT_ENV_ARG_LIMIT=32
+CONFIG_LOCALVERSION=""
+# CONFIG_LOCALVERSION_AUTO is not set
+CONFIG_HAVE_KERNEL_GZIP=y
+CONFIG_HAVE_KERNEL_LZO=y
+CONFIG_KERNEL_GZIP=y
+# CONFIG_KERNEL_BZIP2 is not set
+# CONFIG_KERNEL_LZMA is not set
+# CONFIG_KERNEL_LZO is not set
+CONFIG_SWAP=y
+CONFIG_SYSVIPC=y
+CONFIG_SYSVIPC_SYSCTL=y
+CONFIG_POSIX_MQUEUE=y
+CONFIG_POSIX_MQUEUE_SYSCTL=y
+# CONFIG_BSD_PROCESS_ACCT is not set
+# CONFIG_TASKSTATS is not set
+# CONFIG_AUDIT is not set
+
+#
+# RCU Subsystem
+#
+CONFIG_TREE_RCU=y
+# CONFIG_TREE_PREEMPT_RCU is not set
+# CONFIG_TINY_RCU is not set
+# CONFIG_RCU_TRACE is not set
+CONFIG_RCU_FANOUT=32
+# CONFIG_RCU_FANOUT_EXACT is not set
+# CONFIG_TREE_RCU_TRACE is not set
+CONFIG_IKCONFIG=y
+CONFIG_IKCONFIG_PROC=y
+CONFIG_LOG_BUF_SHIFT=14
+CONFIG_GROUP_SCHED=y
+CONFIG_FAIR_GROUP_SCHED=y
+# CONFIG_RT_GROUP_SCHED is not set
+CONFIG_USER_SCHED=y
+# CONFIG_CGROUP_SCHED is not set
+# CONFIG_CGROUPS is not set
+# CONFIG_SYSFS_DEPRECATED_V2 is not set
+# CONFIG_RELAY is not set
+# CONFIG_NAMESPACES is not set
+CONFIG_BLK_DEV_INITRD=y
+CONFIG_INITRAMFS_SOURCE=""
+CONFIG_RD_GZIP=y
+# CONFIG_RD_BZIP2 is not set
+# CONFIG_RD_LZMA is not set
+# CONFIG_RD_LZO is not set
+CONFIG_CC_OPTIMIZE_FOR_SIZE=y
+CONFIG_SYSCTL=y
+CONFIG_ANON_INODES=y
+CONFIG_EMBEDDED=y
+CONFIG_UID16=y
+CONFIG_SYSCTL_SYSCALL=y
+CONFIG_KALLSYMS=y
+# CONFIG_KALLSYMS_EXTRA_PASS is not set
+CONFIG_HOTPLUG=y
+CONFIG_PRINTK=y
+CONFIG_BUG=y
+CONFIG_ELF_CORE=y
+CONFIG_BASE_FULL=y
+CONFIG_FUTEX=y
+CONFIG_EPOLL=y
+CONFIG_SIGNALFD=y
+CONFIG_TIMERFD=y
+CONFIG_EVENTFD=y
+CONFIG_SHMEM=y
+CONFIG_AIO=y
+
+#
+# Kernel Performance Events And Counters
+#
+CONFIG_VM_EVENT_COUNTERS=y
+CONFIG_SLUB_DEBUG=y
+CONFIG_COMPAT_BRK=y
+# CONFIG_SLAB is not set
+CONFIG_SLUB=y
+# CONFIG_SLOB is not set
+# CONFIG_PROFILING is not set
+CONFIG_HAVE_OPROFILE=y
+# CONFIG_KPROBES is not set
+CONFIG_HAVE_KPROBES=y
+CONFIG_HAVE_KRETPROBES=y
+CONFIG_HAVE_CLK=y
+
+#
+# GCOV-based kernel profiling
+#
+# CONFIG_GCOV_KERNEL is not set
+# CONFIG_SLOW_WORK is not set
+CONFIG_HAVE_GENERIC_DMA_COHERENT=y
+CONFIG_SLABINFO=y
+CONFIG_RT_MUTEXES=y
+CONFIG_BASE_SMALL=0
+CONFIG_MODULES=y
+# CONFIG_MODULE_FORCE_LOAD is not set
+CONFIG_MODULE_UNLOAD=y
+CONFIG_MODULE_FORCE_UNLOAD=y
+CONFIG_MODVERSIONS=y
+# CONFIG_MODULE_SRCVERSION_ALL is not set
+CONFIG_BLOCK=y
+CONFIG_LBDAF=y
+# CONFIG_BLK_DEV_BSG is not set
+# CONFIG_BLK_DEV_INTEGRITY is not set
+
+#
+# IO Schedulers
+#
+CONFIG_IOSCHED_NOOP=y
+# CONFIG_IOSCHED_DEADLINE is not set
+# CONFIG_IOSCHED_CFQ is not set
+# CONFIG_DEFAULT_DEADLINE is not set
+# CONFIG_DEFAULT_CFQ is not set
+CONFIG_DEFAULT_NOOP=y
+CONFIG_DEFAULT_IOSCHED="noop"
+# CONFIG_INLINE_SPIN_TRYLOCK is not set
+# CONFIG_INLINE_SPIN_TRYLOCK_BH is not set
+# CONFIG_INLINE_SPIN_LOCK is not set
+# CONFIG_INLINE_SPIN_LOCK_BH is not set
+# CONFIG_INLINE_SPIN_LOCK_IRQ is not set
+# CONFIG_INLINE_SPIN_LOCK_IRQSAVE is not set
+# CONFIG_INLINE_SPIN_UNLOCK is not set
+# CONFIG_INLINE_SPIN_UNLOCK_BH is not set
+# CONFIG_INLINE_SPIN_UNLOCK_IRQ is not set
+# CONFIG_INLINE_SPIN_UNLOCK_IRQRESTORE is not set
+# CONFIG_INLINE_READ_TRYLOCK is not set
+# CONFIG_INLINE_READ_LOCK is not set
+# CONFIG_INLINE_READ_LOCK_BH is not set
+# CONFIG_INLINE_READ_LOCK_IRQ is not set
+# CONFIG_INLINE_READ_LOCK_IRQSAVE is not set
+# CONFIG_INLINE_READ_UNLOCK is not set
+# CONFIG_INLINE_READ_UNLOCK_BH is not set
+# CONFIG_INLINE_READ_UNLOCK_IRQ is not set
+# CONFIG_INLINE_READ_UNLOCK_IRQRESTORE is not set
+# CONFIG_INLINE_WRITE_TRYLOCK is not set
+# CONFIG_INLINE_WRITE_LOCK is not set
+# CONFIG_INLINE_WRITE_LOCK_BH is not set
+# CONFIG_INLINE_WRITE_LOCK_IRQ is not set
+# CONFIG_INLINE_WRITE_LOCK_IRQSAVE is not set
+# CONFIG_INLINE_WRITE_UNLOCK is not set
+# CONFIG_INLINE_WRITE_UNLOCK_BH is not set
+# CONFIG_INLINE_WRITE_UNLOCK_IRQ is not set
+# CONFIG_INLINE_WRITE_UNLOCK_IRQRESTORE is not set
+# CONFIG_MUTEX_SPIN_ON_OWNER is not set
+CONFIG_FREEZER=y
+
+#
+# System Type
+#
+CONFIG_MMU=y
+# CONFIG_ARCH_AAEC2000 is not set
+# CONFIG_ARCH_INTEGRATOR is not set
+# CONFIG_ARCH_REALVIEW is not set
+# CONFIG_ARCH_VERSATILE is not set
+# CONFIG_ARCH_AT91 is not set
+# CONFIG_ARCH_CLPS711X is not set
+# CONFIG_ARCH_GEMINI is not set
+# CONFIG_ARCH_EBSA110 is not set
+# CONFIG_ARCH_EP93XX is not set
+# CONFIG_ARCH_FOOTBRIDGE is not set
+# CONFIG_ARCH_MXC is not set
+# CONFIG_ARCH_STMP3XXX is not set
+# CONFIG_ARCH_NETX is not set
+# CONFIG_ARCH_H720X is not set
+# CONFIG_ARCH_NOMADIK is not set
+# CONFIG_ARCH_IOP13XX is not set
+# CONFIG_ARCH_IOP32X is not set
+# CONFIG_ARCH_IOP33X is not set
+# CONFIG_ARCH_IXP23XX is not set
+# CONFIG_ARCH_IXP2000 is not set
+# CONFIG_ARCH_IXP4XX is not set
+# CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_DOVE is not set
+# CONFIG_ARCH_KIRKWOOD is not set
+# CONFIG_ARCH_LOKI is not set
+# CONFIG_ARCH_MV78XX0 is not set
+# CONFIG_ARCH_ORION5X is not set
+# CONFIG_ARCH_MMP is not set
+# CONFIG_ARCH_KS8695 is not set
+# CONFIG_ARCH_NS9XXX is not set
+# CONFIG_ARCH_W90X900 is not set
+# CONFIG_ARCH_PNX4008 is not set
+# CONFIG_ARCH_PXA is not set
+# CONFIG_ARCH_MSM is not set
+# CONFIG_ARCH_RPC is not set
+# CONFIG_ARCH_SA1100 is not set
+# CONFIG_ARCH_S3C2410 is not set
+# CONFIG_ARCH_S3C64XX is not set
+# CONFIG_ARCH_S5PC1XX is not set
+# CONFIG_ARCH_SHARK is not set
+# CONFIG_ARCH_LH7A40X is not set
+# CONFIG_ARCH_U300 is not set
+CONFIG_ARCH_DAVINCI=y
+# CONFIG_ARCH_OMAP is not set
+# CONFIG_ARCH_BCMRING is not set
+# CONFIG_ARCH_U8500 is not set
+CONFIG_CP_INTC=y
+
+#
+# TI DaVinci Implementations
+#
+
+#
+# DaVinci Core Type
+#
+# CONFIG_ARCH_DAVINCI_DM644x is not set
+# CONFIG_ARCH_DAVINCI_DM355 is not set
+# CONFIG_ARCH_DAVINCI_DM646x is not set
+# CONFIG_ARCH_DAVINCI_DA830 is not set
+CONFIG_ARCH_DAVINCI_DA850=y
+# CONFIG_DA8XX_MAX_SPEED_300 is not set
+# CONFIG_DA8XX_MAX_SPEED_372 is not set
+# CONFIG_DA8XX_MAX_SPEED_408 is not set
+CONFIG_DA8XX_MAX_SPEED_456=y
+CONFIG_ARCH_DAVINCI_DA8XX=y
+# CONFIG_ARCH_DAVINCI_DM365 is not set
+
+#
+# DaVinci Board Type
+#
+# CONFIG_MACH_DAVINCI_DA850_EVM is not set
+CONFIG_MACH_OMAPL138_HAWKBOARD=y
+CONFIG_DAVINCI_MUX=y
+# CONFIG_DAVINCI_MUX_DEBUG is not set
+# CONFIG_DAVINCI_MUX_WARNINGS is not set
+CONFIG_DAVINCI_RESET_CLOCKS=y
+CONFIG_DAVINCI_MCBSP=y
+# CONFIG_DAVINCI_MCBSP0 is not set
+CONFIG_DAVINCI_MCBSP1=y
+
+#
+# Processor Type
+#
+CONFIG_CPU_ARM926T=y
+CONFIG_CPU_32v5=y
+CONFIG_CPU_ABRT_EV5TJ=y
+CONFIG_CPU_PABRT_LEGACY=y
+CONFIG_CPU_CACHE_VIVT=y
+CONFIG_CPU_COPY_V4WB=y
+CONFIG_CPU_TLB_V4WBI=y
+CONFIG_CPU_CP15=y
+CONFIG_CPU_CP15_MMU=y
+
+#
+# Processor Features
+#
+CONFIG_ARM_THUMB=y
+# CONFIG_CPU_ICACHE_DISABLE is not set
+# CONFIG_CPU_DCACHE_DISABLE is not set
+# CONFIG_CPU_DCACHE_WRITETHROUGH is not set
+# CONFIG_CPU_CACHE_ROUND_ROBIN is not set
+CONFIG_ARM_L1_CACHE_SHIFT=5
+CONFIG_COMMON_CLKDEV=y
+
+#
+# Bus support
+#
+# CONFIG_PCI_SYSCALL is not set
+# CONFIG_ARCH_SUPPORTS_MSI is not set
+# CONFIG_PCCARD is not set
+
+#
+# Kernel Features
+#
+CONFIG_TICK_ONESHOT=y
+CONFIG_NO_HZ=y
+CONFIG_HIGH_RES_TIMERS=y
+CONFIG_GENERIC_CLOCKEVENTS_BUILD=y
+CONFIG_VMSPLIT_3G=y
+# CONFIG_VMSPLIT_2G is not set
+# CONFIG_VMSPLIT_1G is not set
+CONFIG_PAGE_OFFSET=0xC0000000
+# CONFIG_PREEMPT_NONE is not set
+# CONFIG_PREEMPT_VOLUNTARY is not set
+CONFIG_PREEMPT=y
+CONFIG_HZ=100
+CONFIG_AEABI=y
+# CONFIG_OABI_COMPAT is not set
+CONFIG_ARCH_HAS_HOLES_MEMORYMODEL=y
+# CONFIG_ARCH_SPARSEMEM_DEFAULT is not set
+# CONFIG_ARCH_SELECT_MEMORY_MODEL is not set
+# CONFIG_HIGHMEM is not set
+CONFIG_SELECT_MEMORY_MODEL=y
+CONFIG_FLATMEM_MANUAL=y
+# CONFIG_DISCONTIGMEM_MANUAL is not set
+# CONFIG_SPARSEMEM_MANUAL is not set
+CONFIG_FLATMEM=y
+CONFIG_FLAT_NODE_MEM_MAP=y
+CONFIG_PAGEFLAGS_EXTENDED=y
+CONFIG_SPLIT_PTLOCK_CPUS=999999
+# CONFIG_PHYS_ADDR_T_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=1
+CONFIG_BOUNCE=y
+CONFIG_VIRT_TO_BUS=y
+# CONFIG_KSM is not set
+CONFIG_DEFAULT_MMAP_MIN_ADDR=4096
+CONFIG_LEDS=y
+# CONFIG_LEDS_CPU is not set
+CONFIG_ALIGNMENT_TRAP=y
+# CONFIG_UACCESS_WITH_MEMCPY is not set
+
+#
+# Boot options
+#
+CONFIG_ZBOOT_ROM_TEXT=0x0
+CONFIG_ZBOOT_ROM_BSS=0x0
+CONFIG_CMDLINE=""
+# CONFIG_XIP_KERNEL is not set
+# CONFIG_KEXEC is not set
+
+#
+# CPU Power Management
+#
+CONFIG_CPU_FREQ=y
+CONFIG_CPU_FREQ_TABLE=y
+# CONFIG_CPU_FREQ_DEBUG is not set
+CONFIG_CPU_FREQ_STAT=y
+# CONFIG_CPU_FREQ_STAT_DETAILS is not set
+# CONFIG_CPU_FREQ_DEFAULT_GOV_PERFORMANCE is not set
+# CONFIG_CPU_FREQ_DEFAULT_GOV_POWERSAVE is not set
+CONFIG_CPU_FREQ_DEFAULT_GOV_USERSPACE=y
+# CONFIG_CPU_FREQ_DEFAULT_GOV_ONDEMAND is not set
+# CONFIG_CPU_FREQ_DEFAULT_GOV_CONSERVATIVE is not set
+CONFIG_CPU_FREQ_GOV_PERFORMANCE=y
+CONFIG_CPU_FREQ_GOV_POWERSAVE=y
+CONFIG_CPU_FREQ_GOV_USERSPACE=y
+CONFIG_CPU_FREQ_GOV_ONDEMAND=y
+CONFIG_CPU_FREQ_GOV_CONSERVATIVE=y
+CONFIG_CPU_IDLE=y
+CONFIG_CPU_IDLE_GOV_LADDER=y
+CONFIG_CPU_IDLE_GOV_MENU=y
+
+#
+# Floating point emulation
+#
+
+#
+# At least one emulation must be selected
+#
+# CONFIG_VFP is not set
+
+#
+# Userspace binary formats
+#
+CONFIG_BINFMT_ELF=y
+# CONFIG_CORE_DUMP_DEFAULT_ELF_HEADERS is not set
+CONFIG_HAVE_AOUT=y
+# CONFIG_BINFMT_AOUT is not set
+# CONFIG_BINFMT_MISC is not set
+
+#
+# Power management options
+#
+CONFIG_PM=y
+# CONFIG_PM_DEBUG is not set
+CONFIG_PM_SLEEP=y
+CONFIG_SUSPEND=y
+CONFIG_SUSPEND_FREEZER=y
+# CONFIG_APM_EMULATION is not set
+# CONFIG_PM_RUNTIME is not set
+CONFIG_ARCH_SUSPEND_POSSIBLE=y
+CONFIG_NET=y
+
+#
+# Networking options
+#
+CONFIG_PACKET=y
+# CONFIG_PACKET_MMAP is not set
+CONFIG_UNIX=y
+CONFIG_XFRM=y
+# CONFIG_XFRM_USER is not set
+# CONFIG_XFRM_SUB_POLICY is not set
+# CONFIG_XFRM_MIGRATE is not set
+# CONFIG_XFRM_STATISTICS is not set
+# CONFIG_NET_KEY is not set
+CONFIG_INET=y
+# CONFIG_IP_MULTICAST is not set
+# CONFIG_IP_ADVANCED_ROUTER is not set
+CONFIG_IP_FIB_HASH=y
+CONFIG_IP_PNP=y
+CONFIG_IP_PNP_DHCP=y
+# CONFIG_IP_PNP_BOOTP is not set
+# CONFIG_IP_PNP_RARP is not set
+# CONFIG_NET_IPIP is not set
+# CONFIG_NET_IPGRE is not set
+# CONFIG_ARPD is not set
+# CONFIG_SYN_COOKIES is not set
+# CONFIG_INET_AH is not set
+# CONFIG_INET_ESP is not set
+# CONFIG_INET_IPCOMP is not set
+# CONFIG_INET_XFRM_TUNNEL is not set
+CONFIG_INET_TUNNEL=m
+CONFIG_INET_XFRM_MODE_TRANSPORT=y
+CONFIG_INET_XFRM_MODE_TUNNEL=y
+CONFIG_INET_XFRM_MODE_BEET=y
+# CONFIG_INET_LRO is not set
+CONFIG_INET_DIAG=y
+CONFIG_INET_TCP_DIAG=y
+# CONFIG_TCP_CONG_ADVANCED is not set
+CONFIG_TCP_CONG_CUBIC=y
+CONFIG_DEFAULT_TCP_CONG="cubic"
+# CONFIG_TCP_MD5SIG is not set
+CONFIG_IPV6=m
+# CONFIG_IPV6_PRIVACY is not set
+# CONFIG_IPV6_ROUTER_PREF is not set
+# CONFIG_IPV6_OPTIMISTIC_DAD is not set
+# CONFIG_INET6_AH is not set
+# CONFIG_INET6_ESP is not set
+# CONFIG_INET6_IPCOMP is not set
+# CONFIG_IPV6_MIP6 is not set
+# CONFIG_INET6_XFRM_TUNNEL is not set
+# CONFIG_INET6_TUNNEL is not set
+CONFIG_INET6_XFRM_MODE_TRANSPORT=m
+CONFIG_INET6_XFRM_MODE_TUNNEL=m
+CONFIG_INET6_XFRM_MODE_BEET=m
+# CONFIG_INET6_XFRM_MODE_ROUTEOPTIMIZATION is not set
+CONFIG_IPV6_SIT=m
+# CONFIG_IPV6_SIT_6RD is not set
+CONFIG_IPV6_NDISC_NODETYPE=y
+# CONFIG_IPV6_TUNNEL is not set
+# CONFIG_IPV6_MULTIPLE_TABLES is not set
+# CONFIG_IPV6_MROUTE is not set
+# CONFIG_NETWORK_SECMARK is not set
+CONFIG_NETFILTER=y
+# CONFIG_NETFILTER_DEBUG is not set
+CONFIG_NETFILTER_ADVANCED=y
+
+#
+# Core Netfilter Configuration
+#
+# CONFIG_NETFILTER_NETLINK_QUEUE is not set
+# CONFIG_NETFILTER_NETLINK_LOG is not set
+# CONFIG_NF_CONNTRACK is not set
+# CONFIG_NETFILTER_XTABLES is not set
+# CONFIG_IP_VS is not set
+
+#
+# IP: Netfilter Configuration
+#
+# CONFIG_NF_DEFRAG_IPV4 is not set
+# CONFIG_IP_NF_QUEUE is not set
+# CONFIG_IP_NF_IPTABLES is not set
+# CONFIG_IP_NF_ARPTABLES is not set
+
+#
+# IPv6: Netfilter Configuration
+#
+# CONFIG_IP6_NF_QUEUE is not set
+# CONFIG_IP6_NF_IPTABLES is not set
+# CONFIG_IP_DCCP is not set
+# CONFIG_IP_SCTP is not set
+# CONFIG_RDS is not set
+# CONFIG_TIPC is not set
+# CONFIG_ATM is not set
+# CONFIG_BRIDGE is not set
+# CONFIG_NET_DSA is not set
+# CONFIG_VLAN_8021Q is not set
+# CONFIG_DECNET is not set
+# CONFIG_LLC2 is not set
+# CONFIG_IPX is not set
+# CONFIG_ATALK is not set
+# CONFIG_X25 is not set
+# CONFIG_LAPB is not set
+# CONFIG_ECONET is not set
+# CONFIG_WAN_ROUTER is not set
+# CONFIG_PHONET is not set
+# CONFIG_IEEE802154 is not set
+# CONFIG_NET_SCHED is not set
+# CONFIG_DCB is not set
+
+#
+# Network testing
+#
+# CONFIG_NET_PKTGEN is not set
+# CONFIG_HAMRADIO is not set
+# CONFIG_CAN is not set
+# CONFIG_IRDA is not set
+# CONFIG_BT is not set
+# CONFIG_AF_RXRPC is not set
+CONFIG_WIRELESS=y
+# CONFIG_CFG80211 is not set
+# CONFIG_LIB80211 is not set
+
+#
+# CFG80211 needs to be enabled for MAC80211
+#
+# CONFIG_WIMAX is not set
+# CONFIG_RFKILL is not set
+# CONFIG_NET_9P is not set
+
+#
+# Device Drivers
+#
+
+#
+# Generic Driver Options
+#
+CONFIG_UEVENT_HELPER_PATH="/sbin/hotplug"
+# CONFIG_DEVTMPFS is not set
+CONFIG_STANDALONE=y
+CONFIG_PREVENT_FIRMWARE_BUILD=y
+# CONFIG_FW_LOADER is not set
+# CONFIG_SYS_HYPERVISOR is not set
+# CONFIG_CONNECTOR is not set
+CONFIG_MTD=y
+# CONFIG_MTD_DEBUG is not set
+# CONFIG_MTD_TESTS is not set
+# CONFIG_MTD_CONCAT is not set
+CONFIG_MTD_PARTITIONS=y
+# CONFIG_MTD_REDBOOT_PARTS is not set
+# CONFIG_MTD_CMDLINE_PARTS is not set
+# CONFIG_MTD_AFS_PARTS is not set
+# CONFIG_MTD_AR7_PARTS is not set
+
+#
+# User Modules And Translation Layers
+#
+CONFIG_MTD_CHAR=y
+CONFIG_MTD_BLKDEVS=y
+CONFIG_MTD_BLOCK=y
+# CONFIG_FTL is not set
+# CONFIG_NFTL is not set
+# CONFIG_INFTL is not set
+# CONFIG_RFD_FTL is not set
+# CONFIG_SSFDC is not set
+# CONFIG_MTD_OOPS is not set
+
+#
+# RAM/ROM/Flash chip drivers
+#
+# CONFIG_MTD_CFI is not set
+# CONFIG_MTD_JEDECPROBE is not set
+CONFIG_MTD_MAP_BANK_WIDTH_1=y
+CONFIG_MTD_MAP_BANK_WIDTH_2=y
+CONFIG_MTD_MAP_BANK_WIDTH_4=y
+# CONFIG_MTD_MAP_BANK_WIDTH_8 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_16 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_32 is not set
+CONFIG_MTD_CFI_I1=y
+CONFIG_MTD_CFI_I2=y
+# CONFIG_MTD_CFI_I4 is not set
+# CONFIG_MTD_CFI_I8 is not set
+# CONFIG_MTD_RAM is not set
+# CONFIG_MTD_ROM is not set
+# CONFIG_MTD_ABSENT is not set
+
+#
+# Mapping drivers for chip access
+#
+# CONFIG_MTD_COMPLEX_MAPPINGS is not set
+# CONFIG_MTD_PLATRAM is not set
+
+#
+# Self-contained MTD device drivers
+#
+# CONFIG_MTD_DATAFLASH is not set
+CONFIG_MTD_M25P80=y
+CONFIG_M25PXX_USE_FAST_READ=y
+# CONFIG_MTD_SST25L is not set
+# CONFIG_MTD_SLRAM is not set
+# CONFIG_MTD_PHRAM is not set
+# CONFIG_MTD_MTDRAM is not set
+# CONFIG_MTD_BLOCK2MTD is not set
+
+#
+# Disk-On-Chip Device Drivers
+#
+# CONFIG_MTD_DOC2000 is not set
+# CONFIG_MTD_DOC2001 is not set
+# CONFIG_MTD_DOC2001PLUS is not set
+# CONFIG_MTD_NAND is not set
+# CONFIG_MTD_ONENAND is not set
+
+#
+# LPDDR flash memory drivers
+#
+# CONFIG_MTD_LPDDR is not set
+
+#
+# UBI - Unsorted block images
+#
+# CONFIG_MTD_UBI is not set
+# CONFIG_PARPORT is not set
+CONFIG_BLK_DEV=y
+# CONFIG_BLK_DEV_COW_COMMON is not set
+CONFIG_BLK_DEV_LOOP=m
+# CONFIG_BLK_DEV_CRYPTOLOOP is not set
+
+#
+# DRBD disabled because PROC_FS, INET or CONNECTOR not selected
+#
+# CONFIG_BLK_DEV_NBD is not set
+# CONFIG_BLK_DEV_UB is not set
+CONFIG_BLK_DEV_RAM=y
+CONFIG_BLK_DEV_RAM_COUNT=1
+CONFIG_BLK_DEV_RAM_SIZE=32768
+# CONFIG_BLK_DEV_XIP is not set
+# CONFIG_CDROM_PKTCDVD is not set
+# CONFIG_ATA_OVER_ETH is not set
+# CONFIG_MG_DISK is not set
+CONFIG_MISC_DEVICES=y
+# CONFIG_AD525X_DPOT is not set
+# CONFIG_ICS932S401 is not set
+# CONFIG_ENCLOSURE_SERVICES is not set
+# CONFIG_ISL29003 is not set
+# CONFIG_DS1682 is not set
+# CONFIG_TI_DAC7512 is not set
+# CONFIG_C2PORT is not set
+
+#
+# EEPROM support
+#
+CONFIG_EEPROM_AT24=y
+# CONFIG_EEPROM_AT25 is not set
+# CONFIG_EEPROM_LEGACY is not set
+# CONFIG_EEPROM_MAX6875 is not set
+# CONFIG_EEPROM_93CX6 is not set
+# CONFIG_IWMC3200TOP is not set
+CONFIG_HAVE_IDE=y
+# CONFIG_IDE is not set
+
+#
+# SCSI device support
+#
+# CONFIG_RAID_ATTRS is not set
+CONFIG_SCSI=y
+CONFIG_SCSI_DMA=y
+# CONFIG_SCSI_TGT is not set
+# CONFIG_SCSI_NETLINK is not set
+CONFIG_SCSI_PROC_FS=y
+
+#
+# SCSI support type (disk, tape, CD-ROM)
+#
+CONFIG_BLK_DEV_SD=y
+# CONFIG_CHR_DEV_ST is not set
+# CONFIG_CHR_DEV_OSST is not set
+# CONFIG_BLK_DEV_SR is not set
+CONFIG_CHR_DEV_SG=y
+# CONFIG_CHR_DEV_SCH is not set
+# CONFIG_SCSI_MULTI_LUN is not set
+# CONFIG_SCSI_CONSTANTS is not set
+# CONFIG_SCSI_LOGGING is not set
+# CONFIG_SCSI_SCAN_ASYNC is not set
+CONFIG_SCSI_WAIT_SCAN=m
+
+#
+# SCSI Transports
+#
+# CONFIG_SCSI_SPI_ATTRS is not set
+# CONFIG_SCSI_FC_ATTRS is not set
+# CONFIG_SCSI_ISCSI_ATTRS is not set
+# CONFIG_SCSI_SAS_LIBSAS is not set
+# CONFIG_SCSI_SRP_ATTRS is not set
+CONFIG_SCSI_LOWLEVEL=y
+# CONFIG_ISCSI_TCP is not set
+# CONFIG_LIBFC is not set
+# CONFIG_LIBFCOE is not set
+# CONFIG_SCSI_DEBUG is not set
+# CONFIG_SCSI_DH is not set
+# CONFIG_SCSI_OSD_INITIATOR is not set
+CONFIG_ATA=y
+# CONFIG_ATA_NONSTANDARD is not set
+CONFIG_ATA_VERBOSE_ERROR=y
+CONFIG_SATA_PMP=y
+CONFIG_SATA_AHCI=y
+# CONFIG_ATA_SFF is not set
+# CONFIG_MD is not set
+CONFIG_NETDEVICES=y
+# CONFIG_DUMMY is not set
+# CONFIG_BONDING is not set
+# CONFIG_MACVLAN is not set
+# CONFIG_EQUALIZER is not set
+# CONFIG_TUN is not set
+# CONFIG_VETH is not set
+CONFIG_PHYLIB=y
+
+#
+# MII PHY device drivers
+#
+# CONFIG_MARVELL_PHY is not set
+# CONFIG_DAVICOM_PHY is not set
+# CONFIG_QSEMI_PHY is not set
+CONFIG_LXT_PHY=y
+# CONFIG_CICADA_PHY is not set
+# CONFIG_VITESSE_PHY is not set
+CONFIG_SMSC_PHY=y
+# CONFIG_BROADCOM_PHY is not set
+# CONFIG_ICPLUS_PHY is not set
+# CONFIG_REALTEK_PHY is not set
+# CONFIG_NATIONAL_PHY is not set
+# CONFIG_STE10XP is not set
+CONFIG_LSI_ET1011C_PHY=y
+# CONFIG_FIXED_PHY is not set
+# CONFIG_MDIO_BITBANG is not set
+CONFIG_NET_ETHERNET=y
+CONFIG_MII=y
+# CONFIG_AX88796 is not set
+# CONFIG_SMC91X is not set
+CONFIG_TI_DAVINCI_EMAC=y
+# CONFIG_DM9000 is not set
+# CONFIG_ENC28J60 is not set
+# CONFIG_ETHOC is not set
+# CONFIG_SMC911X is not set
+# CONFIG_SMSC911X is not set
+# CONFIG_DNET is not set
+# CONFIG_IBM_NEW_EMAC_ZMII is not set
+# CONFIG_IBM_NEW_EMAC_RGMII is not set
+# CONFIG_IBM_NEW_EMAC_TAH is not set
+# CONFIG_IBM_NEW_EMAC_EMAC4 is not set
+# CONFIG_IBM_NEW_EMAC_NO_FLOW_CTRL is not set
+# CONFIG_IBM_NEW_EMAC_MAL_CLR_ICINTSTAT is not set
+# CONFIG_IBM_NEW_EMAC_MAL_COMMON_ERR is not set
+# CONFIG_B44 is not set
+# CONFIG_KS8842 is not set
+# CONFIG_KS8851 is not set
+# CONFIG_KS8851_MLL is not set
+# CONFIG_NETDEV_1000 is not set
+# CONFIG_NETDEV_10000 is not set
+CONFIG_WLAN=y
+# CONFIG_USB_ZD1201 is not set
+# CONFIG_HOSTAP is not set
+
+#
+# Enable WiMAX (Networking options) to see the WiMAX drivers
+#
+
+#
+# USB Network Adapters
+#
+# CONFIG_USB_CATC is not set
+# CONFIG_USB_KAWETH is not set
+# CONFIG_USB_PEGASUS is not set
+# CONFIG_USB_RTL8150 is not set
+# CONFIG_USB_USBNET is not set
+# CONFIG_WAN is not set
+# CONFIG_PPP is not set
+# CONFIG_SLIP is not set
+CONFIG_NETCONSOLE=y
+# CONFIG_NETCONSOLE_DYNAMIC is not set
+CONFIG_NETPOLL=y
+CONFIG_NETPOLL_TRAP=y
+CONFIG_NET_POLL_CONTROLLER=y
+# CONFIG_ISDN is not set
+# CONFIG_PHONE is not set
+
+#
+# Input device support
+#
+CONFIG_INPUT=y
+# CONFIG_INPUT_FF_MEMLESS is not set
+# CONFIG_INPUT_POLLDEV is not set
+# CONFIG_INPUT_SPARSEKMAP is not set
+
+#
+# Userland interfaces
+#
+# CONFIG_INPUT_MOUSEDEV is not set
+# CONFIG_INPUT_JOYDEV is not set
+CONFIG_INPUT_EVDEV=y
+# CONFIG_INPUT_EVBUG is not set
+
+#
+# Input Device Drivers
+#
+CONFIG_INPUT_KEYBOARD=y
+# CONFIG_KEYBOARD_ADP5588 is not set
+CONFIG_KEYBOARD_ATKBD=m
+# CONFIG_QT2160 is not set
+# CONFIG_KEYBOARD_LKKBD is not set
+CONFIG_KEYBOARD_GPIO=y
+# CONFIG_KEYBOARD_MATRIX is not set
+# CONFIG_KEYBOARD_MAX7359 is not set
+# CONFIG_KEYBOARD_NEWTON is not set
+# CONFIG_KEYBOARD_OPENCORES is not set
+# CONFIG_KEYBOARD_STOWAWAY is not set
+# CONFIG_KEYBOARD_SUNKBD is not set
+CONFIG_KEYBOARD_XTKBD=m
+# CONFIG_INPUT_MOUSE is not set
+# CONFIG_INPUT_JOYSTICK is not set
+# CONFIG_INPUT_TABLET is not set
+CONFIG_INPUT_TOUCHSCREEN=y
+# CONFIG_TOUCHSCREEN_ADS7846 is not set
+# CONFIG_TOUCHSCREEN_AD7877 is not set
+# CONFIG_TOUCHSCREEN_AD7879_I2C is not set
+# CONFIG_TOUCHSCREEN_AD7879_SPI is not set
+# CONFIG_TOUCHSCREEN_AD7879 is not set
+# CONFIG_TOUCHSCREEN_DYNAPRO is not set
+# CONFIG_TOUCHSCREEN_EETI is not set
+# CONFIG_TOUCHSCREEN_FUJITSU is not set
+# CONFIG_TOUCHSCREEN_GUNZE is not set
+# CONFIG_TOUCHSCREEN_ELO is not set
+# CONFIG_TOUCHSCREEN_WACOM_W8001 is not set
+# CONFIG_TOUCHSCREEN_MCS5000 is not set
+# CONFIG_TOUCHSCREEN_MTOUCH is not set
+# CONFIG_TOUCHSCREEN_INEXIO is not set
+# CONFIG_TOUCHSCREEN_MK712 is not set
+# CONFIG_TOUCHSCREEN_PENMOUNT is not set
+# CONFIG_TOUCHSCREEN_TOUCHRIGHT is not set
+# CONFIG_TOUCHSCREEN_TOUCHWIN is not set
+# CONFIG_TOUCHSCREEN_USB_COMPOSITE is not set
+# CONFIG_TOUCHSCREEN_TOUCHIT213 is not set
+# CONFIG_TOUCHSCREEN_TSC2007 is not set
+# CONFIG_TOUCHSCREEN_TSC2004 is not set
+# CONFIG_TOUCHSCREEN_W90X900 is not set
+CONFIG_TOUCHSCREEN_TPS6507X=y
+# CONFIG_INPUT_MISC is not set
+
+#
+# Hardware I/O ports
+#
+CONFIG_SERIO=y
+CONFIG_SERIO_SERPORT=y
+CONFIG_SERIO_LIBPS2=y
+# CONFIG_SERIO_RAW is not set
+# CONFIG_SERIO_ALTERA_PS2 is not set
+# CONFIG_GAMEPORT is not set
+
+#
+# Character devices
+#
+CONFIG_VT=y
+CONFIG_CONSOLE_TRANSLATIONS=y
+# CONFIG_VT_CONSOLE is not set
+CONFIG_HW_CONSOLE=y
+# CONFIG_VT_HW_CONSOLE_BINDING is not set
+CONFIG_DEVKMEM=y
+# CONFIG_SERIAL_NONSTANDARD is not set
+
+#
+# Serial drivers
+#
+CONFIG_SERIAL_8250=y
+CONFIG_SERIAL_8250_CONSOLE=y
+CONFIG_SERIAL_8250_NR_UARTS=3
+CONFIG_SERIAL_8250_RUNTIME_UARTS=3
+# CONFIG_SERIAL_8250_EXTENDED is not set
+
+#
+# Non-8250 serial port support
+#
+# CONFIG_SERIAL_MAX3100 is not set
+CONFIG_SERIAL_CORE=y
+CONFIG_SERIAL_CORE_CONSOLE=y
+CONFIG_UNIX98_PTYS=y
+# CONFIG_DEVPTS_MULTIPLE_INSTANCES is not set
+CONFIG_LEGACY_PTYS=y
+CONFIG_LEGACY_PTY_COUNT=8
+# CONFIG_IPMI_HANDLER is not set
+CONFIG_HW_RANDOM=m
+# CONFIG_HW_RANDOM_TIMERIOMEM is not set
+# CONFIG_R3964 is not set
+# CONFIG_RAW_DRIVER is not set
+# CONFIG_TCG_TPM is not set
+CONFIG_I2C=y
+CONFIG_I2C_BOARDINFO=y
+CONFIG_I2C_COMPAT=y
+CONFIG_I2C_CHARDEV=y
+CONFIG_I2C_HELPER_AUTO=y
+CONFIG_I2C_ALGOBIT=y
+
+#
+# I2C Hardware Bus support
+#
+
+#
+# I2C system bus drivers (mostly embedded / system-on-chip)
+#
+CONFIG_I2C_DAVINCI=y
+# CONFIG_I2C_DESIGNWARE is not set
+CONFIG_I2C_GPIO=y
+# CONFIG_I2C_OCORES is not set
+# CONFIG_I2C_SIMTEC is not set
+
+#
+# External I2C/SMBus adapter drivers
+#
+# CONFIG_I2C_PARPORT_LIGHT is not set
+# CONFIG_I2C_TAOS_EVM is not set
+# CONFIG_I2C_TINY_USB is not set
+
+#
+# Other I2C/SMBus bus drivers
+#
+# CONFIG_I2C_PCA_PLATFORM is not set
+# CONFIG_I2C_STUB is not set
+
+#
+# Miscellaneous I2C Chip support
+#
+# CONFIG_SENSORS_TSL2550 is not set
+# CONFIG_I2C_DEBUG_CORE is not set
+# CONFIG_I2C_DEBUG_ALGO is not set
+# CONFIG_I2C_DEBUG_BUS is not set
+# CONFIG_I2C_DEBUG_CHIP is not set
+CONFIG_SPI=y
+CONFIG_SPI_MASTER=y
+
+#
+# SPI Master Controller Drivers
+#
+CONFIG_SPI_DAVINCI=y
+CONFIG_SPI_BITBANG=y
+# CONFIG_SPI_GPIO is not set
+# CONFIG_SPI_XILINX is not set
+# CONFIG_SPI_DESIGNWARE is not set
+
+#
+# SPI Protocol Masters
+#
+# CONFIG_SPI_SPIDEV is not set
+# CONFIG_SPI_TLE62X0 is not set
+
+#
+# PPS support
+#
+# CONFIG_PPS is not set
+CONFIG_ARCH_REQUIRE_GPIOLIB=y
+CONFIG_GPIOLIB=y
+# CONFIG_GPIO_SYSFS is not set
+
+#
+# Memory mapped GPIO expanders:
+#
+
+#
+# I2C GPIO expanders:
+#
+# CONFIG_GPIO_MAX732X is not set
+CONFIG_GPIO_PCA953X=y
+CONFIG_GPIO_PCF857X=y
+# CONFIG_GPIO_ADP5588 is not set
+
+#
+# PCI GPIO expanders:
+#
+
+#
+# SPI GPIO expanders:
+#
+# CONFIG_GPIO_MAX7301 is not set
+# CONFIG_GPIO_MCP23S08 is not set
+# CONFIG_GPIO_MC33880 is not set
+
+#
+# AC97 GPIO expanders:
+#
+# CONFIG_W1 is not set
+# CONFIG_POWER_SUPPLY is not set
+# CONFIG_HWMON is not set
+# CONFIG_THERMAL is not set
+CONFIG_WATCHDOG=y
+# CONFIG_WATCHDOG_NOWAYOUT is not set
+
+#
+# Watchdog Device Drivers
+#
+# CONFIG_SOFT_WATCHDOG is not set
+CONFIG_DAVINCI_WATCHDOG=y
+
+#
+# USB-based Watchdog Cards
+#
+# CONFIG_USBPCWATCHDOG is not set
+CONFIG_SSB_POSSIBLE=y
+
+#
+# Sonics Silicon Backplane
+#
+# CONFIG_SSB is not set
+
+#
+# Multifunction device drivers
+#
+# CONFIG_MFD_CORE is not set
+# CONFIG_MFD_SM501 is not set
+# CONFIG_MFD_ASIC3 is not set
+# CONFIG_HTC_EGPIO is not set
+# CONFIG_HTC_PASIC3 is not set
+# CONFIG_TPS65010 is not set
+CONFIG_TPS6507x=y
+# CONFIG_TWL4030_CORE is not set
+# CONFIG_MFD_TMIO is not set
+# CONFIG_MFD_T7L66XB is not set
+# CONFIG_MFD_TC6387XB is not set
+# CONFIG_MFD_TC6393XB is not set
+# CONFIG_PMIC_DA903X is not set
+# CONFIG_PMIC_ADP5520 is not set
+# CONFIG_MFD_WM8400 is not set
+# CONFIG_MFD_WM831X is not set
+# CONFIG_MFD_WM8350_I2C is not set
+# CONFIG_MFD_PCF50633 is not set
+# CONFIG_MFD_MC13783 is not set
+# CONFIG_AB3100_CORE is not set
+# CONFIG_EZX_PCAP is not set
+# CONFIG_MFD_88PM8607 is not set
+# CONFIG_AB4500_CORE is not set
+# CONFIG_REGULATOR is not set
+CONFIG_MEDIA_SUPPORT=y
+
+#
+# Multimedia core support
+#
+CONFIG_VIDEO_DEV=y
+CONFIG_VIDEO_V4L2_COMMON=y
+CONFIG_VIDEO_ALLOW_V4L1=y
+CONFIG_VIDEO_V4L1_COMPAT=y
+# CONFIG_DVB_CORE is not set
+CONFIG_VIDEO_MEDIA=y
+
+#
+# Multimedia drivers
+#
+CONFIG_IR_CORE=y
+CONFIG_VIDEO_IR=y
+# CONFIG_MEDIA_ATTACH is not set
+CONFIG_MEDIA_TUNER=y
+# CONFIG_MEDIA_TUNER_CUSTOMISE is not set
+CONFIG_MEDIA_TUNER_SIMPLE=y
+CONFIG_MEDIA_TUNER_TDA8290=y
+CONFIG_MEDIA_TUNER_TDA9887=y
+CONFIG_MEDIA_TUNER_TEA5761=y
+CONFIG_MEDIA_TUNER_TEA5767=y
+CONFIG_MEDIA_TUNER_MT20XX=y
+CONFIG_MEDIA_TUNER_XC2028=y
+CONFIG_MEDIA_TUNER_XC5000=y
+CONFIG_MEDIA_TUNER_MC44S803=y
+CONFIG_VIDEO_V4L2=y
+CONFIG_VIDEO_V4L1=y
+CONFIG_VIDEOBUF_GEN=y
+CONFIG_VIDEOBUF_DMA_CONTIG=y
+CONFIG_VIDEO_CAPTURE_DRIVERS=y
+# CONFIG_VIDEO_ADV_DEBUG is not set
+# CONFIG_VIDEO_FIXED_MINOR_RANGES is not set
+# CONFIG_VIDEO_HELPER_CHIPS_AUTO is not set
+# CONFIG_VIDEO_IR_I2C is not set
+
+#
+# Encoders/decoders and other helper chips
+#
+
+#
+# Audio decoders
+#
+# CONFIG_VIDEO_TVAUDIO is not set
+# CONFIG_VIDEO_TDA7432 is not set
+# CONFIG_VIDEO_TDA9840 is not set
+# CONFIG_VIDEO_TDA9875 is not set
+# CONFIG_VIDEO_TEA6415C is not set
+# CONFIG_VIDEO_TEA6420 is not set
+# CONFIG_VIDEO_MSP3400 is not set
+# CONFIG_VIDEO_CS5345 is not set
+# CONFIG_VIDEO_CS53L32A is not set
+# CONFIG_VIDEO_M52790 is not set
+# CONFIG_VIDEO_TLV320AIC23B is not set
+# CONFIG_VIDEO_WM8775 is not set
+# CONFIG_VIDEO_WM8739 is not set
+# CONFIG_VIDEO_VP27SMPX is not set
+
+#
+# RDS decoders
+#
+# CONFIG_VIDEO_SAA6588 is not set
+
+#
+# Video decoders
+#
+# CONFIG_VIDEO_ADV7180 is not set
+# CONFIG_VIDEO_BT819 is not set
+# CONFIG_VIDEO_BT856 is not set
+# CONFIG_VIDEO_BT866 is not set
+# CONFIG_VIDEO_KS0127 is not set
+# CONFIG_VIDEO_OV7670 is not set
+# CONFIG_VIDEO_MT9V011 is not set
+# CONFIG_VIDEO_TCM825X is not set
+# CONFIG_VIDEO_SAA7110 is not set
+# CONFIG_VIDEO_SAA711X is not set
+# CONFIG_VIDEO_SAA717X is not set
+# CONFIG_VIDEO_SAA7191 is not set
+CONFIG_VIDEO_TVP514X=y
+# CONFIG_VIDEO_TVP5150 is not set
+# CONFIG_VIDEO_VPX3220 is not set
+
+#
+# Video and audio decoders
+#
+# CONFIG_VIDEO_CX25840 is not set
+
+#
+# MPEG video encoders
+#
+# CONFIG_VIDEO_CX2341X is not set
+
+#
+# Video encoders
+#
+# CONFIG_VIDEO_SAA7127 is not set
+# CONFIG_VIDEO_SAA7185 is not set
+# CONFIG_VIDEO_ADV7170 is not set
+# CONFIG_VIDEO_ADV7175 is not set
+# CONFIG_VIDEO_THS7303 is not set
+# CONFIG_VIDEO_ADV7343 is not set
+
+#
+# Video improvement chips
+#
+# CONFIG_VIDEO_UPD64031A is not set
+# CONFIG_VIDEO_UPD64083 is not set
+CONFIG_VIDEO_DAVINCI_VPIF_CAPTURE=y
+CONFIG_VIDEO_DAVINCI_VPIF=y
+# CONFIG_VIDEO_VIVI is not set
+# CONFIG_VIDEO_VPSS_SYSTEM is not set
+# CONFIG_VIDEO_VPFE_CAPTURE is not set
+# CONFIG_VIDEO_CPIA is not set
+# CONFIG_VIDEO_CPIA2 is not set
+# CONFIG_VIDEO_SAA5246A is not set
+# CONFIG_VIDEO_SAA5249 is not set
+# CONFIG_SOC_CAMERA is not set
+CONFIG_V4L_USB_DRIVERS=y
+CONFIG_USB_VIDEO_CLASS=y
+# CONFIG_USB_VIDEO_CLASS_INPUT_EVDEV is not set
+# CONFIG_USB_GSPCA is not set
+# CONFIG_VIDEO_PVRUSB2 is not set
+# CONFIG_VIDEO_HDPVR is not set
+# CONFIG_VIDEO_EM28XX is not set
+# CONFIG_VIDEO_CX231XX is not set
+# CONFIG_VIDEO_USBVISION is not set
+# CONFIG_USB_VICAM is not set
+# CONFIG_USB_IBMCAM is not set
+# CONFIG_USB_KONICAWC is not set
+# CONFIG_USB_QUICKCAM_MESSENGER is not set
+# CONFIG_USB_ET61X251 is not set
+# CONFIG_VIDEO_OVCAMCHIP is not set
+# CONFIG_USB_OV511 is not set
+# CONFIG_USB_SE401 is not set
+# CONFIG_USB_SN9C102 is not set
+# CONFIG_USB_STV680 is not set
+# CONFIG_USB_ZC0301 is not set
+# CONFIG_USB_PWC is not set
+# CONFIG_USB_PWC_INPUT_EVDEV is not set
+# CONFIG_USB_ZR364XX is not set
+# CONFIG_USB_STKWEBCAM is not set
+# CONFIG_USB_S2255 is not set
+# CONFIG_RADIO_ADAPTERS is not set
+# CONFIG_DAB is not set
+
+#
+# Graphics support
+#
+# CONFIG_VGASTATE is not set
+# CONFIG_VIDEO_OUTPUT_CONTROL is not set
+CONFIG_FB=y
+# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_FB_DDC is not set
+# CONFIG_FB_BOOT_VESA_SUPPORT is not set
+CONFIG_FB_CFB_FILLRECT=y
+CONFIG_FB_CFB_COPYAREA=y
+CONFIG_FB_CFB_IMAGEBLIT=y
+# CONFIG_FB_CFB_REV_PIXELS_IN_BYTE is not set
+# CONFIG_FB_SYS_FILLRECT is not set
+# CONFIG_FB_SYS_COPYAREA is not set
+# CONFIG_FB_SYS_IMAGEBLIT is not set
+# CONFIG_FB_FOREIGN_ENDIAN is not set
+# CONFIG_FB_SYS_FOPS is not set
+# CONFIG_FB_SVGALIB is not set
+# CONFIG_FB_MACMODES is not set
+# CONFIG_FB_BACKLIGHT is not set
+# CONFIG_FB_MODE_HELPERS is not set
+# CONFIG_FB_TILEBLITTING is not set
+
+#
+# Frame buffer hardware drivers
+#
+# CONFIG_FB_S1D13XXX is not set
+# CONFIG_FB_DAVINCI is not set
+# CONFIG_FB_VIRTUAL is not set
+CONFIG_FB_DA8XX=y
+# CONFIG_FB_METRONOME is not set
+# CONFIG_FB_MB862XX is not set
+# CONFIG_FB_BROADSHEET is not set
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
+
+#
+# Display device support
+#
+# CONFIG_DISPLAY_SUPPORT is not set
+
+#
+# Console display driver support
+#
+# CONFIG_VGA_CONSOLE is not set
+CONFIG_DUMMY_CONSOLE=y
+CONFIG_FRAMEBUFFER_CONSOLE=y
+# CONFIG_FRAMEBUFFER_CONSOLE_DETECT_PRIMARY is not set
+# CONFIG_FRAMEBUFFER_CONSOLE_ROTATION is not set
+# CONFIG_FONTS is not set
+CONFIG_FONT_8x8=y
+CONFIG_FONT_8x16=y
+CONFIG_LOGO=y
+CONFIG_LOGO_LINUX_MONO=y
+CONFIG_LOGO_LINUX_VGA16=y
+CONFIG_LOGO_LINUX_CLUT224=y
+CONFIG_SOUND=y
+# CONFIG_SOUND_OSS_CORE is not set
+CONFIG_SND=y
+CONFIG_SND_TIMER=y
+CONFIG_SND_PCM=y
+CONFIG_SND_HWDEP=y
+CONFIG_SND_RAWMIDI=y
+CONFIG_SND_JACK=y
+# CONFIG_SND_SEQUENCER is not set
+# CONFIG_SND_MIXER_OSS is not set
+# CONFIG_SND_PCM_OSS is not set
+# CONFIG_SND_HRTIMER is not set
+# CONFIG_SND_DYNAMIC_MINORS is not set
+CONFIG_SND_SUPPORT_OLD_API=y
+CONFIG_SND_VERBOSE_PROCFS=y
+# CONFIG_SND_VERBOSE_PRINTK is not set
+# CONFIG_SND_DEBUG is not set
+# CONFIG_SND_RAWMIDI_SEQ is not set
+# CONFIG_SND_OPL3_LIB_SEQ is not set
+# CONFIG_SND_OPL4_LIB_SEQ is not set
+# CONFIG_SND_SBAWE_SEQ is not set
+# CONFIG_SND_EMU10K1_SEQ is not set
+CONFIG_SND_DRIVERS=y
+# CONFIG_SND_DUMMY is not set
+# CONFIG_SND_MTPAV is not set
+# CONFIG_SND_SERIAL_U16550 is not set
+# CONFIG_SND_MPU401 is not set
+CONFIG_SND_ARM=y
+CONFIG_SND_SPI=y
+CONFIG_SND_USB=y
+CONFIG_SND_USB_AUDIO=y
+# CONFIG_SND_USB_CAIAQ is not set
+CONFIG_SND_SOC=y
+CONFIG_SND_DAVINCI_SOC=y
+CONFIG_SND_DAVINCI_SOC_MCASP=y
+CONFIG_SND_DA850_SOC_EVM=y
+CONFIG_SND_SOC_I2C_AND_SPI=y
+# CONFIG_SND_SOC_ALL_CODECS is not set
+CONFIG_SND_SOC_TLV320AIC3X=y
+# CONFIG_SOUND_PRIME is not set
+CONFIG_HID_SUPPORT=y
+CONFIG_HID=y
+# CONFIG_HIDRAW is not set
+
+#
+# USB Input Devices
+#
+CONFIG_USB_HID=y
+# CONFIG_HID_PID is not set
+# CONFIG_USB_HIDDEV is not set
+
+#
+# Special HID drivers
+#
+# CONFIG_HID_A4TECH is not set
+# CONFIG_HID_APPLE is not set
+# CONFIG_HID_BELKIN is not set
+# CONFIG_HID_CHERRY is not set
+# CONFIG_HID_CHICONY is not set
+# CONFIG_HID_CYPRESS is not set
+# CONFIG_HID_DRAGONRISE is not set
+# CONFIG_HID_EZKEY is not set
+# CONFIG_HID_KYE is not set
+# CONFIG_HID_GYRATION is not set
+# CONFIG_HID_TWINHAN is not set
+# CONFIG_HID_KENSINGTON is not set
+# CONFIG_HID_LOGITECH is not set
+# CONFIG_HID_MICROSOFT is not set
+# CONFIG_HID_MONTEREY is not set
+# CONFIG_HID_NTRIG is not set
+# CONFIG_HID_PANTHERLORD is not set
+# CONFIG_HID_PETALYNX is not set
+# CONFIG_HID_SAMSUNG is not set
+# CONFIG_HID_SONY is not set
+# CONFIG_HID_SUNPLUS is not set
+# CONFIG_HID_GREENASIA is not set
+# CONFIG_HID_SMARTJOYPLUS is not set
+# CONFIG_HID_TOPSEED is not set
+# CONFIG_HID_THRUSTMASTER is not set
+# CONFIG_HID_ZEROPLUS is not set
+CONFIG_USB_SUPPORT=y
+CONFIG_USB_ARCH_HAS_HCD=y
+CONFIG_USB_ARCH_HAS_OHCI=y
+# CONFIG_USB_ARCH_HAS_EHCI is not set
+CONFIG_USB=y
+# CONFIG_USB_DEBUG is not set
+# CONFIG_USB_ANNOUNCE_NEW_DEVICES is not set
+
+#
+# Miscellaneous USB options
+#
+# CONFIG_USB_DEVICEFS is not set
+# CONFIG_USB_DEVICE_CLASS is not set
+# CONFIG_USB_DYNAMIC_MINORS is not set
+CONFIG_USB_SUSPEND=y
+# CONFIG_USB_OTG is not set
+# CONFIG_USB_OTG_WHITELIST is not set
+# CONFIG_USB_OTG_BLACKLIST_HUB is not set
+# CONFIG_USB_MON is not set
+# CONFIG_USB_WUSB is not set
+# CONFIG_USB_WUSB_CBAF is not set
+
+#
+# USB Host Controller Drivers
+#
+# CONFIG_USB_C67X00_HCD is not set
+# CONFIG_USB_OXU210HP_HCD is not set
+# CONFIG_USB_ISP116X_HCD is not set
+# CONFIG_USB_ISP1760_HCD is not set
+# CONFIG_USB_ISP1362_HCD is not set
+CONFIG_USB_OHCI_HCD=y
+# CONFIG_USB_OHCI_BIG_ENDIAN_DESC is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_MMIO is not set
+CONFIG_USB_OHCI_LITTLE_ENDIAN=y
+# CONFIG_USB_SL811_HCD is not set
+# CONFIG_USB_R8A66597_HCD is not set
+# CONFIG_USB_HWA_HCD is not set
+CONFIG_USB_MUSB_HDRC=y
+CONFIG_USB_MUSB_SOC=y
+CONFIG_USB_MUSB_HOST=y
+# CONFIG_USB_MUSB_PERIPHERAL is not set
+# CONFIG_USB_MUSB_OTG is not set
+CONFIG_USB_MUSB_HDRC_HCD=y
+# CONFIG_MUSB_PIO_ONLY is not set
+# CONFIG_USB_INVENTRA_DMA is not set
+# CONFIG_USB_TI_CPPI_DMA is not set
+CONFIG_USB_TI_CPPI41_DMA=y
+CONFIG_USB_MUSB_DEBUG=y
+
+#
+# USB Device Class drivers
+#
+# CONFIG_USB_ACM is not set
+# CONFIG_USB_PRINTER is not set
+# CONFIG_USB_WDM is not set
+# CONFIG_USB_TMC is not set
+
+#
+# NOTE: USB_STORAGE depends on SCSI but BLK_DEV_SD may
+#
+
+#
+# also be needed; see USB_STORAGE Help for more info
+#
+CONFIG_USB_STORAGE=y
+# CONFIG_USB_STORAGE_DEBUG is not set
+# CONFIG_USB_STORAGE_DATAFAB is not set
+# CONFIG_USB_STORAGE_FREECOM is not set
+# CONFIG_USB_STORAGE_ISD200 is not set
+# CONFIG_USB_STORAGE_USBAT is not set
+# CONFIG_USB_STORAGE_SDDR09 is not set
+# CONFIG_USB_STORAGE_SDDR55 is not set
+# CONFIG_USB_STORAGE_JUMPSHOT is not set
+# CONFIG_USB_STORAGE_ALAUDA is not set
+# CONFIG_USB_STORAGE_ONETOUCH is not set
+# CONFIG_USB_STORAGE_KARMA is not set
+# CONFIG_USB_STORAGE_CYPRESS_ATACB is not set
+# CONFIG_USB_LIBUSUAL is not set
+
+#
+# USB Imaging devices
+#
+# CONFIG_USB_MDC800 is not set
+# CONFIG_USB_MICROTEK is not set
+
+#
+# USB port drivers
+#
+# CONFIG_USB_SERIAL is not set
+
+#
+# USB Miscellaneous drivers
+#
+# CONFIG_USB_EMI62 is not set
+# CONFIG_USB_EMI26 is not set
+# CONFIG_USB_ADUTUX is not set
+# CONFIG_USB_SEVSEG is not set
+# CONFIG_USB_RIO500 is not set
+# CONFIG_USB_LEGOTOWER is not set
+# CONFIG_USB_LCD is not set
+# CONFIG_USB_BERRY_CHARGE is not set
+# CONFIG_USB_LED is not set
+# CONFIG_USB_CYPRESS_CY7C63 is not set
+# CONFIG_USB_CYTHERM is not set
+# CONFIG_USB_IDMOUSE is not set
+# CONFIG_USB_FTDI_ELAN is not set
+# CONFIG_USB_APPLEDISPLAY is not set
+# CONFIG_USB_SISUSBVGA is not set
+# CONFIG_USB_LD is not set
+# CONFIG_USB_TRANCEVIBRATOR is not set
+# CONFIG_USB_IOWARRIOR is not set
+# CONFIG_USB_TEST is not set
+# CONFIG_USB_ISIGHTFW is not set
+# CONFIG_USB_VST is not set
+# CONFIG_USB_GADGET is not set
+
+#
+# OTG and related infrastructure
+#
+CONFIG_USB_OTG_UTILS=y
+# CONFIG_USB_GPIO_VBUS is not set
+# CONFIG_USB_ULPI is not set
+CONFIG_NOP_USB_XCEIV=y
+CONFIG_MMC=y
+# CONFIG_MMC_DEBUG is not set
+# CONFIG_MMC_UNSAFE_RESUME is not set
+
+#
+# MMC/SD/SDIO Card Drivers
+#
+CONFIG_MMC_BLOCK=y
+CONFIG_MMC_BLOCK_BOUNCE=y
+# CONFIG_SDIO_UART is not set
+# CONFIG_MMC_TEST is not set
+
+#
+# MMC/SD/SDIO Host Controller Drivers
+#
+# CONFIG_MMC_SDHCI is not set
+# CONFIG_MMC_AT91 is not set
+# CONFIG_MMC_ATMELMCI is not set
+CONFIG_MMC_DAVINCI=y
+# CONFIG_MMC_SPI is not set
+# CONFIG_MEMSTICK is not set
+# CONFIG_NEW_LEDS is not set
+# CONFIG_ACCESSIBILITY is not set
+CONFIG_RTC_LIB=y
+CONFIG_RTC_CLASS=y
+CONFIG_RTC_HCTOSYS=y
+CONFIG_RTC_HCTOSYS_DEVICE="rtc0"
+# CONFIG_RTC_DEBUG is not set
+
+#
+# RTC interfaces
+#
+CONFIG_RTC_INTF_SYSFS=y
+CONFIG_RTC_INTF_PROC=y
+CONFIG_RTC_INTF_DEV=y
+# CONFIG_RTC_INTF_DEV_UIE_EMUL is not set
+# CONFIG_RTC_DRV_TEST is not set
+
+#
+# I2C RTC drivers
+#
+# CONFIG_RTC_DRV_DS1307 is not set
+# CONFIG_RTC_DRV_DS1374 is not set
+# CONFIG_RTC_DRV_DS1672 is not set
+# CONFIG_RTC_DRV_MAX6900 is not set
+# CONFIG_RTC_DRV_RS5C372 is not set
+# CONFIG_RTC_DRV_ISL1208 is not set
+# CONFIG_RTC_DRV_X1205 is not set
+# CONFIG_RTC_DRV_PCF8563 is not set
+# CONFIG_RTC_DRV_PCF8583 is not set
+# CONFIG_RTC_DRV_M41T80 is not set
+# CONFIG_RTC_DRV_BQ32K is not set
+# CONFIG_RTC_DRV_S35390A is not set
+# CONFIG_RTC_DRV_FM3130 is not set
+# CONFIG_RTC_DRV_RX8581 is not set
+# CONFIG_RTC_DRV_RX8025 is not set
+
+#
+# SPI RTC drivers
+#
+# CONFIG_RTC_DRV_M41T94 is not set
+# CONFIG_RTC_DRV_DS1305 is not set
+# CONFIG_RTC_DRV_DS1390 is not set
+# CONFIG_RTC_DRV_MAX6902 is not set
+# CONFIG_RTC_DRV_R9701 is not set
+# CONFIG_RTC_DRV_RS5C348 is not set
+# CONFIG_RTC_DRV_DS3234 is not set
+# CONFIG_RTC_DRV_PCF2123 is not set
+
+#
+# Platform RTC drivers
+#
+# CONFIG_RTC_DRV_CMOS is not set
+# CONFIG_RTC_DRV_DS1286 is not set
+# CONFIG_RTC_DRV_DS1511 is not set
+# CONFIG_RTC_DRV_DS1553 is not set
+# CONFIG_RTC_DRV_DS1742 is not set
+# CONFIG_RTC_DRV_STK17TA8 is not set
+# CONFIG_RTC_DRV_M48T86 is not set
+# CONFIG_RTC_DRV_M48T35 is not set
+# CONFIG_RTC_DRV_M48T59 is not set
+# CONFIG_RTC_DRV_MSM6242 is not set
+# CONFIG_RTC_DRV_BQ4802 is not set
+# CONFIG_RTC_DRV_RP5C01 is not set
+# CONFIG_RTC_DRV_V3020 is not set
+
+#
+# on-CPU RTC drivers
+#
+# CONFIG_RTC_DRV_OMAP is not set
+# CONFIG_DMADEVICES is not set
+# CONFIG_AUXDISPLAY is not set
+# CONFIG_UIO is not set
+
+#
+# TI VLYNQ
+#
+# CONFIG_STAGING is not set
+
+#
+# File systems
+#
+CONFIG_EXT2_FS=y
+# CONFIG_EXT2_FS_XATTR is not set
+# CONFIG_EXT2_FS_XIP is not set
+CONFIG_EXT3_FS=y
+# CONFIG_EXT3_DEFAULTS_TO_ORDERED is not set
+CONFIG_EXT3_FS_XATTR=y
+# CONFIG_EXT3_FS_POSIX_ACL is not set
+# CONFIG_EXT3_FS_SECURITY is not set
+# CONFIG_EXT4_FS is not set
+CONFIG_JBD=y
+# CONFIG_JBD_DEBUG is not set
+CONFIG_FS_MBCACHE=y
+# CONFIG_REISERFS_FS is not set
+# CONFIG_JFS_FS is not set
+# CONFIG_FS_POSIX_ACL is not set
+# CONFIG_XFS_FS is not set
+# CONFIG_GFS2_FS is not set
+# CONFIG_OCFS2_FS is not set
+# CONFIG_BTRFS_FS is not set
+# CONFIG_NILFS2_FS is not set
+CONFIG_FILE_LOCKING=y
+CONFIG_FSNOTIFY=y
+CONFIG_DNOTIFY=y
+CONFIG_INOTIFY=y
+CONFIG_INOTIFY_USER=y
+# CONFIG_QUOTA is not set
+# CONFIG_AUTOFS_FS is not set
+CONFIG_AUTOFS4_FS=m
+# CONFIG_FUSE_FS is not set
+
+#
+# Caches
+#
+# CONFIG_FSCACHE is not set
+
+#
+# CD-ROM/DVD Filesystems
+#
+# CONFIG_ISO9660_FS is not set
+# CONFIG_UDF_FS is not set
+
+#
+# DOS/FAT/NT Filesystems
+#
+CONFIG_FAT_FS=y
+CONFIG_MSDOS_FS=y
+CONFIG_VFAT_FS=y
+CONFIG_FAT_DEFAULT_CODEPAGE=437
+CONFIG_FAT_DEFAULT_IOCHARSET="iso8859-1"
+# CONFIG_NTFS_FS is not set
+
+#
+# Pseudo filesystems
+#
+CONFIG_PROC_FS=y
+CONFIG_PROC_SYSCTL=y
+CONFIG_PROC_PAGE_MONITOR=y
+CONFIG_SYSFS=y
+CONFIG_TMPFS=y
+# CONFIG_TMPFS_POSIX_ACL is not set
+# CONFIG_HUGETLB_PAGE is not set
+# CONFIG_CONFIGFS_FS is not set
+CONFIG_MISC_FILESYSTEMS=y
+# CONFIG_ADFS_FS is not set
+# CONFIG_AFFS_FS is not set
+# CONFIG_HFS_FS is not set
+# CONFIG_HFSPLUS_FS is not set
+# CONFIG_BEFS_FS is not set
+# CONFIG_BFS_FS is not set
+# CONFIG_EFS_FS is not set
+CONFIG_JFFS2_FS=y
+CONFIG_JFFS2_FS_DEBUG=0
+CONFIG_JFFS2_FS_WRITEBUFFER=y
+# CONFIG_JFFS2_FS_WBUF_VERIFY is not set
+# CONFIG_JFFS2_SUMMARY is not set
+# CONFIG_JFFS2_FS_XATTR is not set
+# CONFIG_JFFS2_COMPRESSION_OPTIONS is not set
+CONFIG_JFFS2_ZLIB=y
+# CONFIG_JFFS2_LZO is not set
+CONFIG_JFFS2_RTIME=y
+# CONFIG_JFFS2_RUBIN is not set
+CONFIG_CRAMFS=y
+# CONFIG_SQUASHFS is not set
+# CONFIG_VXFS_FS is not set
+CONFIG_MINIX_FS=m
+# CONFIG_OMFS_FS is not set
+# CONFIG_HPFS_FS is not set
+# CONFIG_QNX4FS_FS is not set
+# CONFIG_ROMFS_FS is not set
+# CONFIG_SYSV_FS is not set
+# CONFIG_UFS_FS is not set
+CONFIG_NETWORK_FILESYSTEMS=y
+CONFIG_NFS_FS=y
+CONFIG_NFS_V3=y
+# CONFIG_NFS_V3_ACL is not set
+# CONFIG_NFS_V4 is not set
+CONFIG_ROOT_NFS=y
+CONFIG_NFSD=m
+CONFIG_NFSD_V3=y
+# CONFIG_NFSD_V3_ACL is not set
+# CONFIG_NFSD_V4 is not set
+CONFIG_LOCKD=y
+CONFIG_LOCKD_V4=y
+CONFIG_EXPORTFS=m
+CONFIG_NFS_COMMON=y
+CONFIG_SUNRPC=y
+# CONFIG_RPCSEC_GSS_KRB5 is not set
+# CONFIG_RPCSEC_GSS_SPKM3 is not set
+CONFIG_SMB_FS=m
+# CONFIG_SMB_NLS_DEFAULT is not set
+# CONFIG_CIFS is not set
+# CONFIG_NCP_FS is not set
+# CONFIG_CODA_FS is not set
+# CONFIG_AFS_FS is not set
+
+#
+# Partition Types
+#
+CONFIG_PARTITION_ADVANCED=y
+# CONFIG_ACORN_PARTITION is not set
+# CONFIG_OSF_PARTITION is not set
+# CONFIG_AMIGA_PARTITION is not set
+# CONFIG_ATARI_PARTITION is not set
+# CONFIG_MAC_PARTITION is not set
+CONFIG_MSDOS_PARTITION=y
+# CONFIG_BSD_DISKLABEL is not set
+# CONFIG_MINIX_SUBPARTITION is not set
+# CONFIG_SOLARIS_X86_PARTITION is not set
+# CONFIG_UNIXWARE_DISKLABEL is not set
+# CONFIG_LDM_PARTITION is not set
+# CONFIG_SGI_PARTITION is not set
+# CONFIG_ULTRIX_PARTITION is not set
+# CONFIG_SUN_PARTITION is not set
+# CONFIG_KARMA_PARTITION is not set
+# CONFIG_EFI_PARTITION is not set
+# CONFIG_SYSV68_PARTITION is not set
+CONFIG_NLS=y
+CONFIG_NLS_DEFAULT="iso8859-1"
+CONFIG_NLS_CODEPAGE_437=y
+# CONFIG_NLS_CODEPAGE_737 is not set
+# CONFIG_NLS_CODEPAGE_775 is not set
+# CONFIG_NLS_CODEPAGE_850 is not set
+# CONFIG_NLS_CODEPAGE_852 is not set
+# CONFIG_NLS_CODEPAGE_855 is not set
+# CONFIG_NLS_CODEPAGE_857 is not set
+# CONFIG_NLS_CODEPAGE_860 is not set
+# CONFIG_NLS_CODEPAGE_861 is not set
+# CONFIG_NLS_CODEPAGE_862 is not set
+# CONFIG_NLS_CODEPAGE_863 is not set
+# CONFIG_NLS_CODEPAGE_864 is not set
+# CONFIG_NLS_CODEPAGE_865 is not set
+# CONFIG_NLS_CODEPAGE_866 is not set
+# CONFIG_NLS_CODEPAGE_869 is not set
+# CONFIG_NLS_CODEPAGE_936 is not set
+# CONFIG_NLS_CODEPAGE_950 is not set
+# CONFIG_NLS_CODEPAGE_932 is not set
+# CONFIG_NLS_CODEPAGE_949 is not set
+# CONFIG_NLS_CODEPAGE_874 is not set
+# CONFIG_NLS_ISO8859_8 is not set
+# CONFIG_NLS_CODEPAGE_1250 is not set
+# CONFIG_NLS_CODEPAGE_1251 is not set
+CONFIG_NLS_ASCII=m
+CONFIG_NLS_ISO8859_1=y
+# CONFIG_NLS_ISO8859_2 is not set
+# CONFIG_NLS_ISO8859_3 is not set
+# CONFIG_NLS_ISO8859_4 is not set
+# CONFIG_NLS_ISO8859_5 is not set
+# CONFIG_NLS_ISO8859_6 is not set
+# CONFIG_NLS_ISO8859_7 is not set
+# CONFIG_NLS_ISO8859_9 is not set
+# CONFIG_NLS_ISO8859_13 is not set
+# CONFIG_NLS_ISO8859_14 is not set
+# CONFIG_NLS_ISO8859_15 is not set
+# CONFIG_NLS_KOI8_R is not set
+# CONFIG_NLS_KOI8_U is not set
+CONFIG_NLS_UTF8=m
+# CONFIG_DLM is not set
+
+#
+# Kernel hacking
+#
+# CONFIG_PRINTK_TIME is not set
+# CONFIG_ENABLE_WARN_DEPRECATED is not set
+# CONFIG_ENABLE_MUST_CHECK is not set
+CONFIG_FRAME_WARN=1024
+# CONFIG_MAGIC_SYSRQ is not set
+# CONFIG_STRIP_ASM_SYMS is not set
+# CONFIG_UNUSED_SYMBOLS is not set
+CONFIG_DEBUG_FS=y
+# CONFIG_HEADERS_CHECK is not set
+# CONFIG_DEBUG_KERNEL is not set
+# CONFIG_SLUB_DEBUG_ON is not set
+# CONFIG_SLUB_STATS is not set
+CONFIG_DEBUG_BUGVERBOSE=y
+# CONFIG_DEBUG_MEMORY_INIT is not set
+CONFIG_FRAME_POINTER=y
+# CONFIG_RCU_CPU_STALL_DETECTOR is not set
+# CONFIG_LATENCYTOP is not set
+# CONFIG_SYSCTL_SYSCALL_CHECK is not set
+CONFIG_HAVE_FUNCTION_TRACER=y
+CONFIG_TRACING_SUPPORT=y
+# CONFIG_FTRACE is not set
+# CONFIG_DYNAMIC_DEBUG is not set
+# CONFIG_SAMPLES is not set
+CONFIG_HAVE_ARCH_KGDB=y
+# CONFIG_ARM_UNWIND is not set
+# CONFIG_DEBUG_USER is not set
+# CONFIG_OC_ETM is not set
+
+#
+# Security options
+#
+# CONFIG_KEYS is not set
+# CONFIG_SECURITY is not set
+# CONFIG_SECURITYFS is not set
+# CONFIG_DEFAULT_SECURITY_SELINUX is not set
+# CONFIG_DEFAULT_SECURITY_SMACK is not set
+# CONFIG_DEFAULT_SECURITY_TOMOYO is not set
+CONFIG_DEFAULT_SECURITY_DAC=y
+CONFIG_DEFAULT_SECURITY=""
+CONFIG_CRYPTO=y
+
+#
+# Crypto core or helper
+#
+# CONFIG_CRYPTO_MANAGER is not set
+# CONFIG_CRYPTO_MANAGER2 is not set
+# CONFIG_CRYPTO_GF128MUL is not set
+# CONFIG_CRYPTO_NULL is not set
+# CONFIG_CRYPTO_CRYPTD is not set
+# CONFIG_CRYPTO_AUTHENC is not set
+# CONFIG_CRYPTO_TEST is not set
+
+#
+# Authenticated Encryption with Associated Data
+#
+# CONFIG_CRYPTO_CCM is not set
+# CONFIG_CRYPTO_GCM is not set
+# CONFIG_CRYPTO_SEQIV is not set
+
+#
+# Block modes
+#
+# CONFIG_CRYPTO_CBC is not set
+# CONFIG_CRYPTO_CTR is not set
+# CONFIG_CRYPTO_CTS is not set
+# CONFIG_CRYPTO_ECB is not set
+# CONFIG_CRYPTO_LRW is not set
+# CONFIG_CRYPTO_PCBC is not set
+# CONFIG_CRYPTO_XTS is not set
+
+#
+# Hash modes
+#
+# CONFIG_CRYPTO_HMAC is not set
+# CONFIG_CRYPTO_XCBC is not set
+# CONFIG_CRYPTO_VMAC is not set
+
+#
+# Digest
+#
+# CONFIG_CRYPTO_CRC32C is not set
+# CONFIG_CRYPTO_GHASH is not set
+# CONFIG_CRYPTO_MD4 is not set
+# CONFIG_CRYPTO_MD5 is not set
+# CONFIG_CRYPTO_MICHAEL_MIC is not set
+# CONFIG_CRYPTO_RMD128 is not set
+# CONFIG_CRYPTO_RMD160 is not set
+# CONFIG_CRYPTO_RMD256 is not set
+# CONFIG_CRYPTO_RMD320 is not set
+# CONFIG_CRYPTO_SHA1 is not set
+# CONFIG_CRYPTO_SHA256 is not set
+# CONFIG_CRYPTO_SHA512 is not set
+# CONFIG_CRYPTO_TGR192 is not set
+# CONFIG_CRYPTO_WP512 is not set
+
+#
+# Ciphers
+#
+# CONFIG_CRYPTO_AES is not set
+# CONFIG_CRYPTO_ANUBIS is not set
+# CONFIG_CRYPTO_ARC4 is not set
+# CONFIG_CRYPTO_BLOWFISH is not set
+# CONFIG_CRYPTO_CAMELLIA is not set
+# CONFIG_CRYPTO_CAST5 is not set
+# CONFIG_CRYPTO_CAST6 is not set
+# CONFIG_CRYPTO_DES is not set
+# CONFIG_CRYPTO_FCRYPT is not set
+# CONFIG_CRYPTO_KHAZAD is not set
+# CONFIG_CRYPTO_SALSA20 is not set
+# CONFIG_CRYPTO_SEED is not set
+# CONFIG_CRYPTO_SERPENT is not set
+# CONFIG_CRYPTO_TEA is not set
+# CONFIG_CRYPTO_TWOFISH is not set
+
+#
+# Compression
+#
+# CONFIG_CRYPTO_DEFLATE is not set
+# CONFIG_CRYPTO_ZLIB is not set
+# CONFIG_CRYPTO_LZO is not set
+
+#
+# Random Number Generation
+#
+# CONFIG_CRYPTO_ANSI_CPRNG is not set
+# CONFIG_CRYPTO_HW is not set
+# CONFIG_BINARY_PRINTF is not set
+
+#
+# Library routines
+#
+CONFIG_BITREVERSE=y
+CONFIG_GENERIC_FIND_LAST_BIT=y
+CONFIG_CRC_CCITT=m
+# CONFIG_CRC16 is not set
+CONFIG_CRC_T10DIF=m
+# CONFIG_CRC_ITU_T is not set
+CONFIG_CRC32=y
+# CONFIG_CRC7 is not set
+# CONFIG_LIBCRC32C is not set
+CONFIG_ZLIB_INFLATE=y
+CONFIG_ZLIB_DEFLATE=y
+CONFIG_DECOMPRESS_GZIP=y
+CONFIG_GENERIC_ALLOCATOR=y
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_IOPORT=y
+CONFIG_HAS_DMA=y
+CONFIG_NLATTR=y
diff --git a/arch/arm/mach-davinci/Kconfig b/arch/arm/mach-davinci/Kconfig
index c6d89c9..40c9a45 100644
--- a/arch/arm/mach-davinci/Kconfig
+++ b/arch/arm/mach-davinci/Kconfig
@@ -205,6 +205,13 @@ config DA850_UI_VIDEO_PORT
 	  select Video Port Interface.
 endchoice
 
+config MACH_OMAPL138_HAWKBOARD
+	bool "TI DA850/OMAP-L138/AM18xx Hawkboard(.org) Platform"
+	default ARCH_DAVINCI_DA850
+	depends on ARCH_DAVINCI_DA850
+	help
+	  Say Y here to select the TI DA850/OMAP-L138/AM18xx Hawkboard.
+
 config DAVINCI_MUX
 	bool "DAVINCI multiplexing support"
 	depends on ARCH_DAVINCI
diff --git a/arch/arm/mach-davinci/Makefile b/arch/arm/mach-davinci/Makefile
index f4e55de..ad0e75e 100644
--- a/arch/arm/mach-davinci/Makefile
+++ b/arch/arm/mach-davinci/Makefile
@@ -30,6 +30,7 @@ obj-$(CONFIG_MACH_DAVINCI_DM6467_EVM)	+= board-dm646x-evm.o cdce949.o
 obj-$(CONFIG_MACH_DAVINCI_DM365_EVM)	+= board-dm365-evm.o
 obj-$(CONFIG_MACH_DAVINCI_DA830_EVM)	+= board-da830-evm.o
 obj-$(CONFIG_MACH_DAVINCI_DA850_EVM)	+= board-da850-evm.o
+obj-$(CONFIG_MACH_OMAPL138_HAWKBOARD)	+= board-da850-hawk.o
 
 # Power Management
 obj-$(CONFIG_CPU_FREQ)			+= cpufreq.o
diff --git a/arch/arm/mach-davinci/board-da850-hawk.c b/arch/arm/mach-davinci/board-da850-hawk.c
new file mode 100644
index 0000000..87ed017
--- /dev/null
+++ b/arch/arm/mach-davinci/board-da850-hawk.c
@@ -0,0 +1,657 @@
+/*
+ * TI DA850/OMAP-L138 Hawkboard board
+ *
+ * Copyright (C) 2009 Texas Instruments Incorporated - http://www.ti.com/
+ *
+ * Derived from: arch/arm/mach-davinci/board-da830-hawk.c
+ * Original Copyrights follow:
+ *
+ * 2007, 2009 (c) MontaVista Software, Inc. This file is licensed under
+ * the terms of the GNU General Public License version 2. This program
+ * is licensed "as is" without any warranty of any kind, whether express
+ * or implied.
+ */
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/console.h>
+#include <linux/i2c.h>
+#include <linux/i2c/at24.h>
+#include <linux/i2c/pca953x.h>
+#include <linux/mfd/tps6507x.h>
+#include <linux/gpio.h>
+#include <linux/delay.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/nand.h>
+#include <linux/mtd/partitions.h>
+#include <linux/regulator/machine.h>
+#include <linux/spi/spi.h>
+#include <linux/spi/flash.h>
+#include <linux/usb/musb.h>
+#include <linux/i2c-gpio.h>
+
+#include <asm/mach-types.h>
+#include <asm/mach/arch.h>
+
+#include <mach/cp_intc.h>
+#include <mach/da8xx.h>
+#include <mach/nand.h>
+#include <mach/mux.h>
+#include <mach/flash.h>
+#include <mach/vpif.h>
+
+#include <media/tvp514x.h>
+
+// TODO - check - why is this different from EVM? - default modes - check DS
+#define DA850_HAWK_PHY_MASK		0x1 << 7
+#define DA850_HAWK_MDIO_FREQUENCY	2200000 /* PHY bus frequency */
+
+#define DA850_HAWK_MMCSD_CD_PIN		GPIO_TO_PIN(3, 12)
+#define DA850_HAWK_MMCSD_WP_PIN		GPIO_TO_PIN(3, 13)
+
+#define TVP5147_CH0		"tvp514x-0"
+
+#define VPIF_STATUS	(0x002C)
+#define VPIF_STATUS_CLR	(0x0030)
+
+static struct davinci_pm_config da850_pm_pdata = {
+	.sleepcount = 128,
+};
+
+static struct platform_device da850_pm_device = {
+	.name           = "pm-davinci",
+	.dev = {
+		.platform_data	= &da850_pm_pdata,
+	},
+	.id             = -1,
+};
+
+/* DA850/OMAP-L138 Hawkboard includes a 128 MByte large-page NAND flash
+ * (128K blocks) /?? TODO?
+ */
+struct mtd_partition da850_hawk_nandflash_partition[] = {
+	{
+		.name		= "u-boot env",
+		.offset		= 0,
+		.size		= SZ_128K,
+		.mask_flags	= MTD_WRITEABLE,
+	 },
+	{
+		.name		= "UBL",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= SZ_128K,
+		.mask_flags	= MTD_WRITEABLE,
+	},
+	{
+		.name		= "u-boot",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= 4 * SZ_128K,
+		.mask_flags	= MTD_WRITEABLE,
+	},
+	{
+		.name		= "kernel",
+		.offset		= 0x200000,
+		.size		= SZ_4M,
+		.mask_flags	= 0,
+	},
+	{
+		.name		= "filesystem",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= MTDPART_SIZ_FULL,
+		.mask_flags	= 0,
+	},
+};
+
+// TODO - check timings with Data Sheet
+static struct davinci_aemif_timing da850_hawk_nandflash_timing = {
+	.wsetup		= 0,
+	.wstrobe	= 30,
+	.whold		= 30,
+	.rsetup		= 20,
+	.rstrobe	= 40,
+	.rhold		= 0,
+	.ta		= 0,
+};
+
+static struct davinci_nand_pdata da850_hawk_nandflash_data = {
+	.parts		= da850_hawk_nandflash_partition,
+	.nr_parts	= ARRAY_SIZE(da850_hawk_nandflash_partition),
+	.ecc_mode	= NAND_ECC_HW,
+	.ecc_bits	= 4,
+	.options	= NAND_USE_FLASH_BBT,
+	.timing		= &da850_hawk_nandflash_timing,
+};
+
+static struct resource da850_hawk_nandflash_resource[] = {
+	{
+		.start	= DA8XX_AEMIF_CS3_BASE,
+		.end	= DA8XX_AEMIF_CS3_BASE + SZ_512K + 2 * SZ_1K - 1,
+		.flags	= IORESOURCE_MEM,
+	},
+	{
+		.start	= DA8XX_AEMIF_CTL_BASE,
+		.end	= DA8XX_AEMIF_CTL_BASE + SZ_32K - 1,
+		.flags	= IORESOURCE_MEM,
+	},
+};
+
+static struct platform_device da850_hawk_nandflash_device = {
+	.name		= "davinci_nand",
+	.id		= 1,
+	.dev		= {
+		.platform_data	= &da850_hawk_nandflash_data,
+	},
+	.num_resources	= ARRAY_SIZE(da850_hawk_nandflash_resource),
+	.resource	= da850_hawk_nandflash_resource,
+};
+
+static struct platform_device *da850_hawk_devices[] __initdata = {
+	&da850_hawk_nandflash_device,
+};
+
+#if defined(CONFIG_MMC_DAVINCI) || \
+    defined(CONFIG_MMC_DAVINCI_MODULE)
+#define HAS_MMC 1
+#else
+#define HAS_MMC 0
+#endif
+
+static struct i2c_board_info __initdata da850_hawk_i2c_devices[] = {
+	{
+		I2C_BOARD_INFO("tlv320aic3x", 0x18),
+	},
+// TODO - DDC VGA device I2C?
+};
+
+static struct davinci_uart_config da850_hawk_uart_config __initdata = {
+	.enabled_uarts = 0x7,
+};
+
+/* davinci da850 hawk audio machine driver */
+static u8 da850_iis_serializer_direction[] = {
+	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,
+	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,
+	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,	INACTIVE_MODE,
+	INACTIVE_MODE,	TX_MODE,	RX_MODE,	INACTIVE_MODE,
+};
+
+static struct snd_platform_data da850_hawk_snd_data = {
+	.tx_dma_offset	= 0x2000,
+	.rx_dma_offset	= 0x2000,
+	.op_mode	= DAVINCI_MCASP_IIS_MODE,
+	.num_serializer	= ARRAY_SIZE(da850_iis_serializer_direction),
+	.tdm_slots	= 2,
+	.serial_dir	= da850_iis_serializer_direction,
+	.eventq_no	= EVENTQ_1,
+	.version	= MCASP_VERSION_2,
+	.txnumevt	= 1,
+	.rxnumevt	= 1,
+};
+
+static struct davinci_mcbsp_platform_data da850_mcbsp0_config = {
+	.inst	= 0,
+};
+
+static struct davinci_mcbsp_platform_data da850_mcbsp1_config = {
+	.inst	= 1,
+};
+
+static int da850_hawk_mmc_get_ro(int index)
+{
+	return gpio_get_value(DA850_HAWK_MMCSD_WP_PIN);
+}
+
+static int da850_hawk_mmc_get_cd(int index)
+{
+	return !gpio_get_value(DA850_HAWK_MMCSD_CD_PIN);
+}
+
+static struct davinci_mmc_config da850_mmc_config = {
+	.get_ro		= da850_hawk_mmc_get_ro,
+	.get_cd		= da850_hawk_mmc_get_cd,
+	.wires		= 4,
+	.max_freq	= 50000000,
+	.caps		= MMC_CAP_MMC_HIGHSPEED | MMC_CAP_SD_HIGHSPEED,
+	.version	= MMC_CTLR_VERSION_2,
+};
+
+static int da850_lcd_hw_init(void)
+{
+	void __iomem *cfg_mstpri2_base;
+	u32 val;
+
+	/*
+	 * Reconfigure the LCDC priority to the highest to ensure that
+	 * the throughput/latency requirements for the LCDC are met.
+	 */
+	cfg_mstpri2_base = DA8XX_SYSCFG0_VIRT(DA8XX_MSTPRI2_REG);
+
+	val = __raw_readl(cfg_mstpri2_base);
+	val &= 0x0fffffff;
+	__raw_writel(val, cfg_mstpri2_base);
+
+	return 0;
+}
+
+static int __init da850_hawk_config_emac(void)
+{
+	void __iomem *cfg_chip3_base;
+	int ret;
+	u32 val;
+	struct davinci_soc_info *soc_info = &davinci_soc_info;
+
+	if (!machine_is_omapl138_hawkboard())
+		return 0;
+
+	cfg_chip3_base = DA8XX_SYSCFG0_VIRT(DA8XX_CFGCHIP3_REG);
+
+	val = __raw_readl(cfg_chip3_base);
+
+	val &= ~BIT(8);
+	ret = da8xx_pinmux_setup(da850_cpgmac_pins);
+	if (ret)
+		pr_warning("da850_evm_init: cpgmac/rmii mux setup failed: %d\n",
+				ret);
+
+	/* configure the CFGCHIP3 register for MII */
+	__raw_writel(val, cfg_chip3_base);
+
+	soc_info->emac_pdata->phy_mask = DA850_HAWK_PHY_MASK;
+	soc_info->emac_pdata->mdio_max_freq = DA850_HAWK_MDIO_FREQUENCY;
+
+	ret = da8xx_register_emac();
+	if (ret)
+		pr_warning("da850_hawk_init: emac registration failed: %d\n",
+				ret);
+
+	return 0;
+}
+device_initcall(da850_hawk_config_emac);
+
+static int da850_setup_vpif_input_channel_mode(int mux_mode)
+{
+	return 0;
+}
+
+static int da850_vpif_intr_status(void __iomem *vpif_base, int channel)
+{
+	int status = 0;
+	int mask;
+
+	// TODO - only one channel active on hawk?
+	if (channel < 0 || channel > 3)
+		return 0;
+
+	mask = 1 << channel;
+	status = __raw_readl((vpif_base + VPIF_STATUS)) & mask;
+	__raw_writel(status, (vpif_base + VPIF_STATUS_CLR));
+
+	return status;
+}
+
+/* VPIF capture configuration */
+static struct tvp514x_platform_data tvp5146_pdata = {
+	.clk_polarity = 0,
+	.hs_polarity = 1,
+	.vs_polarity = 1
+};
+
+#define TVP514X_STD_ALL (V4L2_STD_NTSC | V4L2_STD_PAL)
+
+static struct vpif_subdev_info da850_vpif_capture_sdev_info[] = {
+	{
+		.name	= TVP5147_CH0,
+		.board_info = {
+			I2C_BOARD_INFO("tvp5146", 0x5d),
+			.platform_data = &tvp5146_pdata,
+		},
+		.input = INPUT_CVBS_VI2B,
+		.output = OUTPUT_10BIT_422_EMBEDDED_SYNC,
+		.can_route = 1,
+		.vpif_if = {
+			.if_type = VPIF_IF_BT656,
+			.hd_pol = 1,
+			.vd_pol = 1,
+			.fid_pol = 0,
+		},
+	},
+};
+
+static const struct vpif_input da850_ch0_inputs[] = {
+	{
+		.input = {
+			.index = 0,
+			.name = "Composite",
+			.type = V4L2_INPUT_TYPE_CAMERA,
+			.std = TVP514X_STD_ALL,
+		},
+		.subdev_name = TVP5147_CH0,
+	},
+};
+
+// TODO - V4L2 device creates 2 device nodes for 2 channels - why?
+// - do we need to set .chan_config[1] to NULL?
+static struct vpif_capture_config da850_vpif_capture_config = {
+	.setup_input_channel_mode = da850_setup_vpif_input_channel_mode,
+	.intr_status = da850_vpif_intr_status,
+	.subdev_info = da850_vpif_capture_sdev_info,
+	.subdev_count = ARRAY_SIZE(da850_vpif_capture_sdev_info),
+	.chan_config[0] = {
+		.inputs = da850_ch0_inputs,
+		.input_count = ARRAY_SIZE(da850_ch0_inputs),
+	},
+        .card_name      = "DA850/OMAP-L138 Video Capture",
+};
+
+// TODO - fix all these references to _UI
+
+#if defined(CONFIG_DAVINCI_MCBSP0)
+#define HAS_MCBSP0 1
+#else
+#define HAS_MCBSP0 0
+#endif
+
+#if defined(CONFIG_DAVINCI_MCBSP1)
+#define HAS_MCBSP1 1
+#else
+#define HAS_MCBSP1 0
+#endif
+
+#if defined(CONFIG_TI_DAVINCI_EMAC) || \
+	defined(CONFIG_TI_DAVINCI_EMAC_MODULE)
+#define HAS_EMAC 1
+#else
+#define HAS_EMAC 0
+#endif
+
+//TODO - fix dependence on _EVM
+#if defined(CONFIG_SND_DA850_SOC_EVM) || \
+	defined(CONFIG_SND_DA850_SOC_EVM_MODULE)
+#define HAS_MCASP 1
+#else
+#define HAS_MCASP 0
+#endif
+
+#if defined(CONFIG_DA850_UI_RMII) && (HAS_EMAC)
+#define HAS_RMII 1
+#else
+#define HAS_RMII 0
+#endif
+
+#if defined(CONFIG_DA850_UI_LCD) && defined(CONFIG_FB_DA8XX) ||\
+		defined(CONFIG_FB_DA8XX_MODULE)
+#define HAS_GLCD 1
+#else
+#define HAS_GLCD 0
+#endif
+
+#if defined(CONFIG_VIDEO_DAVINCI_VPIF_DISPLAY) ||\
+		defined(CONFIG_VIDEO_DAVINCI_VPIF_DISPLAY_MODULE)
+#define HAS_VPIF_DISPLAY 1
+#else
+#define HAS_VPIF_DISPLAY 0
+#endif
+
+#if defined(CONFIG_VIDEO_DAVINCI_VPIF_CAPTURE) ||\
+		defined(CONFIG_VIDEO_DAVINCI_VPIF_CAPTURE_MODULE)
+#define HAS_VPIF_CAPTURE 1
+#else
+#define HAS_VPIF_CAPTURE 0
+#endif
+
+static struct da8xx_ohci_root_hub da850_hawk_usb11_pdata = {
+};
+
+static struct musb_hdrc_platform_data usb_hawk_data[] = {
+	{
+#ifdef CONFIG_USB_MUSB_OTG
+		.mode = MUSB_OTG,
+#elif defined(CONFIG_USB_MUSB_DUAL_ROLE)
+		.mode = MUSB_DUAL_ROLE,
+#elif defined(CONFIG_USB_MUSB_PERIPHERAL)
+		.mode =  MUSB_PERIPHERAL,
+#elif defined(CONFIG_USB_MUSB_HOST)
+		.mode = MUSB_HOST,
+#endif
+		.power = 255,
+		.potpgt = 8,
+		.set_vbus = NULL, /* VBUs is directly controlled by the IP */
+	}
+};
+
+static __init void da850_hawk_usb_init(void)
+{
+	int ret;
+	u32 cfgchip2;
+
+	/*
+	 * Setup the Ref. clock frequency for the HAWK at 24 MHz.
+	 */
+	cfgchip2 = __raw_readl(DA8XX_SYSCFG0_VIRT(DA8XX_CFGCHIP2_REG));
+	cfgchip2 &= ~CFGCHIP2_REFFREQ;
+	cfgchip2 |=  CFGCHIP2_REFFREQ_24MHZ;
+	__raw_writel(cfgchip2, DA8XX_SYSCFG0_VIRT(DA8XX_CFGCHIP2_REG));
+
+	da8xx_usb20_configure(usb_hawk_data, ARRAY_SIZE(usb_hawk_data));
+
+	ret = da8xx_register_usb11(&da850_hawk_usb11_pdata);
+	if (ret)
+		pr_warning("%s: USB 1.1 registration failed: %d\n",
+			   __func__, ret);
+}
+
+static struct i2c_gpio_platform_data da850_gpio_i2c_pdata = {
+	.sda_pin	= GPIO_TO_PIN(1, 4),
+	.scl_pin	= GPIO_TO_PIN(1, 5),
+	.udelay		= 2,			/* 250 KHz */
+};
+
+static struct platform_device da850_gpio_i2c = {
+	.name		= "i2c-gpio",
+	.id		= 1,
+	.dev		= {
+	.platform_data	= &da850_gpio_i2c_pdata,
+	},
+};
+
+static __init void da850_hawk_init(void)
+{
+	int ret;
+
+	ret = da8xx_register_edma();
+	if (ret)
+		pr_warning("da850_hawk_init: edma registration failed: %d\n",
+				ret);
+
+	// TODO - check safe to enable alongside MMC
+	ret = da8xx_pinmux_setup(da850_nand_pins);
+	if (ret)
+		pr_warning("da850_hawk_init: nand mux setup failed: "
+				"%d\n", ret);
+
+	platform_add_devices(da850_hawk_devices,
+				ARRAY_SIZE(da850_hawk_devices));
+
+	ret = da8xx_pinmux_setup(da850_i2c0_pins);
+	if (ret)
+		pr_warning("da850_hawk_init: i2c0 mux setup failed: %d\n",
+				ret);
+
+	platform_device_register(&da850_gpio_i2c);
+
+	ret = da8xx_register_watchdog();
+	if (ret)
+		pr_warning("da830_hawk_init: watchdog registration failed: %d\n",
+				ret);
+
+	if (HAS_MMC) {
+		ret = da8xx_pinmux_setup(da850_mmcsd0_pins);
+		if (ret)
+			pr_warning("da850_hawk_init: mmcsd0 mux setup failed:"
+					" %d\n", ret);
+
+		ret = gpio_request(DA850_HAWK_MMCSD_CD_PIN, "MMC CD\n");
+		if (ret)
+			pr_warning("da850_hawk_init: can not open GPIO %d\n",
+					DA850_HAWK_MMCSD_CD_PIN);
+		gpio_direction_input(DA850_HAWK_MMCSD_CD_PIN);
+
+		ret = gpio_request(DA850_HAWK_MMCSD_WP_PIN, "MMC WP\n");
+		if (ret)
+			pr_warning("da850_hawk_init: can not open GPIO %d\n",
+					DA850_HAWK_MMCSD_WP_PIN);
+		gpio_direction_input(DA850_HAWK_MMCSD_WP_PIN);
+
+		ret = da8xx_register_mmcsd0(&da850_mmc_config);
+		if (ret)
+			pr_warning("da850_hawk_init: mmcsd0 registration failed:"
+					" %d\n", ret);
+	}
+
+	davinci_serial_init(&da850_hawk_uart_config);
+
+	i2c_register_board_info(1, da850_hawk_i2c_devices,
+			ARRAY_SIZE(da850_hawk_i2c_devices));
+
+	/*
+	 * shut down uart 0 and 1; they are not used on the board and
+	 * accessing them causes endless "too much work in irq53" messages
+	 * with arago fs
+	 */
+	__raw_writel(0, IO_ADDRESS(DA8XX_UART1_BASE) + 0x30);
+	__raw_writel(0, IO_ADDRESS(DA8XX_UART0_BASE) + 0x30);
+
+	if (HAS_MCBSP0) {
+		if (HAS_EMAC)
+			pr_warning("WARNING: both MCBSP0 and EMAC are "
+				"enabled, but they share pins.\n"
+				"\tDisable one of them.\n");
+
+		ret = da8xx_pinmux_setup(da850_mcbsp0_pins);
+		if (ret)
+			pr_warning("da850_hawk_init: mcbsp0 mux setup failed:"
+					" %d\n", ret);
+
+		ret = da850_init_mcbsp(&da850_mcbsp0_config);
+		if (ret)
+			pr_warning("da850_hawk_init: mcbsp0 registration"
+					"failed: %d\n",	ret);
+	}
+
+	if (HAS_MCBSP1) {
+		ret = da8xx_pinmux_setup(da850_mcbsp1_pins);
+		if (ret)
+			pr_warning("da850_hawl_init: mcbsp1 mux setup failed:"
+					" %d\n", ret);
+
+		ret = da850_init_mcbsp(&da850_mcbsp1_config);
+		if (ret)
+			pr_warning("da850_hawk_init: mcbsp1 registration"
+					" failed: %d\n", ret);
+	}
+
+	if (HAS_MCASP) {
+		if ((HAS_MCBSP0 || HAS_MCBSP1))
+			pr_warning("WARNING: both McASP and McBSP are enabled, "
+					"but they share pins.\n"
+					"\tDisable one of them.\n");
+
+		ret = da8xx_pinmux_setup(da850_mcasp_pins);
+		if (ret)
+			pr_warning("da850_hawk_init: mcasp mux setup failed:"
+					"%d\n", ret);
+
+		da8xx_register_mcasp(0, &da850_hawk_snd_data);
+	}
+
+	ret = da8xx_pinmux_setup(da850_lcdcntl_pins);
+	if (ret)
+		pr_warning("da850_evm_init: lcdcntl mux setup failed: %d\n",
+				ret);
+
+	ret = da850_lcd_hw_init();
+	if (ret)
+		pr_warning("da850_hawk_init: lcd initialization failed: %d\n",
+				ret);
+
+	ret = da8xx_register_lcdc(&vga_monitor_pdata);
+	if (ret)
+		pr_warning("da850_hawk_init: lcdc registration failed: %d\n",
+				ret);
+
+	// Default hawkboard doesn't have RTC battery - so CONFIG_RTC_DRV_OMAP
+	//  should be disabled by default
+        ret = da8xx_register_rtc();
+	if (ret)
+		pr_warning("da850_hawk_init: rtc setup failed: %d\n", ret);
+
+	// Generic da850(.c) CPUFREQ support ok as long as CONFIG_REGULATOR disabled
+        ret = da850_register_cpufreq();
+	if (ret)
+		pr_warning("da850_hawk_init: cpufreq registration failed: %d\n",
+				ret);
+
+	ret = da8xx_register_cpuidle();
+	if (ret)
+		pr_warning("da850_hawk_init: cpuidle registration failed: %d\n",
+				ret);
+
+        // Wake-Up relies upon RTC (which requires battery fitted
+	ret = da850_register_pm(&da850_pm_device);
+	if (ret)
+		pr_warning("da850_hawk_init: suspend registration failed: %d\n",
+				ret);
+
+	da850_hawk_usb_init();
+
+	ret = da8xx_register_sata();
+	if (ret)
+		pr_warning("da850_hawk_init: SATA registration failed: %d\n",
+						ret);
+
+	ret = da850_register_vpif();
+	if (ret)
+		pr_warning("da850_hawk_init: VPIF registration failed: "
+					"%d\n",	ret);
+
+	ret = da8xx_pinmux_setup(da850_vpif_capture_pins);
+	if (ret)
+		pr_warning("da850_hawk_init: vpif capture mux failed: "
+					"%d\n",	ret);
+
+	ret = da850_register_vpif_capture(&da850_vpif_capture_config);
+	if (ret)
+		pr_warning("da850_hawk_init: VPIF registration failed: "
+					"%d\n",	ret);
+}
+
+#ifdef CONFIG_SERIAL_8250_CONSOLE
+static int __init da850_hawk_console_init(void)
+{
+	return add_preferred_console("ttyS", 2, "115200");
+}
+console_initcall(da850_hawk_console_init);
+#endif
+
+static __init void da850_hawk_irq_init(void)
+{
+	struct davinci_soc_info *soc_info = &davinci_soc_info;
+
+	cp_intc_init((void __iomem *)DA8XX_CP_INTC_VIRT, DA850_N_CP_INTC_IRQ,
+			soc_info->intc_irq_prios);
+}
+
+static void __init da850_hawk_map_io(void)
+{
+	da850_init();
+}
+
+MACHINE_START(OMAPL138_HAWKBOARD, "DaVinci DA850/OMAP-L138/AM18xx Hawkboard(.org)")
+	.phys_io	= IO_PHYS,
+	.io_pg_offst	= (__IO_ADDRESS(IO_PHYS) >> 18) & 0xfffc,
+	.boot_params	= (DA8XX_DDR_BASE + 0x100),
+	.map_io		= da850_hawk_map_io,
+	.init_irq	= da850_hawk_irq_init,
+	.timer		= &davinci_timer,
+	.init_machine	= da850_hawk_init,
+MACHINE_END
diff --git a/arch/arm/mach-davinci/da850.c b/arch/arm/mach-davinci/da850.c
index cfecd3c..a32c636 100755
--- a/arch/arm/mach-davinci/da850.c
+++ b/arch/arm/mach-davinci/da850.c
@@ -720,7 +720,7 @@ const short da850_rmii_pins[] __initdata = {
 const short da850_mcasp_pins[] __initdata = {
 	DA850_AHCLKX, DA850_ACLKX, DA850_AFSX,
 	DA850_AHCLKR, DA850_ACLKR, DA850_AFSR, DA850_AMUTE,
-	DA850_AXR_11, DA850_AXR_12,
+	DA850_AXR_11, DA850_AXR_12, DA850_AXR_13, DA850_AXR_14,
 	-1
 };
 
diff --git a/arch/arm/mach-davinci/devices-da8xx.c b/arch/arm/mach-davinci/devices-da8xx.c
index 0842590..97a4611 100755
--- a/arch/arm/mach-davinci/devices-da8xx.c
+++ b/arch/arm/mach-davinci/devices-da8xx.c
@@ -560,6 +560,12 @@ struct da8xx_lcdc_platform_data sharp_lk043t1dg01_pdata = {
 	.type			= "Sharp_LK043T1DG01",
 };
 
+struct da8xx_lcdc_platform_data vga_monitor_pdata = {
+	.manu_name		= "vga_mon",
+	.controller_data	= &lcd_cfg,
+	.type			= "VGA_Monitor",
+};
+
 #if !defined(CONFIG_FB_DA8XX) && !defined(CONFIG_FB_DA8XX_MODULE)
 static struct da8xx_clcd_platform_data da8xx_evm_clcd_pdata = {
 	.version = CONFIG_SPACE_1,
@@ -664,9 +670,11 @@ int da8xx_register_rtc(void)
 {
 	int ret;
 
+#ifdef CONFIG_RTC_DRV_OMAP
 	/* Unlock the rtc's registers */
 	__raw_writel(0x83e70b13, IO_ADDRESS(DA8XX_RTC_BASE + 0x6c));
 	__raw_writel(0x95a4f1e0, IO_ADDRESS(DA8XX_RTC_BASE + 0x70));
+#endif
 
 	ret = platform_device_register(&da8xx_rtc_device);
 	if (!ret)
diff --git a/arch/arm/mach-davinci/include/mach/da8xx.h b/arch/arm/mach-davinci/include/mach/da8xx.h
index f76433f..c39b5b0 100755
--- a/arch/arm/mach-davinci/include/mach/da8xx.h
+++ b/arch/arm/mach-davinci/include/mach/da8xx.h
@@ -168,6 +168,8 @@ extern struct platform_device da8xx_serial_device;
 extern struct emac_platform_data da8xx_emac_pdata;
 extern struct da8xx_lcdc_platform_data sharp_lcd035q3dg01_pdata;
 extern struct da8xx_lcdc_platform_data sharp_lk043t1dg01_pdata;
+extern struct da8xx_lcdc_platform_data vga_monitor_pdata;
+
 void da8xx_usb20_configure(struct musb_hdrc_platform_data *pdata, u8 num_inst);
 
 extern const short da830_emif25_pins[];
diff --git a/arch/arm/mach-davinci/include/mach/debug-macro.S b/arch/arm/mach-davinci/include/mach/debug-macro.S
index 17ab523..f04c481 100644
--- a/arch/arm/mach-davinci/include/mach/debug-macro.S
+++ b/arch/arm/mach-davinci/include/mach/debug-macro.S
@@ -27,7 +27,8 @@
 #if defined(CONFIG_ARCH_DAVINCI_DA8XX) && defined(CONFIG_ARCH_DAVINCI_DMx)
 #error Cannot enable DaVinci and DA8XX platforms concurrently
 #elif defined(CONFIG_MACH_DAVINCI_DA830_EVM) || \
-	defined(CONFIG_MACH_DAVINCI_DA850_EVM)
+	defined(CONFIG_MACH_DAVINCI_DA850_EVM) || \
+		defined(CONFIG_MACH_OMAPL138_HAWKBOARD)
 		orr	\rx, \rx, #0x00d00000	@ physical base address
 		orr	\rx, \rx, #0x0000d000	@ of UART 2
 #else
diff --git a/drivers/media/video/Kconfig b/drivers/media/video/Kconfig
index d0db690..ea91489 100644
--- a/drivers/media/video/Kconfig
+++ b/drivers/media/video/Kconfig
@@ -513,11 +513,11 @@ config VIDEO_DAVINCI_VPIF_DISPLAY
 
 config VIDEO_DAVINCI_VPIF_CAPTURE
 	tristate "DaVinci Video VPIF Capture"
-	depends on VIDEO_DEV && (MACH_DAVINCI_DM6467_EVM || MACH_DAVINCI_DA850_EVM)
+	depends on VIDEO_DEV && (MACH_DAVINCI_DM6467_EVM || MACH_DAVINCI_DA850_EVM || MACH_OMAPL138_HAWKBOARD)
 	select VIDEOBUF_DMA_CONTIG
 	select VIDEO_DAVINCI_VPIF
 	help
-	  Support for DaVinci VPIF Capture on DM6467 EVM and/or DA850/OMAP-L138/AM18xx EVM.
+	  Support for DaVinci VPIF Capture on DM6467 EVM and/or DA850/OMAP-L138/AM18xx EVM/Hawkboard.
 
 	  To compile this driver as a module, choose M here: the
 	  module will be called vpif_capture.
diff --git a/drivers/video/da8xx-fb.c b/drivers/video/da8xx-fb.c
index faa1fd3..d416923 100644
--- a/drivers/video/da8xx-fb.c
+++ b/drivers/video/da8xx-fb.c
@@ -196,6 +196,20 @@ static struct da8xx_panel known_lcd_panels[] = {
 		.pxl_clk = 7833600,
 		.invert_pxl_clk = 0,
 	},
+	/* CRT Monitor or LCD Screen */
+	[2] = {
+		.name = "VGA_Monitor",
+		.width = 640,
+		.height = 480,
+		.hfp = 48,
+		.hbp = 48,
+		.hsw = 63,
+		.vfp = 11,
+		.vbp = 31,
+		.vsw = 1,
+		.pxl_clk = 25000000,
+		.invert_pxl_clk = 1,
+	},
 };
 
 /* Enable the Raster Engine of the LCD Controller */
diff --git a/sound/soc/davinci/Kconfig b/sound/soc/davinci/Kconfig
index 62dab95..8b34b5b 100644
--- a/sound/soc/davinci/Kconfig
+++ b/sound/soc/davinci/Kconfig
@@ -53,11 +53,11 @@ config  SND_DA830_SOC_EVM
 	  DA830/OMAP-L137/AM17xx EVM
 
 config  SND_DA850_SOC_EVM
-	tristate "SoC Audio support for DA850/OMAP-L138/AM18xx EVM"
-	depends on SND_DAVINCI_SOC && MACH_DAVINCI_DA850_EVM
+	tristate "SoC Audio support for DA850/OMAP-L138/AM18xx EVM / Hawkboard"
+	depends on SND_DAVINCI_SOC && (MACH_DAVINCI_DA850_EVM || MACH_OMAPL138_HAWKBOARD)
 	select SND_DAVINCI_SOC_MCASP
 	select SND_SOC_TLV320AIC3X
 	help
 	  Say Y if you want to add support for SoC audio on TI
-	  DA850/OMAP-L138/AM18xx EVM
+	  DA850/OMAP-L138/AM18xx EVM/Hawkboard
 
diff --git a/sound/soc/davinci/davinci-evm.c b/sound/soc/davinci/davinci-evm.c
index 7ccbe66..a7594b8 100644
--- a/sound/soc/davinci/davinci-evm.c
+++ b/sound/soc/davinci/davinci-evm.c
@@ -57,7 +57,8 @@ static int evm_hw_params(struct snd_pcm_substream *substream,
 		sysclk = 12288000;
 
 	else if (machine_is_davinci_da830_evm() ||
-				machine_is_davinci_da850_evm())
+				machine_is_davinci_da850_evm() ||
+				machine_is_omapl138_hawkboard() )
 		sysclk = 24576000;
 
 	else
@@ -256,7 +257,7 @@ static int __init evm_init(void)
 	} else if (machine_is_davinci_da830_evm()) {
 		evm_snd_dev_data = &da830_evm_snd_devdata;
 		index = 1;
-	} else if (machine_is_davinci_da850_evm()) {
+	} else if (machine_is_davinci_da850_evm() || machine_is_omapl138_hawkboard()) {
 		evm_snd_dev_data = &da850_evm_snd_devdata;
 		index = 0;
 	} else
-- 
1.6.0.6

