From 12c00e7ab93ca9cb7621bb62f6b27304fedf4be8 Mon Sep 17 00:00:00 2001
From: Andy Green <andy@warmcat.com>
Date: Sun, 10 Jul 2011 05:27:15 -0600
Subject: [PATCH 072/149] I2C: OMAP2+: Tag all OMAP2+ hwmod defintions with I2C IP revision

Since we cannot trust (or even reliably find) the OMAP I2C
peripheral unit's own revision register, we must inform the
OMAP i2c driver of which IP version it is running on.  We
do this by tagging the omap_hwmod_class for i2c on all the
OMAP2+ platform / cpu specific hwmod init and passing it up
to the driver (next patches).

Cc: patches@linaro.org
Cc: Ben Dooks <ben-linux@fluff.org>
Reported-by: Peter Maydell <peter.maydell@linaro.org>
Signed-off-by: Andy Green <andy.green@linaro.org>
Signed-off-by: Tony Lindgren <tony@atomide.com>
Signed-off-by: Kevin Hilman <khilman@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/omap_hwmod_2420_data.c |    1 +
 arch/arm/mach-omap2/omap_hwmod_2430_data.c |    1 +
 arch/arm/mach-omap2/omap_hwmod_3xxx_data.c |    1 +
 arch/arm/mach-omap2/omap_hwmod_44xx_data.c |    1 +
 4 files changed, 4 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/omap_hwmod_2420_data.c b/arch/arm/mach-omap2/omap_hwmod_2420_data.c
index f3901ab..95f547c 100644
--- a/arch/arm/mach-omap2/omap_hwmod_2420_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_2420_data.c
@@ -1029,6 +1029,7 @@ static struct omap_hwmod_class_sysconfig i2c_sysc = {
 static struct omap_hwmod_class i2c_class = {
 	.name		= "i2c",
 	.sysc		= &i2c_sysc,
+	.rev		= OMAP_I2C_IP_VERSION_1,
 };
 
 static struct omap_i2c_dev_attr i2c_dev_attr;
diff --git a/arch/arm/mach-omap2/omap_hwmod_2430_data.c b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
index 19ddf08..d7ed51b 100644
--- a/arch/arm/mach-omap2/omap_hwmod_2430_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
@@ -1078,6 +1078,7 @@ static struct omap_hwmod_class_sysconfig i2c_sysc = {
 static struct omap_hwmod_class i2c_class = {
 	.name		= "i2c",
 	.sysc		= &i2c_sysc,
+	.rev		= OMAP_I2C_IP_VERSION_1,
 };
 
 static struct omap_i2c_dev_attr i2c_dev_attr = {
diff --git a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
index 542a11b..58ec1e2 100644
--- a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
@@ -1308,6 +1308,7 @@ static struct omap_hwmod omap3xxx_uart4_hwmod = {
 static struct omap_hwmod_class i2c_class = {
 	.name = "i2c",
 	.sysc = &i2c_sysc,
+	.rev  = OMAP_I2C_IP_VERSION_1,
 };
 
 static struct omap_hwmod_dma_info omap3xxx_dss_sdma_chs[] = {
diff --git a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
index 2ebccb8..1bed3b8 100644
--- a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
@@ -2160,6 +2160,7 @@ static struct omap_hwmod_class_sysconfig omap44xx_i2c_sysc = {
 static struct omap_hwmod_class omap44xx_i2c_hwmod_class = {
 	.name	= "i2c",
 	.sysc	= &omap44xx_i2c_sysc,
+	.rev	= OMAP_I2C_IP_VERSION_2,
 };
 
 /* i2c1 */
-- 
1.6.6.1

