From c510bdc2684b5a755c4526071f1f3ca726ac1d1d Mon Sep 17 00:00:00 2001
From: Jason Kridner <jkridner@beagleboard.org>
Date: Tue, 19 Apr 2011 10:55:26 -0500
Subject: [PATCH 25/30] BeagleBoard: fix LED 0/1 in driver

Fixed USR0/USR1 to be LED 0/1 respectively

Signed-off-by: Jason Kridner <jkridner@beagleboard.org>
Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 board/ti/beagle/led.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/board/ti/beagle/led.c b/board/ti/beagle/led.c
index 08f95a0..d3de51f 100644
--- a/board/ti/beagle/led.c
+++ b/board/ti/beagle/led.c
@@ -27,8 +27,8 @@
 static unsigned int saved_state[2] = {STATUS_LED_OFF, STATUS_LED_OFF};
 
 /* GPIO pins for the LEDs */
-#define BEAGLE_LED_USR0	149
-#define BEAGLE_LED_USR1	150
+#define BEAGLE_LED_USR0	150
+#define BEAGLE_LED_USR1	149
 
 #ifdef STATUS_LED_GREEN
 void green_LED_off (void)
-- 
1.6.6.1

