From 47ca09682a2c2ce670196443dbb3946057bc39e6 Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Fri, 1 Jul 2011 22:54:05 +0200
Subject: [PATCH 034/149] OMAP2+: hwmod: Fix the HW reset management

The HW reset must be de-assert after the clocks are enabled
but before waiting for the target to be ready. Otherwise the
reset might not work properly since the clock is not running
to proceed the reset.

De-assert the reset after _enable_clocks and before
_wait_target_ready.
Re-assert it only when the clocks are disabled.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/omap_hwmod.c |   32 ++++++++++++++++----------------
 1 files changed, 16 insertions(+), 16 deletions(-)

diff --git a/arch/arm/mach-omap2/omap_hwmod.c b/arch/arm/mach-omap2/omap_hwmod.c
index f401417..df91bb1 100644
--- a/arch/arm/mach-omap2/omap_hwmod.c
+++ b/arch/arm/mach-omap2/omap_hwmod.c
@@ -1250,15 +1250,6 @@ static int _enable(struct omap_hwmod *oh)
 
 	pr_debug("omap_hwmod: %s: enabling\n", oh->name);
 
-	/*
-	 * If an IP contains only one HW reset line, then de-assert it in order
-	 * to allow to enable the clocks. Otherwise the PRCM will return
-	 * Intransition status, and the init will failed.
-	 */
-	if ((oh->_state == _HWMOD_STATE_INITIALIZED ||
-	     oh->_state == _HWMOD_STATE_DISABLED) && oh->rst_lines_cnt == 1)
-		_deassert_hardreset(oh, oh->rst_lines[0].name);
-
 	/* Mux pins for device runtime if populated */
 	if (oh->mux && (!oh->mux->enabled ||
 			((oh->_state == _HWMOD_STATE_IDLE) &&
@@ -1268,6 +1259,15 @@ static int _enable(struct omap_hwmod *oh)
 	_add_initiator_dep(oh, mpu_oh);
 	_enable_clocks(oh);
 
+	/*
+	 * If an IP contains only one HW reset line, then de-assert it in order
+	 * to allow the module state transition. Otherwise the PRCM will return
+	 * Intransition status, and the init will failed.
+	 */
+	if ((oh->_state == _HWMOD_STATE_INITIALIZED ||
+	     oh->_state == _HWMOD_STATE_DISABLED) && oh->rst_lines_cnt == 1)
+		_deassert_hardreset(oh, oh->rst_lines[0].name);
+
 	r = _wait_target_ready(oh);
 	if (!r) {
 		oh->_state = _HWMOD_STATE_ENABLED;
@@ -1396,13 +1396,6 @@ static int _shutdown(struct omap_hwmod *oh)
 		_shutdown_sysc(oh);
 	}
 
-	/*
-	 * If an IP contains only one HW reset line, then assert it
-	 * before disabling the clocks and shutting down the IP.
-	 */
-	if (oh->rst_lines_cnt == 1)
-		_assert_hardreset(oh, oh->rst_lines[0].name);
-
 	/* clocks and deps are already disabled in idle */
 	if (oh->_state == _HWMOD_STATE_ENABLED) {
 		_del_initiator_dep(oh, mpu_oh);
@@ -1411,6 +1404,13 @@ static int _shutdown(struct omap_hwmod *oh)
 	}
 	/* XXX Should this code also force-disable the optional clocks? */
 
+	/*
+	 * If an IP contains only one HW reset line, then assert it
+	 * after disabling the clocks and before shutting down the IP.
+	 */
+	if (oh->rst_lines_cnt == 1)
+		_assert_hardreset(oh, oh->rst_lines[0].name);
+
 	/* Mux pins to safe mode or use populated off mode values */
 	if (oh->mux)
 		omap_hwmod_mux(oh->mux, _HWMOD_STATE_DISABLED);
-- 
1.6.6.1

