From cad762e20178949527118629d7cf1298e38658f2 Mon Sep 17 00:00:00 2001
From: Steve Kipisz <s-kipisz2@ti.com>
Date: Tue, 15 Nov 2011 10:47:40 -0600
Subject: [PATCH 1/3] arm:omap:mux33xx: Add i2c2 pin muix

Signed-off-by: Steve Kipisz <s-kipisz2@ti.com>
Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/mux33xx.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/mux33xx.c b/arch/arm/mach-omap2/mux33xx.c
index 4399003..06719df 100644
--- a/arch/arm/mach-omap2/mux33xx.c
+++ b/arch/arm/mach-omap2/mux33xx.c
@@ -315,10 +315,10 @@ static struct omap_mux __initdata am33xx_muxmodes[] = {
 		"uart0_txd", "spi1_cs1", NULL, NULL,
 		NULL, NULL, NULL, NULL),
 	_AM33XX_MUXENTRY(UART1_CTSN, 0,
-		"uart1_ctsn", NULL, "d_can0_tx", NULL,
+		"uart1_ctsn", NULL, "d_can0_tx", "i2c2_sda",
 		"spi1_cs0", NULL, NULL, NULL),
 	_AM33XX_MUXENTRY(UART1_RTSN, 0,
-		"uart1_rtsn", NULL, "d_can0_rx", NULL,
+		"uart1_rtsn", NULL, "d_can0_rx", "i2c2_scl",
 		"spi1_cs1", NULL, NULL, NULL),
 	_AM33XX_MUXENTRY(UART1_RXD, 0,
 		"uart1_rxd", "mmc1_sdwp", "d_can1_tx", NULL,
-- 
1.7.2.5

