From f728b0620a6bf66fc78c59c23092c5eaea4a78b4 Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Sun, 10 Jul 2011 05:56:32 -0600
Subject: [PATCH 086/149] OMAP4: cm: Add two new APIs for modulemode control

In OMAP4, a new programming model based on module control instead
of clock control was introduced.
Expose two APIs to allow the upper layer (omap_hwmod) to control
the module mode independently of the parent clocks management.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: Rajendra Nayak <rnayak@ti.com>
[paul@pwsan.com: renamed 'omap4_cm_' fns to 'omap4_cminst_'; cleaned up
 kerneldoc]
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/cminst44xx.c |   40 ++++++++++++++++++++++++++++++++++++++
 arch/arm/mach-omap2/cminst44xx.h |    5 ++++
 2 files changed, 45 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/cminst44xx.c b/arch/arm/mach-omap2/cminst44xx.c
index 0fe3f14..eb2a472 100644
--- a/arch/arm/mach-omap2/cminst44xx.c
+++ b/arch/arm/mach-omap2/cminst44xx.c
@@ -309,3 +309,43 @@ int omap4_cminst_wait_module_idle(u8 part, u16 inst, s16 cdoffs, u16 clkctrl_off
 
 	return (i < MAX_MODULE_READY_TIME) ? 0 : -EBUSY;
 }
+
+/**
+ * omap4_cminst_module_enable - Enable the modulemode inside CLKCTRL
+ * @mode: Module mode (SW or HW)
+ * @part: PRCM partition ID that the CM_CLKCTRL register exists in
+ * @inst: CM instance register offset (*_INST macro)
+ * @cdoffs: Clockdomain register offset (*_CDOFFS macro)
+ * @clkctrl_offs: Module clock control register offset (*_CLKCTRL macro)
+ *
+ * No return value.
+ */
+void omap4_cminst_module_enable(u8 mode, u8 part, u16 inst, s16 cdoffs,
+			    u16 clkctrl_offs)
+{
+	u32 v;
+
+	v = omap4_cminst_read_inst_reg(part, inst, clkctrl_offs);
+	v &= ~OMAP4430_MODULEMODE_MASK;
+	v |= mode << OMAP4430_MODULEMODE_SHIFT;
+	omap4_cminst_write_inst_reg(v, part, inst, clkctrl_offs);
+}
+
+/**
+ * omap4_cminst_module_disable - Disable the module inside CLKCTRL
+ * @part: PRCM partition ID that the CM_CLKCTRL register exists in
+ * @inst: CM instance register offset (*_INST macro)
+ * @cdoffs: Clockdomain register offset (*_CDOFFS macro)
+ * @clkctrl_offs: Module clock control register offset (*_CLKCTRL macro)
+ *
+ * No return value.
+ */
+void omap4_cminst_module_disable(u8 part, u16 inst, s16 cdoffs,
+			     u16 clkctrl_offs)
+{
+	u32 v;
+
+	v = omap4_cminst_read_inst_reg(part, inst, clkctrl_offs);
+	v &= ~OMAP4430_MODULEMODE_MASK;
+	omap4_cminst_write_inst_reg(v, part, inst, clkctrl_offs);
+}
diff --git a/arch/arm/mach-omap2/cminst44xx.h b/arch/arm/mach-omap2/cminst44xx.h
index a985400..f2ea645 100644
--- a/arch/arm/mach-omap2/cminst44xx.h
+++ b/arch/arm/mach-omap2/cminst44xx.h
@@ -20,6 +20,11 @@ extern void omap4_cminst_clkdm_force_wakeup(u8 part, s16 inst, u16 cdoffs);
 extern int omap4_cminst_wait_module_ready(u8 part, u16 inst, s16 cdoffs, u16 clkctrl_offs);
 extern int omap4_cminst_wait_module_idle(u8 part, u16 inst, s16 cdoffs, u16 clkctrl_offs);
 
+extern void omap4_cminst_module_enable(u8 mode, u8 part, u16 inst, s16 cdoffs,
+				       u16 clkctrl_offs);
+extern void omap4_cminst_module_disable(u8 part, u16 inst, s16 cdoffs,
+					u16 clkctrl_offs);
+
 /*
  * In an ideal world, we would not export these low-level functions,
  * but this will probably take some time to fix properly
-- 
1.6.6.1

