From 9f31f599f847c7eab995d22a683c8b32aaa5be7f Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Fri, 25 Jun 2010 11:24:07 -0500
Subject: [PATCH 24/75] omap3beagle: camera: Change vaux4 to 1.8v

Both voltage sources seem to need 1.8v.

After this, sensor is detected :)

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 1e9a868..af9b818 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -446,8 +446,8 @@ static struct regulator_init_data beagle_vaux3 = {
 /* VAUX4 for CAM_2V8 */
 static struct regulator_init_data beagle_vaux4 = {
 	.constraints = {
-		.min_uV			= 2800000,
-		.max_uV			= 2800000,
+		.min_uV			= 1800000,
+		.max_uV			= 1800000,
 		.apply_uV		= true,
 		.valid_modes_mask	= REGULATOR_MODE_NORMAL
 					| REGULATOR_MODE_STANDBY,
-- 
1.6.6.1

