From 28416cdd539f217f902178b45f52f38ec41eb779 Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Fri, 1 Jul 2011 22:54:01 +0200
Subject: [PATCH 030/149] OMAP4: hwmod data: Add MSTANDBY_SMART_WKUP flag

Add the flag to every IPs that support it to allow the
framework to enable it instead of the SMART_STANDBY default
mode.
Without that, an IP with busmaster capability will not
be able to wakeup the interconnect at all.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/omap_hwmod_44xx_data.c |    9 +++++----
 1 files changed, 5 insertions(+), 4 deletions(-)

diff --git a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
index e1c69ff..8cbbfbf 100644
--- a/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_44xx_data.c
@@ -660,7 +660,8 @@ static struct omap_hwmod_class_sysconfig omap44xx_aess_sysc = {
 	.sysc_offs	= 0x0010,
 	.sysc_flags	= (SYSC_HAS_MIDLEMODE | SYSC_HAS_SIDLEMODE),
 	.idlemodes	= (SIDLE_FORCE | SIDLE_NO | SIDLE_SMART |
-			   MSTANDBY_FORCE | MSTANDBY_NO | MSTANDBY_SMART),
+			   MSTANDBY_FORCE | MSTANDBY_NO | MSTANDBY_SMART |
+			   MSTANDBY_SMART_WKUP),
 	.sysc_fields	= &omap_hwmod_sysc_type2,
 };
 
@@ -2044,7 +2045,7 @@ static struct omap_hwmod_class_sysconfig omap44xx_hsi_sysc = {
 			   SYSC_HAS_SOFTRESET | SYSS_HAS_RESET_STATUS),
 	.idlemodes	= (SIDLE_FORCE | SIDLE_NO | SIDLE_SMART |
 			   SIDLE_SMART_WKUP | MSTANDBY_FORCE | MSTANDBY_NO |
-			   MSTANDBY_SMART),
+			   MSTANDBY_SMART | MSTANDBY_SMART_WKUP),
 	.sysc_fields	= &omap_hwmod_sysc_type1,
 };
 
@@ -2446,7 +2447,7 @@ static struct omap_hwmod_class_sysconfig omap44xx_iss_sysc = {
 			   SYSC_HAS_SIDLEMODE | SYSC_HAS_SOFTRESET),
 	.idlemodes	= (SIDLE_FORCE | SIDLE_NO | SIDLE_SMART |
 			   SIDLE_SMART_WKUP | MSTANDBY_FORCE | MSTANDBY_NO |
-			   MSTANDBY_SMART),
+			   MSTANDBY_SMART | MSTANDBY_SMART_WKUP),
 	.sysc_fields	= &omap_hwmod_sysc_type2,
 };
 
@@ -3420,7 +3421,7 @@ static struct omap_hwmod_class_sysconfig omap44xx_mmc_sysc = {
 			   SYSC_HAS_SOFTRESET),
 	.idlemodes	= (SIDLE_FORCE | SIDLE_NO | SIDLE_SMART |
 			   SIDLE_SMART_WKUP | MSTANDBY_FORCE | MSTANDBY_NO |
-			   MSTANDBY_SMART),
+			   MSTANDBY_SMART | MSTANDBY_SMART_WKUP),
 	.sysc_fields	= &omap_hwmod_sysc_type2,
 };
 
-- 
1.6.6.1

