From 71886bfebaf13c74a55f11264096286a554e5a3d Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Thu, 13 May 2010 21:43:08 +0200
Subject: [PATCH 44/45] ARM: OMAP: beagle: every known beagle (except revB) uses 2 chipselects so don't use NULL for the second chipselect timings

---
 arch/arm/mach-omap2/board-omap3beagle.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index dd830b1..078e026 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -614,7 +614,7 @@ static void __init omap3_beagle_init_irq(void)
         if (cpu_is_omap3630())
         {
                 omap2_init_common_hw(mt46h32m32lf6_sdrc_params,
-                                        NULL,
+                                        mt46h32m32lf6_sdrc_params,
                                         _omap37x_mpu_rate_table,
                                         _omap37x_dsp_rate_table,
                                         _omap37x_l3_rate_table);
@@ -622,7 +622,7 @@ static void __init omap3_beagle_init_irq(void)
         else
         {
                 omap2_init_common_hw(mt46h32m32lf6_sdrc_params,
-                                        NULL,
+                                        mt46h32m32lf6_sdrc_params,
                                         _omap35x_mpu_rate_table,
                                         _omap35x_dsp_rate_table,
                                         _omap35x_l3_rate_table);
-- 
1.6.6.1

