From 949d2c98bb76cc321e5ef5a96a632d831e5953bf Mon Sep 17 00:00:00 2001
From: Manjunatha Halli <manjunatha_halli@ti.com>
Date: Tue, 11 Jan 2011 11:31:26 +0000
Subject: [PATCH 12/15] drivers:media:radio: wl128x: Kconfig & Makefile for wl128x driver

Signed-off-by: Manjunatha Halli <manjunatha_halli@ti.com>
Reviewed-by: Hans Verkuil <hverkuil@xs4all.nl>
---
 drivers/media/radio/wl128x/Kconfig  |   17 +++++++++++++++++
 drivers/media/radio/wl128x/Makefile |    6 ++++++
 2 files changed, 23 insertions(+), 0 deletions(-)
 create mode 100644 drivers/media/radio/wl128x/Kconfig
 create mode 100644 drivers/media/radio/wl128x/Makefile

diff --git a/drivers/media/radio/wl128x/Kconfig b/drivers/media/radio/wl128x/Kconfig
new file mode 100644
index 0000000..749f67b
--- /dev/null
+++ b/drivers/media/radio/wl128x/Kconfig
@@ -0,0 +1,17 @@
+#
+# TI's wl128x FM driver based on TI's ST driver.
+#
+menu "Texas Instruments WL128x FM driver (ST based)"
+config RADIO_WL128X
+	tristate "Texas Instruments WL128x FM Radio"
+	depends on VIDEO_V4L2 && RFKILL
+	select TI_ST
+	help
+	Choose Y here if you have this FM radio chip.
+
+	In order to control your radio card, you will need to use programs
+	that are compatible with the Video For Linux 2 API.  Information on
+	this API and pointers to "v4l2" programs may be found at
+	<file:Documentation/video4linux/API.html>.
+
+endmenu
diff --git a/drivers/media/radio/wl128x/Makefile b/drivers/media/radio/wl128x/Makefile
new file mode 100644
index 0000000..32a0ead
--- /dev/null
+++ b/drivers/media/radio/wl128x/Makefile
@@ -0,0 +1,6 @@
+#
+# Makefile for TI's shared transport driver based wl128x
+# FM radio.
+#
+obj-$(CONFIG_RADIO_WL128X)	+= fm_drv.o
+fm_drv-objs		:= fmdrv_common.o fmdrv_rx.o fmdrv_tx.o fmdrv_v4l2.o
-- 
1.6.6.1

