From b4c914578637d1d92b92842c50b02a98f2a7357d Mon Sep 17 00:00:00 2001
From: Saeed Bishara <saeed@marvell.com>
Date: Tue, 21 Dec 2010 16:53:39 +0200
Subject: [PATCH 48/65] mv_xor: fix race in tasklet function

use mv_xor_slot_cleanup() instead of __mv_xor_slot_cleanup() as the former function
aquires the spin lock that needed to protect the drivers data.

Cc: <stable@kernel.org>
Signed-off-by: Saeed Bishara <saeed@marvell.com>
Signed-off-by: Dan Williams <dan.j.williams@intel.com>
---
 drivers/dma/mv_xor.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/drivers/dma/mv_xor.c b/drivers/dma/mv_xor.c
index 411d5bf..a25f5f6 100644
--- a/drivers/dma/mv_xor.c
+++ b/drivers/dma/mv_xor.c
@@ -449,7 +449,7 @@ mv_xor_slot_cleanup(struct mv_xor_chan *mv_chan)
 static void mv_xor_tasklet(unsigned long data)
 {
 	struct mv_xor_chan *chan = (struct mv_xor_chan *) data;
-	__mv_xor_slot_cleanup(chan);
+	mv_xor_slot_cleanup(chan);
 }
 
 static struct mv_xor_desc_slot *
-- 
1.6.6.1

