From 34d88746a9aa4aedb67e32579e559cbeb91de20f Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Thu, 23 Sep 2010 18:22:48 -0700
Subject: [PATCH 02/10] omap: Beagle: only Cx boards use pin 23 for write protect

system_rev comes from u-boot and is a constant 0x20, so
Bx boards also fall in this 'if' and will get setup with the
wrong gpio_wp pin. Switch to using the Beagle revision routine
to correcly set pin 23 only for C1/2/3 and C4 Boards. Bx boards
will then use the correct default pin setting.

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
Acked-by: Jarkko Nikula <jhnikula@gmail.com>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    3 ++-
 1 files changed, 2 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 7ca2b3b..beb877c 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -444,7 +444,8 @@ static struct gpio_led gpio_leds[];
 static int beagle_twl_gpio_setup(struct device *dev,
 		unsigned gpio, unsigned ngpio)
 {
-	if (system_rev >= 0x20 && system_rev <= 0x34301000) {
+	if ((omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_C1_3) ||
+		(omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_C4)) {
 		omap_mux_init_gpio(23, OMAP_PIN_INPUT);
 		mmc[0].gpio_wp = 23;
 	} else {
-- 
1.6.6.1

