From e1dd1afba99853083da545f632a1f7c6899ae379 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@beagleboard.org>
Date: Tue, 11 Jan 2011 17:13:36 +0000
Subject: [PATCH 02/28] omap3: beaglexm: fix DVI reset GPIO

GPIO reset line for Beagle XM is different from vanilla beagle
so we populate it as part of gpio update routine.

This in part fixes the issue of display not functioning on beagle XM
platform.

[nm@ti.com: split up, added descriptive changelogs]
Signed-off-by: Nishanth Menon <nm@ti.com>
Signed-off-by: Koen Kooi <koen@beagleboard.org>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    8 +++++++-
 1 files changed, 7 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index af1166b..673deb9 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -199,7 +199,7 @@ static struct omap_dss_device beagle_dvi_device = {
 	.name = "dvi",
 	.driver_name = "generic_panel",
 	.phy.dpi.data_lines = 24,
-	.reset_gpio = 170,
+	.reset_gpio = -EINVAL,
 	.platform_enable = beagle_enable_dvi,
 	.platform_disable = beagle_disable_dvi,
 };
@@ -307,6 +307,12 @@ static int beagle_twl_gpio_setup(struct device *dev,
 	else
 		gpio_direction_output(gpio + TWL4030_GPIO_MAX, 0);
 
+	/* DVI reset GPIO is different between beagle revisions */
+	if (omap3_beagle_get_rev() == OMAP3BEAGLE_BOARD_XM)
+		beagle_dvi_device.reset_gpio = 129;
+	else
+		beagle_dvi_device.reset_gpio = 170;
+
 	/* TWL4030_GPIO_MAX + 1 == ledB, PMU_STAT (out, active low LED) */
 	gpio_leds[2].gpio = gpio + TWL4030_GPIO_MAX + 1;
 
-- 
1.6.6.1

