From 7d8868d73fdd95eb928f54f881978590643e50cc Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Thu, 31 Dec 2009 07:05:02 -0800
Subject: [PATCH 12/45] MTD: NAND: omap2: proper fix for subpage read ECC errors

---
 drivers/mtd/nand/omap2.c |   11 +++++++----
 1 files changed, 7 insertions(+), 4 deletions(-)

diff --git a/drivers/mtd/nand/omap2.c b/drivers/mtd/nand/omap2.c
index 08c193c..9b185b0 100644
--- a/drivers/mtd/nand/omap2.c
+++ b/drivers/mtd/nand/omap2.c
@@ -295,11 +295,14 @@ static void omap_read_buf_pref(struct mtd_info *mtd, u_char *buf, int len)
 	u32 *p = (u32 *)buf;
 
 	/* take care of subpage reads */
-	for (; len % 4 != 0; ) {
-		*buf++ = __raw_readb(info->nand.IO_ADDR_R);
-		len--;
+	if (len % 4) {
+		if (info->nand.options & NAND_BUSWIDTH_16)
+			omap_read_buf16(mtd, buf, len % 4);
+		else
+			omap_read_buf8(mtd, buf, len % 4);
+		p = (u32 *) (buf + len % 4);
+		len -= len % 4;
 	}
-	p = (u32 *) buf;
 
 	/* configure and start prefetch transfer */
 	ret = gpmc_prefetch_enable(info->gpmc_cs, 0x0, len, 0x0);
-- 
1.6.6.1

