From c3c9a3de412eeb394594b3a3394c01f24e59614b Mon Sep 17 00:00:00 2001
From: Milan Kocian <milon@wq.cz>
Date: Fri, 3 Feb 2012 14:28:00 +0100
Subject: [PATCH 80/87] USB: usbserial: add new PID number (0xa951) to the
 ftdi driver

commit 90451e6973a5da155c6f315a409ca0a8d3ce6b76 upstream.

Signed-off-by: Milan Kocian <milon@wq.cz>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/serial/ftdi_sio.c     |    1 +
 drivers/usb/serial/ftdi_sio_ids.h |    7 +++++++
 2 files changed, 8 insertions(+)

diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index 058b92c..f030471 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -839,6 +839,7 @@ static struct usb_device_id id_table_combined [] = {
 	{ USB_DEVICE(FTDI_VID, FTDI_SCIENCESCOPE_LOGBOOKML_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_SCIENCESCOPE_LS_LOGBOOK_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_SCIENCESCOPE_HS_LOGBOOK_PID) },
+	{ USB_DEVICE(FTDI_VID, FTDI_CINTERION_MC55I_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_DOTEC_PID) },
 	{ USB_DEVICE(QIHARDWARE_VID, MILKYMISTONE_JTAGSERIAL_PID),
 		.driver_info = (kernel_ulong_t)&ftdi_jtag_quirk },
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index 76d4f31..4eb7715 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -1187,3 +1187,10 @@
  */
 /* ZigBee controller */
 #define FTDI_RF_R106		0x8A28
+
+/*
+ * Product: HCP HIT GPRS modem
+ * Manufacturer: HCP d.o.o.
+ * ATI command output: Cinterion MC55i
+ */
+#define FTDI_CINTERION_MC55I_PID	0xA951
-- 
1.7.9.4

