From 8bfeb0bfde94ba70986c03d0a8ca9ab876073e35 Mon Sep 17 00:00:00 2001
From: Takashi Iwai <tiwai@suse.de>
Date: Wed, 18 Apr 2012 15:21:07 +0200
Subject: [PATCH 66/69] drm/radeon/kms: fix the regression of DVI connector
 check

commit e36325071832f1ba96ac54fb8ba1459f08b05dd8 upstream.

The check of the encoder type in the commit [e00e8b5e: drm/radeon/kms:
fix analog load detection on DVI-I connectors] is obviously wrong, and
it's the culprit of the regression on my workstation with DVI-analog
connection resulting in the blank output.

Fixed the typo now.

Signed-off-by: Takashi Iwai <tiwai@suse.de>
Reviewed-by: Alex Deucher <alexander.deucher@amd.com>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/radeon/radeon_connectors.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/gpu/drm/radeon/radeon_connectors.c b/drivers/gpu/drm/radeon/radeon_connectors.c
index f7d39ac..f19ea2e 100644
--- a/drivers/gpu/drm/radeon/radeon_connectors.c
+++ b/drivers/gpu/drm/radeon/radeon_connectors.c
@@ -946,7 +946,7 @@ radeon_dvi_detect(struct drm_connector *connector, bool force)
 
 			encoder = obj_to_encoder(obj);
 
-			if (encoder->encoder_type != DRM_MODE_ENCODER_DAC ||
+			if (encoder->encoder_type != DRM_MODE_ENCODER_DAC &&
 			    encoder->encoder_type != DRM_MODE_ENCODER_TVDAC)
 				continue;
 
-- 
1.7.9.5

