From 7845ad0aca7c2976dc4021ed0c080f6605aacf09 Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Sat, 9 Jul 2011 19:15:05 -0600
Subject: [PATCH 054/149] OMAP4: powerdomain data: Fix indentation
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Indent flags to be aligned with other fields.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: Rajendra Nayak <rnayak@ti.com>
Cc: Santosh Shilimkar <santosh.shilimkar@ti.com>
[paul@pwsan.com: split this patch from an earlier patch by Benoît;
 edited commit message]
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/powerdomains44xx_data.c |   18 +++++++++---------
 1 files changed, 9 insertions(+), 9 deletions(-)

diff --git a/arch/arm/mach-omap2/powerdomains44xx_data.c b/arch/arm/mach-omap2/powerdomains44xx_data.c
index c4222c7..3a7e678 100644
--- a/arch/arm/mach-omap2/powerdomains44xx_data.c
+++ b/arch/arm/mach-omap2/powerdomains44xx_data.c
@@ -53,7 +53,7 @@ static struct powerdomain core_44xx_pwrdm = {
 		[3] = PWRSTS_ON,	/* ducati_l2ram */
 		[4] = PWRSTS_ON,	/* ducati_unicache */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* gfx_44xx_pwrdm: 3D accelerator power domain */
@@ -70,7 +70,7 @@ static struct powerdomain gfx_44xx_pwrdm = {
 	.pwrsts_mem_on	= {
 		[0] = PWRSTS_ON,	/* gfx_mem */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* abe_44xx_pwrdm: Audio back end power domain */
@@ -90,7 +90,7 @@ static struct powerdomain abe_44xx_pwrdm = {
 		[0] = PWRSTS_ON,	/* aessmem */
 		[1] = PWRSTS_ON,	/* periphmem */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* dss_44xx_pwrdm: Display subsystem power domain */
@@ -108,7 +108,7 @@ static struct powerdomain dss_44xx_pwrdm = {
 	.pwrsts_mem_on	= {
 		[0] = PWRSTS_ON,	/* dss_mem */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* tesla_44xx_pwrdm: Tesla processor power domain */
@@ -130,7 +130,7 @@ static struct powerdomain tesla_44xx_pwrdm = {
 		[1] = PWRSTS_ON,	/* tesla_l1 */
 		[2] = PWRSTS_ON,	/* tesla_l2 */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* wkup_44xx_pwrdm: Wake-up power domain */
@@ -241,7 +241,7 @@ static struct powerdomain ivahd_44xx_pwrdm = {
 		[2] = PWRSTS_ON,	/* tcm1_mem */
 		[3] = PWRSTS_ON,	/* tcm2_mem */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* cam_44xx_pwrdm: Camera subsystem power domain */
@@ -258,7 +258,7 @@ static struct powerdomain cam_44xx_pwrdm = {
 	.pwrsts_mem_on	= {
 		[0] = PWRSTS_ON,	/* cam_mem */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* l3init_44xx_pwrdm: L3 initators pheripherals power domain  */
@@ -276,7 +276,7 @@ static struct powerdomain l3init_44xx_pwrdm = {
 	.pwrsts_mem_on	= {
 		[0] = PWRSTS_ON,	/* l3init_bank1 */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /* l4per_44xx_pwrdm: Target peripherals power domain */
@@ -296,7 +296,7 @@ static struct powerdomain l4per_44xx_pwrdm = {
 		[0] = PWRSTS_ON,	/* nonretained_bank */
 		[1] = PWRSTS_ON,	/* retained_bank */
 	},
-	.flags		= PWRDM_HAS_LOWPOWERSTATECHANGE,
+	.flags		  = PWRDM_HAS_LOWPOWERSTATECHANGE,
 };
 
 /*
-- 
1.7.2.5

