From 713c5b4ce910dacdd75e9616b0f989d643008536 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 19 Oct 2011 12:44:14 +0200
Subject: [PATCH 10/10] ARM: OMAP2+: beagleboard: fix mmc write protect pin when using the wilink expansion board

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 5ffe185..0124060 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -274,7 +274,7 @@ static struct omap2_hsmmc_info mmcbbt[] = {
  	{
  		.mmc		= 1,
  		.caps		= MMC_CAP_4_BIT_DATA | MMC_CAP_8_BIT_DATA,
- 		.gpio_wp	= 29,
+ 		.gpio_wp	= -EINVAL,
  	},
 	{
 		.name		= "wl1271",
-- 
1.7.2.5

