From 23d7e04b5d71feafdd920f4bf4b735cc452fef59 Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Sun, 24 Jan 2010 09:33:56 -0800
Subject: [PATCH 13/14] omap: mmc-twl4030: move clock input selection prior to vcc test

otherwise it is not executed on systems that use non-twl regulators
---
 arch/arm/mach-omap2/hsmmc.c |   14 ++++++--------
 1 files changed, 6 insertions(+), 8 deletions(-)

diff --git a/arch/arm/mach-omap2/hsmmc.c b/arch/arm/mach-omap2/hsmmc.c
index 66868c5..48a6cfb 100644
--- a/arch/arm/mach-omap2/hsmmc.c
+++ b/arch/arm/mach-omap2/hsmmc.c
@@ -192,15 +192,13 @@ static void hsmmc23_before_set_reg(struct device *dev, int slot,
 	if (mmc->slots[0].remux)
 		mmc->slots[0].remux(dev, slot, power_on);
 
-	if (power_on) {
-		/* Only MMC2 supports a CLKIN */
-		if (mmc->slots[0].internal_clock) {
-			u32 reg;
+	/* Only MMC2 supports a CLKIN */
+	if (mmc->slots[0].internal_clock) {
+		u32 reg;
 
-			reg = omap_ctrl_readl(control_devconf1_offset);
-			reg |= OMAP2_MMCSDIO2ADPCLKISEL;
-			omap_ctrl_writel(reg, control_devconf1_offset);
-		}
+		reg = omap_ctrl_readl(control_devconf1_offset);
+		reg |= OMAP2_MMCSDIO2ADPCLKISEL;
+		omap_ctrl_writel(reg, control_devconf1_offset);
 	}
 }
 
-- 
1.7.2.5

