From 42eb98a4b9dc721f8565ce0d3063db8d141f516b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Micha=C5=82=20Wr=C3=B3bel?= <michal.wrobel@flytronic.pl>
Date: Fri, 9 Mar 2012 14:40:18 +0100
Subject: [PATCH 009/147] USB: ftdi_sio: new PID: Distortec JTAG-lock-pick
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit 47594d5528f28a4c025c2955c68104c75815637c upstream.

Signed-off-by: Micha?? Wr??bel <michal.wrobel@flytronic.pl>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/serial/ftdi_sio.c     |    2 ++
 drivers/usb/serial/ftdi_sio_ids.h |    2 ++
 2 files changed, 4 insertions(+)

diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index 363e995..a319eaa 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -846,6 +846,8 @@ static struct usb_device_id id_table_combined [] = {
 	{ USB_DEVICE(ST_VID, ST_STMCLT1030_PID),
 		.driver_info = (kernel_ulong_t)&ftdi_stmclite_quirk },
 	{ USB_DEVICE(FTDI_VID, FTDI_RF_R106) },
+	{ USB_DEVICE(FTDI_VID, FTDI_DISTORTEC_JTAG_LOCK_PICK_PID),
+		.driver_info = (kernel_ulong_t)&ftdi_jtag_quirk },
 	{ },					/* Optional parameter entry */
 	{ }					/* Terminating entry */
 };
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index df87939..bed1b1f 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -97,6 +97,8 @@
 #define FTDI_TACTRIX_OPENPORT_13S_PID	0xCC49	/* OpenPort 1.3 Subaru */
 #define FTDI_TACTRIX_OPENPORT_13U_PID	0xCC4A	/* OpenPort 1.3 Universal */
 
+#define FTDI_DISTORTEC_JTAG_LOCK_PICK_PID	0xCFF8
+
 /* SCS HF Radio Modems PID's (http://www.scs-ptc.com) */
 /* the VID is the standard ftdi vid (FTDI_VID) */
 #define FTDI_SCS_DEVICE_0_PID 0xD010    /* SCS PTC-IIusb */
-- 
1.7.9.4

