From 2ade67b1a3c53567ea131902c3631f7d57b4332f Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Tue, 17 Apr 2012 12:35:01 +0200
Subject: [PATCH 28/29] beaglebone: fix ehrpwm backlight

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index b0ee67e..0d20bb1 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -1434,6 +1434,7 @@ late_initcall(ecap0_init);
 static void enable_ehrpwm1(int evm_id, int profile)
 {
 	ehrpwm_backlight_enable = true;
+	am33xx_register_ehrpwm(1, &pwm_pdata[1]);
 }
 
 /* Setup pwm-backlight for bbtoys7lcd */
-- 
1.7.7.6

