From 40fe12a7ee76b320a7662d8da492c80743deaa1b Mon Sep 17 00:00:00 2001
From: Andiry Xu <andiry.xu@amd.com>
Date: Wed, 4 Jan 2012 15:18:27 +0800
Subject: [PATCH 58/90] usb: gadget: storage: endian fix

commit a85016390135d577c457876d0e905095600751de upstream.

Fix some endian issues for storage gadgets.

Signed-off-by: Andiry Xu <andiry.xu@amd.com>
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/gadget/storage_common.c |    6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/drivers/usb/gadget/storage_common.c b/drivers/usb/gadget/storage_common.c
index c7f291a..85ea14e 100644
--- a/drivers/usb/gadget/storage_common.c
+++ b/drivers/usb/gadget/storage_common.c
@@ -598,16 +598,16 @@ static __maybe_unused struct usb_ss_cap_descriptor fsg_ss_cap_desc = {
 		| USB_5GBPS_OPERATION),
 	.bFunctionalitySupport = USB_LOW_SPEED_OPERATION,
 	.bU1devExitLat =	USB_DEFAULT_U1_DEV_EXIT_LAT,
-	.bU2DevExitLat =	USB_DEFAULT_U2_DEV_EXIT_LAT,
+	.bU2DevExitLat =	cpu_to_le16(USB_DEFAULT_U2_DEV_EXIT_LAT),
 };
 
 static __maybe_unused struct usb_bos_descriptor fsg_bos_desc = {
 	.bLength =		USB_DT_BOS_SIZE,
 	.bDescriptorType =	USB_DT_BOS,
 
-	.wTotalLength =		USB_DT_BOS_SIZE
+	.wTotalLength =		cpu_to_le16(USB_DT_BOS_SIZE
 				+ USB_DT_USB_EXT_CAP_SIZE
-				+ USB_DT_USB_SS_CAP_SIZE,
+				+ USB_DT_USB_SS_CAP_SIZE),
 
 	.bNumDeviceCaps =	2,
 };
-- 
1.7.9.4

