From ca13fa5f840198db430a21a643f3df4788f21b85 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Tue, 31 Jan 2012 10:09:06 +0100
Subject: [PATCH 05/26] beaglebone: disable tsadc

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-am335xevm.c |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/board-am335xevm.c b/arch/arm/mach-omap2/board-am335xevm.c
index 3c67e94..b0f5ce3 100644
--- a/arch/arm/mach-omap2/board-am335xevm.c
+++ b/arch/arm/mach-omap2/board-am335xevm.c
@@ -240,11 +240,11 @@ struct da8xx_lcdc_platform_data dvi_pdata = {
 static struct tsc_data am335x_touchscreen_data  = {
 	.wires  = 4,
 	.x_plate_resistance = 200,
-	.mode = TI_TSCADC_TSCMODE,
+//	.mode = TI_TSCADC_TSCMODE,
 };
 
 static struct tsc_data bone_touchscreen_data  = {
-	.mode = TI_TSCADC_GENMODE,
+//	.mode = TI_TSCADC_GENMODE,
 };
 
 static u8 am335x_iis_serializer_direction1[] = {
-- 
1.7.9.5

