From d4e6ce02459552a127973c9c204509136b940671 Mon Sep 17 00:00:00 2001
From: Sarah Sharp <sarah.a.sharp@linux.intel.com>
Date: Fri, 16 Mar 2012 13:19:35 -0700
Subject: [PATCH 46/69] xhci: Fix register save/restore order.

commit c7713e736526d8c9f6f87716fb90562a8ffaff2c upstream.

The xHCI 1.0 spec errata released on June 13, 2011, changes the ordering
that the xHCI registers are saved and restored in.  It moves the
interrupt pending (IMAN) and interrupt control (IMOD) registers to be
saved and restored last.  I believe that's because the host controller
may attempt to fetch the event ring table when interrupts are
re-enabled.  Therefore we need to restore the event ring registers
before we re-enable interrupts.

This should be backported to kernels as old as 2.6.37, that contain the
commit 5535b1d5f8885695c6ded783c692e3c0d0eda8ca "USB: xHCI: PCI power
management implementation"

Signed-off-by: Sarah Sharp <sarah.a.sharp@linux.intel.com>
Tested-by: Elric Fu <elricfu1@gmail.com>
Cc: Andiry Xu <andiry.xu@amd.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/xhci.c |    8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index 4d44713..4c00606 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -664,11 +664,11 @@ static void xhci_save_registers(struct xhci_hcd *xhci)
 	xhci->s3.dev_nt = xhci_readl(xhci, &xhci->op_regs->dev_notification);
 	xhci->s3.dcbaa_ptr = xhci_read_64(xhci, &xhci->op_regs->dcbaa_ptr);
 	xhci->s3.config_reg = xhci_readl(xhci, &xhci->op_regs->config_reg);
-	xhci->s3.irq_pending = xhci_readl(xhci, &xhci->ir_set->irq_pending);
-	xhci->s3.irq_control = xhci_readl(xhci, &xhci->ir_set->irq_control);
 	xhci->s3.erst_size = xhci_readl(xhci, &xhci->ir_set->erst_size);
 	xhci->s3.erst_base = xhci_read_64(xhci, &xhci->ir_set->erst_base);
 	xhci->s3.erst_dequeue = xhci_read_64(xhci, &xhci->ir_set->erst_dequeue);
+	xhci->s3.irq_pending = xhci_readl(xhci, &xhci->ir_set->irq_pending);
+	xhci->s3.irq_control = xhci_readl(xhci, &xhci->ir_set->irq_control);
 }
 
 static void xhci_restore_registers(struct xhci_hcd *xhci)
@@ -677,11 +677,11 @@ static void xhci_restore_registers(struct xhci_hcd *xhci)
 	xhci_writel(xhci, xhci->s3.dev_nt, &xhci->op_regs->dev_notification);
 	xhci_write_64(xhci, xhci->s3.dcbaa_ptr, &xhci->op_regs->dcbaa_ptr);
 	xhci_writel(xhci, xhci->s3.config_reg, &xhci->op_regs->config_reg);
-	xhci_writel(xhci, xhci->s3.irq_pending, &xhci->ir_set->irq_pending);
-	xhci_writel(xhci, xhci->s3.irq_control, &xhci->ir_set->irq_control);
 	xhci_writel(xhci, xhci->s3.erst_size, &xhci->ir_set->erst_size);
 	xhci_write_64(xhci, xhci->s3.erst_base, &xhci->ir_set->erst_base);
 	xhci_write_64(xhci, xhci->s3.erst_dequeue, &xhci->ir_set->erst_dequeue);
+	xhci_writel(xhci, xhci->s3.irq_pending, &xhci->ir_set->irq_pending);
+	xhci_writel(xhci, xhci->s3.irq_control, &xhci->ir_set->irq_control);
 }
 
 static void xhci_set_cmd_ring_deq(struct xhci_hcd *xhci)
-- 
1.7.9.5

