From 9318b0759a699e6128817bead791603201e73d99 Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Thu, 29 Sep 2011 11:36:22 -0500
Subject: [PATCH 03/14] ksz8851 read_mac_addr

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
---
 drivers/net/ethernet/micrel/ks8851.c |   44 ++++++++++++++++++++++++++++-----
 1 files changed, 37 insertions(+), 7 deletions(-)

diff --git a/drivers/net/ethernet/micrel/ks8851.c b/drivers/net/ethernet/micrel/ks8851.c
index f56743a..da7cbea 100644
--- a/drivers/net/ethernet/micrel/ks8851.c
+++ b/drivers/net/ethernet/micrel/ks8851.c
@@ -367,21 +367,47 @@ static int ks8851_write_mac_addr(struct net_device *dev)
 }
 
 /**
+ * ks8851_read_mac_addr - read mac address from device registers
+ * @dev: The network device
+ *
+ * Update our copy of the KS8851 MAC address from the registers of @dev.
+*/
+static void ks8851_read_mac_addr(struct net_device *dev)
+{
+	struct ks8851_net *ks = netdev_priv(dev);
+	int i;
+
+	mutex_lock(&ks->lock);
+
+	for (i = 0; i < ETH_ALEN; i++)
+		dev->dev_addr[i] = ks8851_rdreg8(ks, KS_MAR(i));
+
+	mutex_unlock(&ks->lock);
+}
+
+/**
  * ks8851_init_mac - initialise the mac address
  * @ks: The device structure
  *
  * Get or create the initial mac address for the device and then set that
- * into the station address register. Currently we assume that the device
- * does not have a valid mac address in it, and so we use random_ether_addr()
+ * into the station address register. If there is an EEPROM present, then
+ * we try that. If no valid mac address is found we use random_ether_addr()
  * to create a new one.
- *
- * In future, the driver should check to see if the device has an EEPROM
- * attached and whether that has a valid ethernet address in it.
  */
 static void ks8851_init_mac(struct ks8851_net *ks)
 {
 	struct net_device *dev = ks->netdev;
 
+	/* first, try reading what we've got already */
+	if (ks->rc_ccr & CCR_EEPROM) {
+		ks8851_read_mac_addr(dev);
+		if (is_valid_ether_addr(dev->dev_addr))
+			return;
+
+		netdev_err(ks->netdev, "invalid mac address read %pM\n",
+			dev->dev_addr);
+	}
+
 	random_ether_addr(dev->dev_addr);
 	ks8851_write_mac_addr(dev);
 }
@@ -1658,6 +1684,9 @@ static int __devinit ks8851_probe(struct spi_device *spi)
 	else
 		ks->eeprom_size = 0;
 
+	/* cache the contents of the CCR register for EEPROM, etc. */
+	ks->rc_ccr = ks8851_rdreg16(ks, KS_CCR);
+
 	ks8851_read_selftest(ks);
 	ks8851_init_mac(ks);
 
@@ -1674,9 +1703,10 @@ static int __devinit ks8851_probe(struct spi_device *spi)
 		goto err_netdev;
 	}
 
-	netdev_info(ndev, "revision %d, MAC %pM, IRQ %d\n",
+	netdev_info(ndev, "revision %d, MAC %pM, IRQ %d %s EEPROM\n",
 		    CIDER_REV_GET(ks8851_rdreg16(ks, KS_CIDER)),
-		    ndev->dev_addr, ndev->irq);
+		    ndev->dev_addr, ndev->irq,
+		    ks->rc_ccr & CCR_EEPROM ? "has" : "no");
 
 	return 0;
 
-- 
1.7.7.4

