From 5efedf1eea47c18e516e55bbfb417e447e76fc0d Mon Sep 17 00:00:00 2001
From: Alex Deucher <alexander.deucher@amd.com>
Date: Fri, 16 Mar 2012 12:22:10 -0400
Subject: [PATCH 073/147] drm/radeon/kms: add connector quirk for Fujitsu
 D3003-S2 board

commit 4c1b2d2da3451f5c8dd59bd7e05bd9729d2aee05 upstream.

vbios lists DVI-I port as VGA and DVI-D.

Fixes:
https://bugs.freedesktop.org/show_bug.cgi?id=47007

Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/radeon/radeon_atombios.c |   14 ++++++++++++++
 1 file changed, 14 insertions(+)

diff --git a/drivers/gpu/drm/radeon/radeon_atombios.c b/drivers/gpu/drm/radeon/radeon_atombios.c
index 5082d17..8e1532f 100644
--- a/drivers/gpu/drm/radeon/radeon_atombios.c
+++ b/drivers/gpu/drm/radeon/radeon_atombios.c
@@ -442,6 +442,20 @@ static bool radeon_atom_apply_quirks(struct drm_device *dev,
 		struct radeon_device *rdev = dev->dev_private;
 		*i2c_bus = radeon_lookup_i2c_gpio(rdev, 0x93);
 	}
+
+	/* Fujitsu D3003-S2 board lists DVI-I as DVI-D and VGA */
+	if ((dev->pdev->device == 0x9802) &&
+	    (dev->pdev->subsystem_vendor == 0x1734) &&
+	    (dev->pdev->subsystem_device == 0x11bd)) {
+		if (*connector_type == DRM_MODE_CONNECTOR_VGA) {
+			*connector_type = DRM_MODE_CONNECTOR_DVII;
+			*line_mux = 0x3103;
+		} else if (*connector_type == DRM_MODE_CONNECTOR_DVID) {
+			*connector_type = DRM_MODE_CONNECTOR_DVII;
+		}
+	}
+
+
 	return true;
 }
 
-- 
1.7.9.4

