From 40cfa9924ed2f94482607fc884f1acb414d492b9 Mon Sep 17 00:00:00 2001
From: Shreyas Bhatewara <sbhatewara@vmware.com>
Date: Tue, 28 Feb 2012 22:17:38 +0000
Subject: [PATCH 20/42] vmxnet3: Fix transport header size

[ Upstream commit efead8710aad9e384730ecf25eae0287878840d7 ]

Fix transport header size

Fix the transpoert header size for UDP packets.

Signed-off-by: Shreyas N Bhatewara <sbhatewara@vmware.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/vmxnet3/vmxnet3_drv.c |    7 +------
 drivers/net/vmxnet3/vmxnet3_int.h |    4 ++--
 2 files changed, 3 insertions(+), 8 deletions(-)

diff --git a/drivers/net/vmxnet3/vmxnet3_drv.c b/drivers/net/vmxnet3/vmxnet3_drv.c
index d96bfb1..d426261 100644
--- a/drivers/net/vmxnet3/vmxnet3_drv.c
+++ b/drivers/net/vmxnet3/vmxnet3_drv.c
@@ -830,13 +830,8 @@ vmxnet3_parse_and_copy_hdr(struct sk_buff *skb, struct vmxnet3_tx_queue *tq,
 					ctx->l4_hdr_size = ((struct tcphdr *)
 					   skb_transport_header(skb))->doff * 4;
 				else if (iph->protocol == IPPROTO_UDP)
-					/*
-					 * Use tcp header size so that bytes to
-					 * be copied are more than required by
-					 * the device.
-					 */
 					ctx->l4_hdr_size =
-							sizeof(struct tcphdr);
+							sizeof(struct udphdr);
 				else
 					ctx->l4_hdr_size = 0;
 			} else {
diff --git a/drivers/net/vmxnet3/vmxnet3_int.h b/drivers/net/vmxnet3/vmxnet3_int.h
index b18eac1..8df921b 100644
--- a/drivers/net/vmxnet3/vmxnet3_int.h
+++ b/drivers/net/vmxnet3/vmxnet3_int.h
@@ -70,10 +70,10 @@
 /*
  * Version numbers
  */
-#define VMXNET3_DRIVER_VERSION_STRING   "1.1.18.0-k"
+#define VMXNET3_DRIVER_VERSION_STRING   "1.1.29.0-k"
 
 /* a 32-bit int, each byte encode a verion number in VMXNET3_DRIVER_VERSION */
-#define VMXNET3_DRIVER_VERSION_NUM      0x01011200
+#define VMXNET3_DRIVER_VERSION_NUM      0x01011D00
 
 #if defined(CONFIG_PCI_MSI)
 	/* RSS only makes sense if MSI-X is supported. */
-- 
1.7.9.4

