From b76642c53d6bad73ed8e4a8e7634ff7f7c366e43 Mon Sep 17 00:00:00 2001
From: Mark Brown <broonie@opensource.wolfsonmicro.com>
Date: Sat, 21 Jan 2012 21:48:53 +0000
Subject: [PATCH 16/90] ASoC: wm8996: Call _POST_PMU callback for CPVDD

commit a14304edcd5e8323205db34b08f709feb5357e64 upstream.

We should be allowing a 5ms delay after the charge pump is started in
order to ensure it has finished ramping.

Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/codecs/wm8996.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/sound/soc/codecs/wm8996.c b/sound/soc/codecs/wm8996.c
index e2afc05..6d98a57 100644
--- a/sound/soc/codecs/wm8996.c
+++ b/sound/soc/codecs/wm8996.c
@@ -1049,7 +1049,8 @@ SND_SOC_DAPM_SUPPLY_S("SYSCLK", 1, WM8996_AIF_CLOCKING_1, 0, 0, NULL, 0),
 SND_SOC_DAPM_SUPPLY_S("SYSDSPCLK", 2, WM8996_CLOCKING_1, 1, 0, NULL, 0),
 SND_SOC_DAPM_SUPPLY_S("AIFCLK", 2, WM8996_CLOCKING_1, 2, 0, NULL, 0),
 SND_SOC_DAPM_SUPPLY_S("Charge Pump", 2, WM8996_CHARGE_PUMP_1, 15, 0, cp_event,
-		      SND_SOC_DAPM_PRE_PMU | SND_SOC_DAPM_POST_PMD),
+		      SND_SOC_DAPM_PRE_PMU | SND_SOC_DAPM_POST_PMU |
+		      SND_SOC_DAPM_POST_PMD),
 SND_SOC_DAPM_SUPPLY("Bandgap", SND_SOC_NOPM, 0, 0, bg_event,
 		    SND_SOC_DAPM_PRE_PMU | SND_SOC_DAPM_POST_PMD),
 SND_SOC_DAPM_SUPPLY("LDO2", WM8996_POWER_MANAGEMENT_2, 1, 0, NULL, 0),
-- 
1.7.9.4

