From cf0a0312929eb18f55e95db15f2129fd28a0adb3 Mon Sep 17 00:00:00 2001
From: "Cho, Yu-Chen" <acho@suse.com>
Date: Wed, 14 Mar 2012 22:01:21 +0200
Subject: [PATCH 63/69] Bluetooth: Add Atheros maryann PIDVID support

commit 07c0ea874d43c299d185948452945a361052b6e3 upstream.

Add Atheros maryann 0cf3:311d PIDVID support
This module is AR3012 Series.

Include /sys/kernel/debug/usb/devices output here for reference

before:
T:  Bus=04 Lev=01 Prnt=01 Port=01 Cnt=01 Dev#=  2 Spd=12   MxCh= 0
D:  Ver= 1.10 Cls=e0(wlcon) Sub=01 Prot=01 MxPS=64 #Cfgs=  1
P:  Vendor=0cf3 ProdID=311d Rev= 0.01
S:  Manufacturer=Atheros Communications
S:  Product=Bluetooth USB Host Controller
S:  SerialNumber=Alaska Day 2006
C:* #Ifs= 2 Cfg#= 1 Atr=e0 MxPwr=100mA
I:* If#= 0 Alt= 0 #EPs= 3 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=81(I) Atr=03(Int.) MxPS=  16 Ivl=1ms
E:  Ad=82(I) Atr=02(Bulk) MxPS=  64 Ivl=0ms
E:  Ad=02(O) Atr=02(Bulk) MxPS=  64 Ivl=0ms
I:* If#= 1 Alt= 0 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=   0 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=   0 Ivl=1ms
I:  If#= 1 Alt= 1 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=   9 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=   9 Ivl=1ms
I:  If#= 1 Alt= 2 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  17 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  17 Ivl=1ms
I:  If#= 1 Alt= 3 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  25 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  25 Ivl=1ms
I:  If#= 1 Alt= 4 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  33 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  33 Ivl=1ms
I:  If#= 1 Alt= 5 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  49 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  49 Ivl=1ms

after:
T:  Bus=04 Lev=01 Prnt=01 Port=01 Cnt=01 Dev#=  2 Spd=12   MxCh= 0
D:  Ver= 1.10 Cls=e0(wlcon) Sub=01 Prot=01 MxPS=64 #Cfgs=  1
P:  Vendor=0cf3 ProdID=311d Rev= 0.02
S:  Manufacturer=Atheros Communications
S:  Product=Bluetooth USB Host Controller
S:  SerialNumber=Alaska Day 2006
C:* #Ifs= 2 Cfg#= 1 Atr=e0 MxPwr=100mA
I:* If#= 0 Alt= 0 #EPs= 3 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=81(I) Atr=03(Int.) MxPS=  16 Ivl=1ms
E:  Ad=82(I) Atr=02(Bulk) MxPS=  64 Ivl=0ms
E:  Ad=02(O) Atr=02(Bulk) MxPS=  64 Ivl=0ms
I:* If#= 1 Alt= 0 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=   0 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=   0 Ivl=1ms
I:  If#= 1 Alt= 1 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=   9 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=   9 Ivl=1ms
I:  If#= 1 Alt= 2 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  17 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  17 Ivl=1ms
I:  If#= 1 Alt= 3 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  25 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  25 Ivl=1ms
I:  If#= 1 Alt= 4 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  33 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  33 Ivl=1ms
I:  If#= 1 Alt= 5 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
E:  Ad=83(I) Atr=01(Isoc) MxPS=  49 Ivl=1ms
E:  Ad=03(O) Atr=01(Isoc) MxPS=  49 Ivl=1ms

Signed-off-by: Cho, Yu-Chen <acho@suse.com>
cked-by: Marcel Holtmann <marcel@holtmann.org>
Signed-off-by: Johan Hedberg <johan.hedberg@intel.com>
Cc: Jonathan Nieder <jrnieder@gmail.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/bluetooth/ath3k.c |    2 ++
 drivers/bluetooth/btusb.c |    1 +
 2 files changed, 3 insertions(+)

diff --git a/drivers/bluetooth/ath3k.c b/drivers/bluetooth/ath3k.c
index 67a79b0..003cd8d 100644
--- a/drivers/bluetooth/ath3k.c
+++ b/drivers/bluetooth/ath3k.c
@@ -71,6 +71,7 @@ static struct usb_device_id ath3k_table[] = {
 
 	/* Atheros AR3012 with sflash firmware*/
 	{ USB_DEVICE(0x0CF3, 0x3004) },
+	{ USB_DEVICE(0x0CF3, 0x311D) },
 	{ USB_DEVICE(0x13d3, 0x3375) },
 
 	/* Atheros AR5BBU12 with sflash firmware */
@@ -88,6 +89,7 @@ static struct usb_device_id ath3k_blist_tbl[] = {
 
 	/* Atheros AR3012 with sflash firmware*/
 	{ USB_DEVICE(0x0cf3, 0x3004), .driver_info = BTUSB_ATH3012 },
+	{ USB_DEVICE(0x0cf3, 0x311D), .driver_info = BTUSB_ATH3012 },
 	{ USB_DEVICE(0x13d3, 0x3375), .driver_info = BTUSB_ATH3012 },
 
 	{ }	/* Terminating entry */
diff --git a/drivers/bluetooth/btusb.c b/drivers/bluetooth/btusb.c
index df0331a..5a87b2e 100644
--- a/drivers/bluetooth/btusb.c
+++ b/drivers/bluetooth/btusb.c
@@ -126,6 +126,7 @@ static struct usb_device_id blacklist_table[] = {
 
 	/* Atheros 3012 with sflash firmware */
 	{ USB_DEVICE(0x0cf3, 0x3004), .driver_info = BTUSB_ATH3012 },
+	{ USB_DEVICE(0x0cf3, 0x311d), .driver_info = BTUSB_ATH3012 },
 	{ USB_DEVICE(0x13d3, 0x3375), .driver_info = BTUSB_ATH3012 },
 
 	/* Atheros AR5BBU12 with sflash firmware */
-- 
1.7.9.5

