From 27c26386a0152b7d0c2b4f173bcbe30805f42749 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Thu, 3 Nov 2011 17:35:50 +0100
Subject: [PATCH 4/4] da8xx-fb: add DVI support for beaglebone

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 drivers/video/da8xx-fb.c |   14 ++++++++++++++
 1 files changed, 14 insertions(+), 0 deletions(-)

diff --git a/drivers/video/da8xx-fb.c b/drivers/video/da8xx-fb.c
index 4347421..9619518 100644
--- a/drivers/video/da8xx-fb.c
+++ b/drivers/video/da8xx-fb.c
@@ -266,6 +266,20 @@ static struct da8xx_panel known_lcd_panels[] = {
 		.pxl_clk = 30000000,
 		.invert_pxl_clk = 0,
 	},
+	[3] = {
+		 /* 1024 x 768 @ 60 Hz  Reduced blanking VESA CVT 0.79M3-R */ 
+		.name = "1024x768@60",
+		.width = 1024,
+		.height = 768,
+		.hfp = 48,
+		.hbp = 80,
+		.hsw = 32,
+		.vfp = 3,
+		.vbp = 15,
+		.vsw = 4,
+		.pxl_clk = 56000000,
+		.invert_pxl_clk = 0,
+	},
 };
 
 /* Enable the Raster Engine of the LCD Controller */
-- 
1.7.2.5

