From a2139a0efb9472a649465a1080799c73470fd201 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Wed, 25 Jan 2012 15:48:36 +0100
Subject: [PATCH] beagleboard: reinstate usage of hi-speed PLL divider

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    5 +++++
 1 files changed, 5 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 016d0985..c4c7a99 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -467,6 +467,11 @@ static struct omap_dss_device beagle_dvi_device = {
 	.driver_name = "generic_dpi_panel",
 	.data = &dvi_panel,
 	.phy.dpi.data_lines = 24,
+	.clocks = {
+		.dispc = {
+			.dispc_fclk_src = OMAP_DSS_CLK_SRC_DSI_PLL_HSDIV_DISPC,
+		},
+	},
 	.reset_gpio = -EINVAL,
 };
 
-- 
1.7.7.5

