From c3d2a211cfeec3d0af0a26603c66e10dd456dd36 Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Thu, 29 Sep 2011 11:37:48 -0500
Subject: [PATCH 06/14] ksz8851 move to header

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
---
 drivers/net/ethernet/micrel/ks8851_mll.c |  263 +-----------------------------
 1 files changed, 5 insertions(+), 258 deletions(-)

diff --git a/drivers/net/ethernet/micrel/ks8851_mll.c b/drivers/net/ethernet/micrel/ks8851_mll.c
index d19c849..530b962 100644
--- a/drivers/net/ethernet/micrel/ks8851_mll.c
+++ b/drivers/net/ethernet/micrel/ks8851_mll.c
@@ -37,6 +37,8 @@
 #include <linux/slab.h>
 #include <asm/io.h>
 
+#include "ks8851.h"
+
 #define	DRV_NAME	"ks8851_mll"
 
 static u8 KS_DEFAULT_MAC_ADDRESS[] = { 0x00, 0x10, 0xA1, 0x86, 0x95, 0x11 };
@@ -45,165 +47,26 @@ static u8 KS_DEFAULT_MAC_ADDRESS[] = { 0x00, 0x10, 0xA1, 0x86, 0x95, 0x11 };
 #define TX_BUF_SIZE			2000
 #define RX_BUF_SIZE			2000
 
-#define KS_CCR				0x08
-#define CCR_EEPROM			(1 << 9)
-#define CCR_SPI				(1 << 8)
 #define CCR_8BIT			(1 << 7)
 #define CCR_16BIT			(1 << 6)
 #define CCR_32BIT			(1 << 5)
 #define CCR_SHARED			(1 << 4)
-#define CCR_32PIN			(1 << 0)
-
-/* MAC address registers */
-#define KS_MARL				0x10
-#define KS_MARM				0x12
-#define KS_MARH				0x14
 
-#define KS_OBCR				0x20
 #define OBCR_ODS_16MA			(1 << 6)
 
-#define KS_EEPCR			0x22
-#define EEPCR_EESA			(1 << 4)
-#define EEPCR_EESB			(1 << 3)
-#define EEPCR_EEDO			(1 << 2)
-#define EEPCR_EESCK			(1 << 1)
-#define EEPCR_EECS			(1 << 0)
-
-#define KS_MBIR				0x24
-#define MBIR_TXMBF			(1 << 12)
-#define MBIR_TXMBFA			(1 << 11)
-#define MBIR_RXMBF			(1 << 4)
-#define MBIR_RXMBFA			(1 << 3)
-
-#define KS_GRR				0x26
-#define GRR_QMU				(1 << 1)
-#define GRR_GSR				(1 << 0)
-
-#define KS_WFCR				0x2A
-#define WFCR_MPRXE			(1 << 7)
-#define WFCR_WF3E			(1 << 3)
-#define WFCR_WF2E			(1 << 2)
-#define WFCR_WF1E			(1 << 1)
-#define WFCR_WF0E			(1 << 0)
-
-#define KS_WF0CRC0			0x30
-#define KS_WF0CRC1			0x32
-#define KS_WF0BM0			0x34
-#define KS_WF0BM1			0x36
-#define KS_WF0BM2			0x38
-#define KS_WF0BM3			0x3A
-
-#define KS_WF1CRC0			0x40
-#define KS_WF1CRC1			0x42
-#define KS_WF1BM0			0x44
-#define KS_WF1BM1			0x46
-#define KS_WF1BM2			0x48
-#define KS_WF1BM3			0x4A
-
-#define KS_WF2CRC0			0x50
-#define KS_WF2CRC1			0x52
-#define KS_WF2BM0			0x54
-#define KS_WF2BM1			0x56
-#define KS_WF2BM2			0x58
-#define KS_WF2BM3			0x5A
-
-#define KS_WF3CRC0			0x60
-#define KS_WF3CRC1			0x62
-#define KS_WF3BM0			0x64
-#define KS_WF3BM1			0x66
-#define KS_WF3BM2			0x68
-#define KS_WF3BM3			0x6A
-
-#define KS_TXCR				0x70
-#define TXCR_TCGICMP			(1 << 8)
-#define TXCR_TCGUDP			(1 << 7)
-#define TXCR_TCGTCP			(1 << 6)
-#define TXCR_TCGIP			(1 << 5)
-#define TXCR_FTXQ			(1 << 4)
-#define TXCR_TXFCE			(1 << 3)
-#define TXCR_TXPE			(1 << 2)
-#define TXCR_TXCRC			(1 << 1)
-#define TXCR_TXE			(1 << 0)
-
-#define KS_TXSR				0x72
-#define TXSR_TXLC			(1 << 13)
-#define TXSR_TXMC			(1 << 12)
-#define TXSR_TXFID_MASK			(0x3f << 0)
-#define TXSR_TXFID_SHIFT		(0)
-#define TXSR_TXFID_GET(_v)		(((_v) >> 0) & 0x3f)
-
-
-#define KS_RXCR1			0x74
-#define RXCR1_FRXQ			(1 << 15)
-#define RXCR1_RXUDPFCC			(1 << 14)
-#define RXCR1_RXTCPFCC			(1 << 13)
-#define RXCR1_RXIPFCC			(1 << 12)
-#define RXCR1_RXPAFMA			(1 << 11)
-#define RXCR1_RXFCE			(1 << 10)
-#define RXCR1_RXEFE			(1 << 9)
-#define RXCR1_RXMAFMA			(1 << 8)
-#define RXCR1_RXBE			(1 << 7)
-#define RXCR1_RXME			(1 << 6)
-#define RXCR1_RXUE			(1 << 5)
-#define RXCR1_RXAE			(1 << 4)
-#define RXCR1_RXINVF			(1 << 1)
-#define RXCR1_RXE			(1 << 0)
 #define RXCR1_FILTER_MASK    		(RXCR1_RXINVF | RXCR1_RXAE | \
 					 RXCR1_RXMAFMA | RXCR1_RXPAFMA)
 
-#define KS_RXCR2			0x76
-#define RXCR2_SRDBL_MASK		(0x7 << 5)
-#define RXCR2_SRDBL_SHIFT		(5)
-#define RXCR2_SRDBL_4B			(0x0 << 5)
-#define RXCR2_SRDBL_8B			(0x1 << 5)
-#define RXCR2_SRDBL_16B			(0x2 << 5)
-#define RXCR2_SRDBL_32B			(0x3 << 5)
-/* #define RXCR2_SRDBL_FRAME		(0x4 << 5) */
-#define RXCR2_IUFFP			(1 << 4)
-#define RXCR2_RXIUFCEZ			(1 << 3)
-#define RXCR2_UDPLFE			(1 << 2)
-#define RXCR2_RXICMPFCC			(1 << 1)
-#define RXCR2_RXSAF			(1 << 0)
-
-#define KS_TXMIR			0x78
-
-#define KS_RXFHSR			0x7C
-#define RXFSHR_RXFV			(1 << 15)
-#define RXFSHR_RXICMPFCS		(1 << 13)
-#define RXFSHR_RXIPFCS			(1 << 12)
-#define RXFSHR_RXTCPFCS			(1 << 11)
-#define RXFSHR_RXUDPFCS			(1 << 10)
-#define RXFSHR_RXBF			(1 << 7)
-#define RXFSHR_RXMF			(1 << 6)
-#define RXFSHR_RXUF			(1 << 5)
-#define RXFSHR_RXMR			(1 << 4)
-#define RXFSHR_RXFT			(1 << 3)
-#define RXFSHR_RXFTL			(1 << 2)
-#define RXFSHR_RXRF			(1 << 1)
-#define RXFSHR_RXCE			(1 << 0)
+#undef RXCR2_SRDBL_FRAME
+
 #define	RXFSHR_ERR			(RXFSHR_RXCE | RXFSHR_RXRF |\
 					RXFSHR_RXFTL | RXFSHR_RXMR |\
 					RXFSHR_RXICMPFCS | RXFSHR_RXIPFCS |\
 					RXFSHR_RXTCPFCS)
+
 #define KS_RXFHBCR			0x7E
 #define RXFHBCR_CNT_MASK		0x0FFF
 
-#define KS_TXQCR			0x80
-#define TXQCR_AETFE			(1 << 2)
-#define TXQCR_TXQMAM			(1 << 1)
-#define TXQCR_METFE			(1 << 0)
-
-#define KS_RXQCR			0x82
-#define RXQCR_RXDTTS			(1 << 12)
-#define RXQCR_RXDBCTS			(1 << 11)
-#define RXQCR_RXFCTS			(1 << 10)
-#define RXQCR_RXIPHTOE			(1 << 9)
-#define RXQCR_RXDTTE			(1 << 7)
-#define RXQCR_RXDBCTE			(1 << 6)
-#define RXQCR_RXFCTE			(1 << 5)
-#define RXQCR_ADRFE			(1 << 4)
-#define RXQCR_SDA			(1 << 3)
-#define RXQCR_RRXEF			(1 << 0)
 #define RXQCR_CMD_CNTL                	(RXQCR_RXFCTE|RXQCR_ADRFE)
 
 #define KS_TXFDPR			0x84
@@ -214,130 +77,14 @@ static u8 KS_DEFAULT_MAC_ADDRESS[] = { 0x00, 0x10, 0xA1, 0x86, 0x95, 0x11 };
 #define KS_RXFDPR			0x86
 #define RXFDPR_RXFPAI			(1 << 14)
 
-#define KS_RXDTTR			0x8C
-#define KS_RXDBCTR			0x8E
-
-#define KS_IER				0x90
-#define KS_ISR				0x92
-#define IRQ_LCI				(1 << 15)
-#define IRQ_TXI				(1 << 14)
-#define IRQ_RXI				(1 << 13)
-#define IRQ_RXOI			(1 << 11)
-#define IRQ_TXPSI			(1 << 9)
-#define IRQ_RXPSI			(1 << 8)
-#define IRQ_TXSAI			(1 << 6)
-#define IRQ_RXWFDI			(1 << 5)
-#define IRQ_RXMPDI			(1 << 4)
-#define IRQ_LDI				(1 << 3)
-#define IRQ_EDI				(1 << 2)
-#define IRQ_SPIBEI			(1 << 1)
-#define IRQ_DEDI			(1 << 0)
-
-#define KS_RXFCTR			0x9C
 #define RXFCTR_THRESHOLD_MASK     	0x00FF
 
-#define KS_RXFC				0x9D
-#define RXFCTR_RXFC_MASK		(0xff << 8)
-#define RXFCTR_RXFC_SHIFT		(8)
-#define RXFCTR_RXFC_GET(_v)		(((_v) >> 8) & 0xff)
-#define RXFCTR_RXFCT_MASK		(0xff << 0)
-#define RXFCTR_RXFCT_SHIFT		(0)
-
-#define KS_TXNTFSR			0x9E
-
-#define KS_MAHTR0			0xA0
-#define KS_MAHTR1			0xA2
-#define KS_MAHTR2			0xA4
-#define KS_MAHTR3			0xA6
-
-#define KS_FCLWR			0xB0
-#define KS_FCHWR			0xB2
-#define KS_FCOWR			0xB4
-
-#define KS_CIDER			0xC0
-#define CIDER_ID			0x8870
-#define CIDER_REV_MASK			(0x7 << 1)
-#define CIDER_REV_SHIFT			(1)
-#define CIDER_REV_GET(_v)		(((_v) >> 1) & 0x7)
-
-#define KS_CGCR				0xC6
-#define KS_IACR				0xC8
-#define IACR_RDEN			(1 << 12)
-#define IACR_TSEL_MASK			(0x3 << 10)
-#define IACR_TSEL_SHIFT			(10)
-#define IACR_TSEL_MIB			(0x3 << 10)
-#define IACR_ADDR_MASK			(0x1f << 0)
-#define IACR_ADDR_SHIFT			(0)
-
-#define KS_IADLR			0xD0
-#define KS_IAHDR			0xD2
-
-#define KS_PMECR			0xD4
-#define PMECR_PME_DELAY			(1 << 14)
-#define PMECR_PME_POL			(1 << 12)
-#define PMECR_WOL_WAKEUP		(1 << 11)
-#define PMECR_WOL_MAGICPKT		(1 << 10)
-#define PMECR_WOL_LINKUP		(1 << 9)
-#define PMECR_WOL_ENERGY		(1 << 8)
-#define PMECR_AUTO_WAKE_EN		(1 << 7)
-#define PMECR_WAKEUP_NORMAL		(1 << 6)
-#define PMECR_WKEVT_MASK		(0xf << 2)
-#define PMECR_WKEVT_SHIFT		(2)
-#define PMECR_WKEVT_GET(_v)		(((_v) >> 2) & 0xf)
-#define PMECR_WKEVT_ENERGY		(0x1 << 2)
-#define PMECR_WKEVT_LINK		(0x2 << 2)
-#define PMECR_WKEVT_MAGICPKT		(0x4 << 2)
-#define PMECR_WKEVT_FRAME		(0x8 << 2)
-#define PMECR_PM_MASK			(0x3 << 0)
-#define PMECR_PM_SHIFT			(0)
-#define PMECR_PM_NORMAL			(0x0 << 0)
-#define PMECR_PM_ENERGY			(0x1 << 0)
-#define PMECR_PM_SOFTDOWN		(0x2 << 0)
-#define PMECR_PM_POWERSAVE		(0x3 << 0)
-
-/* Standard MII PHY data */
-#define KS_P1MBCR			0xE4
 #define P1MBCR_FORCE_FDX		(1 << 8)
 
-#define KS_P1MBSR			0xE6
 #define P1MBSR_AN_COMPLETE		(1 << 5)
 #define P1MBSR_AN_CAPABLE		(1 << 3)
 #define P1MBSR_LINK_UP			(1 << 2)
 
-#define KS_PHY1ILR			0xE8
-#define KS_PHY1IHR			0xEA
-#define KS_P1ANAR			0xEC
-#define KS_P1ANLPR			0xEE
-
-#define KS_P1SCLMD			0xF4
-#define P1SCLMD_LEDOFF			(1 << 15)
-#define P1SCLMD_TXIDS			(1 << 14)
-#define P1SCLMD_RESTARTAN		(1 << 13)
-#define P1SCLMD_DISAUTOMDIX		(1 << 10)
-#define P1SCLMD_FORCEMDIX		(1 << 9)
-#define P1SCLMD_AUTONEGEN		(1 << 7)
-#define P1SCLMD_FORCE100		(1 << 6)
-#define P1SCLMD_FORCEFDX		(1 << 5)
-#define P1SCLMD_ADV_FLOW		(1 << 4)
-#define P1SCLMD_ADV_100BT_FDX		(1 << 3)
-#define P1SCLMD_ADV_100BT_HDX		(1 << 2)
-#define P1SCLMD_ADV_10BT_FDX		(1 << 1)
-#define P1SCLMD_ADV_10BT_HDX		(1 << 0)
-
-#define KS_P1CR				0xF6
-#define P1CR_HP_MDIX			(1 << 15)
-#define P1CR_REV_POL			(1 << 13)
-#define P1CR_OP_100M			(1 << 10)
-#define P1CR_OP_FDX			(1 << 9)
-#define P1CR_OP_MDI			(1 << 7)
-#define P1CR_AN_DONE			(1 << 6)
-#define P1CR_LINK_GOOD			(1 << 5)
-#define P1CR_PNTR_FLOW			(1 << 4)
-#define P1CR_PNTR_100BT_FDX		(1 << 3)
-#define P1CR_PNTR_100BT_HDX		(1 << 2)
-#define P1CR_PNTR_10BT_FDX		(1 << 1)
-#define P1CR_PNTR_10BT_HDX		(1 << 0)
-
 /* TX Frame control */
 
 #define TXFR_TXIC			(1 << 15)
-- 
1.7.7.4

