From a13358a747c33ecda28a976ed9450b9351827c2a Mon Sep 17 00:00:00 2001
From: Eric Benard <eric@eukrea.com>
Date: Fri, 10 Jun 2011 12:21:52 +0000
Subject: [PATCH 08/30] dm3730: enable dpll5
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

which is used to provide 120MHz to USB EHCI
This allows EHCI to work on BeagleBoard XM

Signed-off-by: Eric Bénard <eric@eukrea.com>
---
 arch/arm/cpu/armv7/omap3/clock.c |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

diff --git a/arch/arm/cpu/armv7/omap3/clock.c b/arch/arm/cpu/armv7/omap3/clock.c
index 3d38d08..6a9edcf 100644
--- a/arch/arm/cpu/armv7/omap3/clock.c
+++ b/arch/arm/cpu/armv7/omap3/clock.c
@@ -579,6 +579,7 @@ void prcm_init(void)
 
 		dpll3_init_36xx(0, clk_index);
 		dpll4_init_36xx(0, clk_index);
+		dpll5_init_34xx(0, clk_index);
 		iva_init_36xx(0, clk_index);
 		mpu_init_36xx(0, clk_index);
 
-- 
1.6.6.1

