From c006cccface5a8f4d48c66465d6ebb69abb2b729 Mon Sep 17 00:00:00 2001
From: Francois Romieu <romieu@fr.zoreil.com>
Date: Sun, 8 Jan 2012 13:41:33 +0000
Subject: [PATCH 38/87] 8139cp: fix missing napi_gro_flush.

commit b189e810619a676e6b931a942a3e8387f3d39c21 upstream.

The driver uses __napi_complete and napi_gro_receive. Without it, the
driver hits the BUG_ON(n->gro_list) assertion hard in __napi_complete.

Signed-off-by: Francois Romieu <romieu@fr.zoreil.com>
Tested-by: Marin Glibic <zhilla2@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/ethernet/realtek/8139cp.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/net/ethernet/realtek/8139cp.c b/drivers/net/ethernet/realtek/8139cp.c
index ee5da92..aba4f67 100644
--- a/drivers/net/ethernet/realtek/8139cp.c
+++ b/drivers/net/ethernet/realtek/8139cp.c
@@ -563,6 +563,7 @@ rx_next:
 		if (cpr16(IntrStatus) & cp_rx_intr_mask)
 			goto rx_status_loop;
 
+		napi_gro_flush(napi);
 		spin_lock_irqsave(&cp->lock, flags);
 		__napi_complete(napi);
 		cpw16_f(IntrMask, cp_intr_mask);
-- 
1.7.9.4

