From a5333b50b8a4297f3b9959366fb26ad9b9c55314 Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Thu, 12 Apr 2012 12:49:16 -0700
Subject: [PATCH 15/69] drivers/rtc/rtc-pl031.c: enable clock on all ST
 variants

commit 2f3972168353d355854d6381f1f360ce83b723e5 upstream.

The ST variants of the PL031 all require bit 26 in the control register
to be set before they work properly.  Discovered this when testing on
the Nomadik board where it would suprisingly just stand still.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Cc: Mian Yousaf Kaukab <mian.yousaf.kaukab@stericsson.com>
Cc: Alessandro Rubini <rubini@unipv.it>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/rtc/rtc-pl031.c |    3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

diff --git a/drivers/rtc/rtc-pl031.c b/drivers/rtc/rtc-pl031.c
index ff1b84b..e86edfc 100644
--- a/drivers/rtc/rtc-pl031.c
+++ b/drivers/rtc/rtc-pl031.c
@@ -339,8 +339,7 @@ static int pl031_probe(struct amba_device *adev, const struct amba_id *id)
 	dev_dbg(&adev->dev, "revision = 0x%01x\n", ldata->hw_revision);
 
 	/* Enable the clockwatch on ST Variants */
-	if ((ldata->hw_designer == AMBA_VENDOR_ST) &&
-	    (ldata->hw_revision > 1))
+	if (ldata->hw_designer == AMBA_VENDOR_ST)
 		writel(readl(ldata->base + RTC_CR) | RTC_CR_CWEN,
 		       ldata->base + RTC_CR);
 
-- 
1.7.9.5

