From f9cce3fb45a90fffc8d2bb59a65ebdbfc881d5a8 Mon Sep 17 00:00:00 2001
From: Elric Fu <elricfu1@gmail.com>
Date: Thu, 29 Mar 2012 15:47:50 +0800
Subject: [PATCH 39/69] xHCI: add XHCI_RESET_ON_RESUME quirk for VIA xHCI host

commit 457a4f61f9bfc3ae76e5b49f30f25d86bb696f67 upstream.

The suspend operation of VIA xHCI host have some issues and
hibernate operation works fine, so The XHCI_RESET_ON_RESUME
quirk is added for it.

This patch should base on "xHCI: Don't write zeroed pointer
to xHC registers" that is released by Sarah. Otherwise, the
host system error will ocurr in the hibernate operation
process.

This should be backported to stable kernels as old as 2.6.37,
that contain the commit c877b3b2ad5cb9d4fe523c5496185cc328ff3ae9
"xhci: Add reset on resume quirk for asrock p67 host".

Signed-off-by: Elric Fu <elricfu1@gmail.com>
Signed-off-by: Sarah Sharp <sarah.a.sharp@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/xhci-pci.c |    2 ++
 1 file changed, 2 insertions(+)

diff --git a/drivers/usb/host/xhci-pci.c b/drivers/usb/host/xhci-pci.c
index ef98b38..211296a 100644
--- a/drivers/usb/host/xhci-pci.c
+++ b/drivers/usb/host/xhci-pci.c
@@ -95,6 +95,8 @@ static void xhci_pci_quirks(struct device *dev, struct xhci_hcd *xhci)
 		xhci->quirks |= XHCI_RESET_ON_RESUME;
 		xhci_dbg(xhci, "QUIRK: Resetting on resume\n");
 	}
+	if (pdev->vendor == PCI_VENDOR_ID_VIA)
+		xhci->quirks |= XHCI_RESET_ON_RESUME;
 }
 
 /* called during probe() after chip reset completes */
-- 
1.7.9.5

