From b0f40f6545e9ae32b6cbd2cb03561de805297bf5 Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Thu, 26 May 2011 19:39:19 -0700
Subject: [PATCH 14/19] OMAP2+: cpufreq: put clk if cpu_init failed

Release the mpu_clk in fail paths.

Reported-by: Todd Poynor <toddpoynor@google.com>
Signed-off-by: Nishanth Menon <nm@ti.com>
Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/omap2plus-cpufreq.c |   14 +++++++++++---
 1 files changed, 11 insertions(+), 3 deletions(-)

diff --git a/arch/arm/mach-omap2/omap2plus-cpufreq.c b/arch/arm/mach-omap2/omap2plus-cpufreq.c
index 3af7cda..e019297 100644
--- a/arch/arm/mach-omap2/omap2plus-cpufreq.c
+++ b/arch/arm/mach-omap2/omap2plus-cpufreq.c
@@ -162,8 +162,10 @@ static int __cpuinit omap_cpu_init(struct cpufreq_policy *policy)
 	if (IS_ERR(mpu_clk))
 		return PTR_ERR(mpu_clk);
 
-	if (policy->cpu >= NR_CPUS)
-		return -EINVAL;
+	if (policy->cpu >= NR_CPUS) {
+		result = -EINVAL;
+		goto fail_ck;
+	}
 
 	policy->cur = policy->min = policy->max = omap_getspeed(policy->cpu);
 	result = opp_init_cpufreq_table(mpu_dev, &freq_table);
@@ -171,12 +173,14 @@ static int __cpuinit omap_cpu_init(struct cpufreq_policy *policy)
 	if (result) {
 		dev_err(mpu_dev, "%s: cpu%d: failed creating freq table[%d]\n",
 				__func__, policy->cpu, result);
-		return result;
+		goto fail_ck;
 	}
 
 	result = cpufreq_frequency_table_cpuinfo(policy, freq_table);
 	if (!result)
 		cpufreq_frequency_table_get_attr(freq_table, policy->cpu);
+	else
+		goto fail_ck;
 
 	policy->min = policy->cpuinfo.min_freq;
 	policy->max = policy->cpuinfo.max_freq;
@@ -199,6 +203,10 @@ static int __cpuinit omap_cpu_init(struct cpufreq_policy *policy)
 	policy->cpuinfo.transition_latency = 300 * 1000;
 
 	return 0;
+
+fail_ck:
+	clk_put(mpu_clk);
+	return result;
 }
 
 static int omap_cpu_exit(struct cpufreq_policy *policy)
-- 
1.7.2.5

